1,1,"Proje"
1,2,"GPS"
1,3,"Local System"
1,4,"Olcum"
1,5,"Setting Out"
1,6,"Tools"
1,7,"Ayarlar"
1,8,"Utilities"

1,9,"Baglanti"
1,10,"Position and Satellites"
1,11,"Gezici Ayar"
1,12,"Sabit Ayar"
1,13,"Sitil"
1,14,"Terminal"
1,15,"Other Functions"
1,16,"Disconnect"

1,17,"Yeni"
1,18,"Ofset"
1,19,"Apply Local System"

1,20,"olcum"
1,21,"Surekli"
1,22,"Longitudinal Profile"
1,23,"Cross Sections"
1,24,"Static"
1,25,"Kinematic"

1,26,"Noktalar"
1,27,"Points over Line"
1,28,"Hat Kesisim"
1,29,"Istasyon ve Ofset"
1,30,"Istasyon ve Kod"
1,31,"Crowns and Feets"
1,32,"Slope Control"
1,33,"Simple Cross-Section"

1,34,"Points over Alignment"
1,35,"Point Analysis"
1,36,"Distance between Points"
1,37,"Area among Points"
1,38,"Geodetic Calculator"

1,39,"Styles"
1,40,"Data Capture"
1,41,"Setting Out"
1,42,"Coordinates"
1,43,"Communications"
1,44,"Sounds"
1,45,"Codes Database"
1,46,"Coordinate Systems"

1,47,"Navigation"
1,48,"System Information"
1,49,"About"

1,50,"About TcpGPS"
1,51,"Program"
1,52,"Executable"
1,53,"Cancel"
1,54,"Operating System"
1,55,"GNSS Receiver"
1,56,"Trademark"
1,57,"Model"
1,58,"Identifier"

1,59,"Model"
1,60,"Extern"
1,61,"Intern"
1,62,"Vertical"
1,63,"Egik"

1,64,"Loading file information..."

1,65,"Base Coordinates"
1,66,"Data"
1,67,"Coordinates"
1,68,"Isim"
1,69,"Kayit"

1,70,"Connection Type"
1,71,"Cable"
1,72,"Bluetooth"
1,73,"Connect"

1,74,"Mode"
1,75,"Manual"
1,76,"Station"
1,77,"Dpl"
1,78,"Height"
1,79,"Surface"
1,80,"SH - H"
1,81,"Point Analysis"

1,82,"Points on Alignment"
1,83,"Ofset"
1,84,"Azimuth"
1,85,"Radius"
1,86,"Slope"
1,87,"Calculate"

1,88,"Distance between Points"
1,89,"Initial Point"
1,90,"Final Point"
1,91,"Distance"
1,92,"Results"
1,93,"New"

1,94,"Line"
1,95,"Polyline"
1,96,"Lines and Parallel Lines"
1,97,"Points on Cross-Section"

1,98,"Projected CRS"
1,99,"dX"
1,100,"dY"
1,101,"dZ"
1,102,"Rx"
1,103,"Ry"
1,104,"Rz"
1,105,"dS"
1,106,"Map Projection"
1,107,"North"
1,108,"South"

1,109,"Latitude of natural origin"
1,110,"Longitude of natural origin"
1,111,"Scale factor at natural origin"
1,112,"False easting"
1,113,"False northing"

1,114,"Longitude of false origin"
1,115,"Latitude of false origin"
1,116,"Scale Factor"
1,117,"Easting at false origin"
1,118,"Northing at false origin"
1,119,"Lat. of 1st standard parallel"
1,120,"Lat. of 2nd standard parallel"

1,121,"Post-processing File"

1,122,"Ellipsoid already exists"
1,123,"New Ellipsoid"
1,124,"Ellipsoid Edition"
1,125,"You must enter a code"
1,126,"You must enter a name"
1,127,"Datum already exists"
1,128,"You must select an ellipsoid"
1,129,"New Geodetic Datum"
1,130,"New Vertical Datum"
1,131,"Geodetic Datum Edition"
1,132,"Vertical Datum Edition"
1,133,"Prime Meridian"

1,134,"You must select a file"
1,135,"Transformation Parameters"
1,136,"Geoid File"
1,137,"GDE file"
1,138,"GSB file"
1,139,"You must select a source datum"
1,140,"You must select a target datum"
1,141,"Datum shift already exists"
1,142,"You must enter transformation parameters"
1,143,"New Datum Shift"
1,144,"Datums Shift Edition"
1,145,"CRS already exists"
1,146,"You must select a datum"
1,147,"Geographic CRS"
1,148,"Geocentric CRS"
1,149,"Projection Parameters"
1,150,"Are you sure you want to delete"

1,151,"Radio Type"
1,152,"Set Mode"
1,153,"Error when setting mode"
1,154,"Mode set"

1,155,"Traslations"
1,156,"Helmert (4-parameter similarity transformation)"
1,157,"Helmert (7-parameter similarity transformation)"
1,158,"2D Helmert + Vertical offset"
1,159,"2D Helmert + Vertical offset and slopes"
1,160,"By Parameters"
1,161,"By Points"
1,162,"HTML Report"
1,163,"Are you sure you want to exit?"
1,164,"You must enter the %s parameter value"

1,165,"TX"
1,166,"TY"
1,167,"TZ"
1,168,"RX"
1,169,"RY"
1,170,"RZ"
1,171,"Rot."
1,172,"X0"
1,173,"Y0"
1,174,"X Slope"
1,175,"Y Slope"
1,176,"Control Point"
1,177,"Used"

1,178,"X Source"
1,179,"Y Source"
1,180,"Z Source"
1,181,"X Target"
1,182,"Y Target"
1,183,"Z Target"
1,184,"Max X Residual"
1,185,"Max Y Residual"
1,186,"Max Z Residual"
1,187,"Are you sure you want to delete selected items?"
1,188,"Edit Point"
1,189,"Maximum %d control points"
1,190,"List codes by"
1,191,"Alphabetic order"
1,192,"Newest first"

1,193,"You must select the area"
1,194,"Error when saving the new coordinate system"
1,195,"You must enter a name"
1,196,"The file already exists, do you want to overwrite it?"
1,197,"Files"
1,198,"Rover"
1,199,"Use"

2,1,"Quality"
2,2,"Maximum PDOP"
2,3,"Minimum sats"
2,4,"Elevation mask"
2,5,"High accuracy"
2,6,"Precise nav."
2,7,"Epochs"
2,8,"HP"
2,9,"VP"

2,10,"Port"
2,11,"Speed"
2,12,"Data bits"
2,13,"Parity"
2,14,"Stop bits"
2,15,"Flow control"
2,16,"Device"

2,17,"Base"
2,18,"Survey"
2,19,"Setting Out"
2,20,"Static"
2,21,"Kinematic"
2,22,"Styles"

2,23,"GNSS receiver Set-Up"
2,24,"Work style"
2,25,"Saving style"
2,26,"Configure"

2,27,"Setting Out"
2,28,"Horizontal"
2,29,"Vertical"
2,30,"Transversal"
2,31,"Switch to near mode"
2,32,"Draw using TcpCAD"
2,33,"Save points automatically"
2,34,"Toleranslar"

2,35,"Project properties"
2,36,"Projected CRS"
2,37,"Local System"

2,38,"Sound"
2,39,"Better Quality"
2,40,"Worse Quality"
2,41,"Fatal Error"
2,42,"Saving"
2,43,"Point staked out"

2,44,"Codes"
2,45,"Suffixes"
2,46,"Add codes automatically"
2,47,"Check for repeated"
2,48,"Sanal klavyeyi kullan"
2,49,"Shortcut key"
2,50,"Survey"

2,51,"Radio modem"
2,52,"Channel"

2,53,"Satellite Constellation"
2,54,"Position"
2,55,"Listing"
2,56,"Satellites"

2,57,"Post-Process Kinematic"
2,58,"Baslat"
2,59,"Pause"
2,60,"File"
2,61,"Code"

2,62,"Local System"
2,63,"Create from N Points"
2,64,"Parameters"

2,65,"Post-Process Static"
2,66,"Time"
2,67,"Point"
2,68,"Accuracy"

2,69,"Styles"
2,70,"Saving"
2,71,"Epochs"
2,72,"Isim"
2,73,"Save in file"
2,74,"Saving interval"
2,75,"Positions"
2,76,"Observations"
2,77,"Saving styles"
2,78,"Evet"
2,79,"Hyr"

2,80,"Elevation Mask"
2,81,"Maximum PDOP"
2,82,"Min. Satellites"
2,83,"Epochs"

2,84,"Fixed"
2,85,"Floating"
2,86,"DGPS"
2,87,"Autonomous"
2,88,"Save for post-processing"
2,89,"Saving interval (s)"
2,90,"Saving time"
2,91,"User defined (s)"
2,92,"Manual"
2,93,"Automatic"
2,94,"Positions to save"

2,95,"Real Time"
2,96,"Advanced Options"

2,97,"Invalid project"

2,98,"Local System Report"
2,99,"Local System Data"
2,100,"Date / Time"
2,101,"Parameters"
2,102,"Statistics"
2,103,"Standard Deviation"
2,104,"Control Points"
2,105,"Control"
2,106,"Control Points Count"
2,107,"Helmert (4-parameter similarity transformation)"
2,108,"Traslations"
2,109,"Helmert (7-parameter similarity transformation)"
2,110,"2D Helmert + Vertical offset"
2,111,"2D Helmert + Vertical offset and slopes"
2,112,"Rotation"
2,113,"Ortho. C."

2,115,"You need at least 2 control points"
2,116,"Error when calculating least-squares solution"
2,117,"Scale value is 0.0"
2,118,"X Scale value is 0.0"
2,119,"Y Scale value is 0.0"
2,120,"You need at least 3 control points"
2,121,"Invalid parameter value (A = 0.0)"
2,122,"Invalid parameter value (B = 0.0)"
2,123,"You need at least 1 control point"
2,124,"You need at least 4 control points"
2,125,"The system does not converge"
2,126,"CDB"
2,127,"Error when loading local system file"
2,128,"Source File"
2,129,"Target File"
2,130,""
2,131,""
2,132,""
2,133,""
2,134,""
2,135,""
2,136,"TcpGPS DEMO"
2,137,"This version has disabled the followed options:"
2,138,"- Create and select project from main menu"
2,139,"- Save more than 25 points and stations in the same project"
2,140,"- Use horizontal alignments longer than 100m"
2,141,"- Export points from result file"
2,142,"- Use Shape and WMS carthography"
2,143,"- Edit and apply local systems"
2,144,"- Convert geographic coordinates files"
2,145,"- Analize points over a surface"
2,146,"- Edit elements of the geodesy module"
2,147,"No horizontal alignment file in the project, do you wish to select it now?"
2,148,"GNSS receiver off"
2,149,"GNSS receiver on"
2,150," Turn receiver off"
2,151," Reset receiver"
2,152," Reset NVM"

3,1,"Son Proje"
3,2,"Proje Sec"
3,3,"Yeni Proje"

3,4,"Base Coordinates"
3,5,"Activate NMEA Output"
3,6,"On/Off Receiver"
3,7,"Post-Process"
3,8,"Initialize Receiver"
3,9,"Reinitialize Receiver"
3,10,"Receiver Files"
3,11,"Other Functions"

3,12,"Pause"
3,13,"Continue"
3,14,"Stop"

3,15,"Unknown Position"
3,16,"Select from File"
3,17,"Manual Entry"
3,18,"Configure Base"

3,19,"Antenna Height"
3,20,"Id."
3,21,"WGS84"
3,22,"UTM"
3,23,"Local"
3,24,"Auto"

3,25,"Kopyala"
3,26,"Rename"
3,27,"Sil"
3,29,"Duzenle"

3,30,"Terminal"
3,31,"Pause"
3,32,"Clear"
3,33,"Command"

3,34,"Commands"
3,35,"Send"
3,36,"Script"

3,37,"Points Stake Out"
3,38,"Individual"
3,39,"Graphic"
3,40,"Initial Point"
3,41,"Final Point"
3,42,"CAD"
3,43,"Request Code"

3,44,"Cross Sections Setting Out"
3,45,"Subgrade line"
3,46,"Roadbed"
3,47,"Single Points"
3,48,"Station and Code"
3,49,"Baslangic Km"
3,50,"Side"
3,51,"Sol"
3,52,"Sag"
3,53,"Aralŭk"

3,54,"Station and Offset"
3,55,"Thickness"
3,56,"Polyline"
3,57,"Points on Section"
3,58,"Lines Intersection"
3,59,"Line-Circle Intersection"
3,60,"Circle-circle Intersection"
3,61,"Polar to Rectangular"
3,62,"Geoids"

3,63,"Geographic"
3,64,"Geocentric"
3,65,"Projected"
3,66,"Local"
3,67,"Ellipsoid"

3,68,"Olculen Noktalar"
3,69,"Ara"
3,70,"Numara"
3,71,"Stations"
3,72,"CAD <"
3,73,"Data Links"
3,74,"Displacement"
3,75,"Create from 2 Pts Ref. 0"
3,76,"Create from N Points"
3,77,"Surveying"
3,78,"Continued Pts Meas."
3,79,"Longitudinal Profile"
3,80,"Cross-Section Profile"
3,81,"Static"
3,82,"Kinematic"

3,83,"Settings"
3,84,"Styles"
3,85,"Surveying"
3,86,"Setting Out"
3,87,"Coordinates"
3,88,"Communications"
3,89,"Code Database"
3,90,"Coordinate Systems"
3,91,"Projected CRSs"
3,92,"Datums"
3,93,"Ellipsoids"
3,94,"Sounds"
3,95,"Echosounder"
3,96,"Laser Distancemeter"

3,97,"Points Measurements"
3,98,"Setting Out"
3,99,"Points on Cross-Section"
3,100,"Error reading project settings"
3,101,"Error reading local system"
3,102,"Error reading antenna height"
3,103,"Error reading saving style"
3,104,"Error reading Y-Coordinate of displacement"
3,105,"Error reading Z-Coordinate of displacement"
3,106,"Error reading RTK rover style"
3,107,"Distance > %d m"
3,108,"Last Pt"
3,109,"Mov"
3,110,"No Position"

3,111,"Error when getting vertical alignment information"
3,112,"Error when reading cross-section file"
3,113,"Sta %0.3lf Dpl %0.3lf"
3,114,"RepPkDesp"
3,115,"Error reading superelevation file information"
3,116,"Error reading superelevation file"
3,117,"Error computing theoretical point"
3,118,"Sta %0.3lf Dpl %s"
3,119,"RepPkCod"
3,120,"Cannot find previous station to interpolate"

3,121,"Cannot find next station to interpolate"
3,122,"Cannot find previous station to interpolate"
3,123,"Cannot find code in next station to interpolate"
3,124,"You must select a cross-section file"
3,125,"C & F Sta %0.3lf"
3,126,"RepCyP"
3,127,"Located on aligment"
3,128,"No Intersection"
3,129,"(A)"
3,130,"C.Slope Sta %0.3lf"

3,131,"RepCT"
3,132,"S. Template Sta %0.3lf"
3,133,"RepSecSencilla"
3,134,"Err. height calculation"
3,135,"Err. superelev calculation"
3,136,"Sta %0.3lf Dpl %0.3lf Hdif%s %0.3lf"
3,137,"RepPtSeccion"
3,138,"Station %s"
3,139,"RepPuntos"
3,140,"Point not found"

3,141,"All points have been staked out"
3,142,"Error reading position"
3,143,"Near point not found"
3,144,"Pt Normal"
3,145,"RepPtNormales"
3,146,"Lines intersection not found"
3,147,"Lines intersection"
3,148,"RepInterLin"
3,149,"Points that define line must be different"
3,150,"Lines"

3,151,"Sta %0.3lf L %d D %0.3lf"
3,152,"RepLineas"
3,153,"Creating line..."
3,154,"Error creating line. Insufficient memory"
3,155,"Station out of interval (1)"
3,156,"Station out of interval (2)"
3,157,"Station out of interval (3)"
3,158,"Station out of interval (5)"
3,159,"Station out of interval (7)"
3,160,"Sta %0.3lf Off %0.3lf"

3,161,"RepLinea"
3,162,"Err. Prj. Point"
3,163,"Invalid authorization code (%d)\n\nPlease, check:\n\n-System date (Control Panel > Date/Time)\n\n-Authorization code\n\n-Program version (Basic or Full)"

4,1,"Configure Rover"
4,2,"Change Settings"
4,3,"Continue with Current Set-Up"
4,4,"Antenna"
4,5,"Height"
4,6,"Save for post-processing"
4,7,"File"

4,8,"Manual"
4,9,"Number"
4,10,"Antenna"
4,11,"Code"
4,12,"Epochs"
4,13,"H"
4,14,"V"
4,15,"Desviations"
4,16,"Coordinates"

4,17,"Continuous"
4,18,"Distance"
4,19,"Time (s)"
4,20,"Height Dif. (m)"

4,21,"Profile Survey"
4,22,"Uzunluk"
4,23,"Baslat"
4,24,"Kyt"
4,25,"Gor"

4,26,"Cross Sections Survey"
4,27,"Initial Sta."
4,28,"Final Sta."
4,29,"Interval"
4,30,"Profile Length"
4,31,"Tolerans"

4,32,"Station"
4,33,"Height"
4,34,"Go"
4,35,"Cancel"

4,36,"S"
4,37,"E"

4,38,"Distance (m)"

4,39,"Are you sure you want to quit?"

4,40,"Request code"

4,41,"Height"
4,42,"EMesf"
4,43,"Bitti"
4,44,"Bitti"
4,45,"Station OK"
4,46,"Sol"
4,47,"Sag"
4,48,"ileri"
4,49,"Geri"
4,50,"Sta"
4,51,"Dpl OK"
4,52,"Out"
4,53,"In"
4,54,"North"
4,55,"Alin."
4,56,"Sun"
4,57,"L.Pt."
4,58,"Sta."
4,59,"Mov."
4,60,"R"
4,61,"L"
4,62,"YM OK"
4,63,"Mesafe"
4,64,"EMesf"
4,65,"Dpl"

4,66,"Invalid"
4,67,"Autonom."
4,68,"RTK Fixed"
4,69,"RTK Float."
4,70,"DGPS"

4,71,"UTC Time"
4,72,"Used Sat."
4,73,"Detect. Sat."
4,74,"UTM Zone"
4,75,"Easting"
4,76,"Northing"
4,77,"Ortho. H."
4,78,"Ellip. H."
4,79,"Position Type"
4,80,"Used Sat."
4,81,"Detect. Sat."
4,82,"Age"
4,83,"Ambiguity"
4,84,"Dist. to Ref."
4,85,"Latitude"
4,86,"Constellation"
4,87,"Data Link"

4,88,"Voice Enabled"

4,89,"Version"
4,90,"for Topcon"
4,91,"(c)2006 APLITOP"

4,92,"Current project"

4,93,"Select device..."

4,94,"Terminal Port"
4,95,"Enable"

4,96,"Height Adjust"
4,97,"GPS"
4,98,"Driver"

4,99,"Antenna Height"
4,100,"G."
4,101,"PD:%3.1lf"
4,102,"PD:%3.1lf S:%6s           "
4,103,"YA:-"
4,104,"DA:-"
4,105,"YA:%5s DA:%5s                      "
4,106,"H:%5s"
4,107,"V:%5s"
4,108,"R:%d%%"
4,109,"Sp: %3.1lf Km/h   "
4,110,"Sp: %3.2lf m/s    "

4,111," Project Properties"
4,112," Project Set-Up"
4,113," Surveying"
4,114," Setting Out"
4,115," Coordinates"
4,116," Code Database"
4,117," Coordinate System"
4,118," Projected CRSs"
4,119," Datums"
4,120," Ellipsoids"

4,121," Sounds"
4,122," Echosounder"
4,123," Laser Distancemeter"
4,124," Components"
4,125," Select File"
4,126," Deselect File"
4,127," View"
4,128," Export Points"
4,129,"Key in"
4,130," Move Points"

4,131," Rotate Points"
4,132," Generate Grid"
4,133," Create Station"
4,134," From Points"
4,135," From Station and Offset"
4,136," Latitude and Longitude"
4,137," Convert Polyline"
4,138," Cross-Sections"
4,139," Subgrade"
4,140," Roadbed"

4,141,"Tools/Utilities"
4,142," Points on Alignment"
4,143," Point Analysis"
4,144," Distance between Points"
4,145," Area among Points"
4,146," Intersections"
4,147," Line Intersection"
4,148," Line-Circle Intersection"
4,149," Circle-Circle Intersection"
4,150," Polar - Rectangular"

4,151," Geodetic Calculator"
4,152," Coordinate Trans."
4,153," Local System"
4,154," New"
4,155," Displacement"
4,156," Defined by 2 points ref. 0"
4,157," Defined by N points"
4,158," Delete"
4,159," About..."
4,160," System Information"

4,161," Gps Settop Soft 'About...'"
4,162," Lisans"
4,163," Baglan"
4,164," Position and Satellites"
4,165," Configure Base"
4,166," Configure Rover"
4,167," Configure Ntrip"
4,168," Styles"
4,169," Other Functions"
4,170," Base Coordinates"

4,171," Activate NMEA Output"
4,172," Post-Process"
4,173," Pause"
4,174," Resume"
4,175," Finish"
4,176," Initialize Receiver"
4,177," Reset Receiver"
4,178," Receiver Files"
4,179," Terminal"
4,180," Communications"

4,181," Disconnect"
4,182,"Survey"
4,183," Survey Points"
4,184," Continuous"
4,185," Survey Stations"
4,186," Profiles"
4,187," Cross-Sections"
4,188," Static"
4,189," Cinematic"
4,190,"Stakeout"

4,191," Lines"
4,192," Line Intersection"
4,193," Lines and Parallel"
4,194," Line"
4,195," Polyline"
4,196," Roads"
4,197," Station and Code"
4,198," Crowns and Feet"
4,199," Slope Control"
4,200," Simple Template"


5,1,"Height"
5,2,"Antenna"
5,3,"Type"
5,4,"Measurement Type"

5,5,"Delete"

5,6,"None"
5,7,"Even"
5,8,"Odd"
5,9,"Automatic"

5,10,"System Information"
5,11,"Batteries Status"
5,12,"Main"
5,13,"Free Disk Space"

5,14,"Utils"
5,15,"Coordinates Transformation"
5,16,"Lisans"
5,17,"About"
5,18,"Latitude and Longitude"
5,19,"Convert Polyline"
5,20,"Soil"
5,21,"Roadbed"
5,22,"Apply"
5,23,"Convert observations file"
5,24,"You must select a local system"
5,25,"The selected local system is being used in the current project.\nIt cannot be deleted"
5,26,"Are you sure you want to delete the selected local system?"
5,27,"Error when deleting the local system file"
5,28,"Error when deleting the local system report file"
5,29,"Error when reading the local system file"
5,30,"The selected local system is being used in the current project.\nIt cannot be edited"
5,31,"2 Pts Ref. 0"

5,32,"Select point to adjust height"
5,33,"Position not available"
5,34,"You must select a point"
5,35,"Adjust height from average?"
5,36,"Adjust height from point?"
5,37,"Local"
5,38,"Measured"
5,39,"Error while gathering information from receiver"

5,40,"Base ID"
5,41,"Height"
5,42,"X"
5,43,"Y"
5,44,"Z"
5,45,"N"
5,46,"S"
5,47,"E"
5,48,"W"
5,49,"South"
5,50,"Error when reading projected CRS"

5,51,"VAH - H"
5,52,"Error reading horizontal alignment file"
5,53,"Error reading vertical alignment file"
5,54,"Far Point"
5,55,"No Position"

5,56,"Must be in GPS mode"
5,57,"Point file not found"
5,58,"P"
5,59,"PtAnalysis"
5,60,"Point %ld stored"

5,61,"Error computing point over alignment"
5,62,"PtSobreEje"
5,63,"dx"
5,64,"dy"
5,65,"Point file is empty"
5,66,"Initial point does not exist"
5,67,"Final point does not exist"
5,68,"Points cannot be the same"

5,69,"Project Height"
5,70,"Initial"
5,71,"Final"
5,72,"S"
5,73,"E"
5,74,"ATTENTION!"
5,75,"Base Coordinates different than expected"

5,76,"Expected Coordinates"
5,77,"Received Coordinates"
5,78,"Do not show this message again"
5,79,"X: %0.3lf"
5,80,"Y: %0.3lf"

5,81,"Cartography Properties"
5,82,"Displacements"
5,83,"Cable Connection"
5,84,"Bluetooth Connection"
5,85,"Receiver Port"
5,86,"Handheld Port"
5,87,"Devices"
5,88,"GNSS receiver drivers not found"
5,89,"You must restart program for changes to take effect"

5,90,"Error updating settings file"
5,91,"Laser Distancemeter"
5,92,"Cannot find predefined styles"
5,93,"Error updating settings file"
5,94,"Set-Up Data"
5,95,"GSM Set-Up"
5,96,"PIN"
5,97,"Base Number"
5,98,"Connection Time"
5,99,"Unlimited"
5,100,"Maximum (minutes)"

5,101,"Error when closing COM port"
5,102,"Error when unloading DLL file"
5,103,"There is no communication with the GNSS receiver"
5,104,"Error when opening capture file"
5,105,"Error when initializing the projected CRS"
5,106,"Error when reading the projected CRS"
5,107,"Error when canceling measurement"
5,108,"GPS data file has not name"
5,109,"Error when opening GPS data file"
5,110,"Error when saving data into GPS data file"
5,111,"Point not found in GPS data file"
5,112,"GPS data file not found"
5,113,"GPS data file has not observations"
5,114,"#Projected CRS: %s  Geodetic Datum Shift: %s  Vertical CRS: %s  Vertical Datum Shift: %s  Local System: %s"
5,115,"Error when reading antennas file"
5,116,"Error when obtaining data of the radio modem"
5,117,"Error when establishing channel of radio modem"
5,118,"Channel established"
5,119,"PuntoUnico"
5,120,"3TraslacionesEscala"

5,121,"3Traslaciones"
5,122,"Invalid position"
5,123,"HP invalid %0.3lf"
5,124,"VP invalid %0.3lf"
5,125,"Pdop invalid %0.1lf"
5,126,"Few satellites %d"
5,127,"Error when saving point in the results file"
5,128,"Error when loading echosounder driver"
5,129,"Error when unloading echosounder driver"
5,130,"Error when opening communication port for echosounder device"
5,131,"Error when closing communication port for echosounder device"
5,132,"Error when configuring geodesy module"
5,133,"Cannot find GNSS receiver models"
5,134,"Error when initializing GNSS receiver"
5,135,"Fatal Error\nNot enough memory"
5,136,"You must select a project"
5,137,"Invalid Characters '\\  : ? |'"
5,138,"Minimum %d characters"
5,139,"Maximum %d characters"
5,140,"Invalid number"

5,141,"Minimum %d"
5,142,"Maximum %d"
5,143,"Minimum %0.3lf"
5,144,"Maximum %0.3lf"
5,145,"Current Project: %s"
5,146,"Error when loading bitmap"
5,147,"        Communication Error       "
5,148,"Signal Lost"
5,149,"Course: %3.0lf°    "
5,150,"%3.3lf knots   "
5,151,"Error reading work style file"
5,152,"Error creating work style file"
5,153,"Error updating work style"
5,154,"Error copying work style file"
5,155,"Error reading saving style file"

5,156,"Error creating saving style file"
5,157,"Error updating saving style file"
5,158,"Error copying saving style file"
5,159,"UNKNOWN"
5,160,"Error opening style file"
5,161,"Error modifying style data"
5,162,"Error copying style file"
5,163,"Error creating style file"
5,164,"Current GNSS receiver model does not support selected option"
5,165,"Error creating file"
5,166,"Are you sure you want to\nremove file %s?"
5,167,"File deleted"
5,168,"Error deleting file"
5,169,"This type of file cannot contain Z column. Zero will be assigned to height"
5,170,"Noktalar secilmedi"

5,171,"Station: %0.3lf\nX: %0.3lf\nY: %0.3lf\nAzimuth: %0.3lf\nRadius: %0.3lf\n"
5,172,"Conversion done"
5,173,"Cannot find profile file"
5,174,"File does not contain data for drawing"
5,175,"Project result file not found"
5,176,"Result file is empty"
5,177,"Error creating point file"
5,178,"Nokta dosyasi olusturuldu"
5,179,"Dosya bos"
5,180,"DXF file not found in project"

5,181,"X: %0.3lf\nY: %0.3lf\nHeight: %0.3lf\n"
5,182,"Cannot find surface file in project"
5,183,"Error activating NMEA messages"
5,184,"NMEA output active"
5,185,"Saving stopped"
5,186,"There is not an active saving file. You must configure receiver"
5,187,"GNSS receiver initialized"
5,188,"Process started"
5,189,"Error resetting GNSS receiver"
5,190,"GNSS receiver disconnected"

5,191,"Error disconnecting GNSS receiver. Retry again"
5,192," On / Off Receiver"
5,193,"There's not results file in the project.\nżDo you wish to select it?"
5,194,"Option unavailable"
5,195,"Error when capturing GGA string"
5,196,"Error when creating GGA file"
5,197,"Error when configurating NTRIP"
5,198,"PROJECT"
5,199," New Project"
5,200," Select Project"

6,1,"Work Mode"
6,2,"Numerical Information"
6,3,"Graphic View"
6,4,"Near Mode"
6,5,"Far Mode"
6,6,"You must store a point in one of the stakeout options"
6,7,"You must select a base station"
6,8,"Error updating Set-Up"
6,9,"Sun"
6,10,"Last Point"
6,11,"Movement"
6,12,"Alignment"
6,13,"None"
6,14,"Compass"
6,15,"Target"
6,16,"Plan View"
6,17,"Front View"
6,18,"Lines"
6,19,"Base"

6,20,"Graphic View"
6,21,"Alignment in Plan View"
6,22,"Alignment in Front View"
6,23,"Operator"
6,24,"IP"
6,25,"User"
6,26,"Password"
6,27,"NTRIP Set-Up"
6,28,"TCP/IP Set-Up"

6,29,"Geoid"
6,30,"ATTENTION!\nProjected CRS has changed. Points stored in previous system.\nDo you want to continue?"
6,31,"ATTENTION!\nLocal system has changed. Current aditional displacements will be removed.\nX: %0.3lf\nY: %0.3lf\nZ: %0.3lf\nDo you want to continue?"
6,32,"NONE"
6,33,"Configure Ports"
6,34,"Bits per second"
6,35,"You must restar for changes to take effect"
6,36,"Port configured"
6,37,"Error configuring ports"
6,38,"Bps Port %s: %d"
6,39,"Bps Port %s: Unknown"
6,40,"%s (ASCII): %d"

6,41,"Create Station from Latitude and Longitude"
6,42,"WGS84 Lat"
6,43,"WGS84 Long"
6,44,"WGS84 h"
6,45,"Scale"
6,46,"BaseLatLon"
6,47,"B"
6,48,"CrearBaseLatLon"
6,49,"Error when storing station data"
6,50,"Station stored"
6,51,"Another station with the same name already exists"
6,52,"Error when reading projected CRS"
6,53,"Error computing station projected coordinates"
6,54,"base1"

6,55,"Measure"
6,56,"There are no laser distancemeter drivers"
6,57,"Laser distancemeter driver has not been selected"
6,58,"Error when loading laser distancemeter driver"
6,59,"Error when opening communications port for laser distancemeter device"
6,60,"Error when unloading laser distancemeter driver"
6,61,"Measured Distance: %0.3lf"
6,62,"Error reading distance"

6,63,"Rover Set-Up"
6,64,"Waiting for Data Link..."
6,65,"Waiting for Data Link"
6,66,"Waiting for Accuracy"
6,67,"Waiting for Base Data"
6,68,"Antenna height received is null.\n Do you want to continue?"
6,69,"BaseRef"
6,70,"EnlaceRTK"
6,71,"Waiting for Data Link"

6,72,"You must select at least one option in \"Positions to store\""
6,73,"Remove Style"
6,74,"You must select a style"
6,75,"Are you sure you want to remove selected style?"
6,76,"Style removed"
6,77,"Unable to remove style" 
6,78,"Copy style"
6,79,"A style with the name: %s already exists"
6,80,"New style"
6,81,"Another style with the same name already exists"

6,82,"Offset"
6,83,"Antenna file is empty"
6,84,"Multipath Reduction"
6,85,"Co-op Tracking"
6,86,"Satellite System"
6,87,"GPS + GLONASS"
6,88,"Error reading available radio models"
6,89,"Format"
6,90,"Corrections"
6,91,"Protocol"
6,92,"Details"
6,93,"Position Update"

6,94,"Error reading available RTK formats"
6,95,"Error reading available corrections"
6,96,"RTK"
6,97,"GPS Files"
6,98,"Refresh"
6,99,"Load"
6,100,"GPS files not found"
6,101,"You must select a file from the list"
6,102,"Are you sure you want to remove the selected file?"
6,103,"Error deleting receiver file"
6,104,"Size"
6,105,"Date"
6,106,"Backup"

6,107,"Desc"
6,108,"Error getting available disk space"
6,109,"System memory lower than 1 MB"
6,110,"Available disk space: %I64u KB"
6,111,"Main battery %d %c"
6,112,"%I64u KB"
6,113,"Layer"
6,114,"Visible"

6,115,"Long"
6,116,"Lat"
6,117,"Elev"
6,118,"Error in coordinate conversion (8)"
6,119,"Error in coordinate conversion (9)"
6,120,"Error in coordinate conversion (6)"
6,121,"Error in coordinate conversion (7)"
6,122,"Error in coordinate conversion (10)"
6,123,"Error in coordinate conversion (11)"
6,124,"Error in coordinate conversion (12)"
6,125,"Error in coordinate conversion (13)"

6,126,"Position not available to check distance"
6,127,"Given point is too far from current station"
6,128,"Error starting receiver in base mode (1)"
6,129,"Error starting receiver in base mode (2)"
6,130,"GNSS receiver is configured in base mode"
6,131,"ConfigBase"
6,132,"ATTENTION!\nBase must be configured"
6,133,"Station already exists. You must enter a different name"
6,134,"ATTENTION!\nYou have not changed antenna height.\nContinue?
6,135,"To configure base you must press Start"
6,136,"BR-1"
6,137,"Error in coordinate conversion (2)"
6,138,"Error in coordinate conversion (3)"
6,139,"Error in coordinate conversion (4)"
6,140,"Error in coordinate conversion (5)"

6,141,"HELMERT 3D\n"
6,142,"X = mA * x + mB * y + mX0\n"
6,143,"Y = mD * x + mE * y + mY0\n"
6,144,"Z = z + mZ0\n\n"
6,145,"mA\t%0.10lf\n"
6,146,"mB\t%0.10lf\n"
6,147,"mD\t%0.10lf\n"
6,148,"mE\t%0.10lf\n"
6,149,"mX0\t%0.10lf\n"
6,150,"mY0\t%0.10lf\n"
6,151,"mZ0\t%0.10lf\n\n"

6,152,"HELMERT 2D\n"
6,153,"Y = -mB * x + mA * y + mY0\n"
6,154,"Z = z + mOffsetZ\n\n"
6,155,"mOffsetZ\t%0.10lf\n"
6,156,"More points needed to compute local system"
6,157,"Average"

6,158,"s\t%0.10lf\n"
6,159,"m11\t%0.10lf\n"
6,160,"m12\t%0.10lf\n"
6,161,"m13\t%0.10lf\n"
6,162,"m21\t%0.10lf\n"
6,163,"m22\t%0.10lf\n"
6,164,"m23\t%0.10lf\n"
6,165,"m31\t%0.10lf\n"
6,166,"m32\t%0.10lf\n"
6,167,"m33\t%0.10lf\n"
6,168,"tx\t%0.10lf\n"
6,169,"ty\t%0.10lf\n"
6,170,"tz\t%0.10lf\n\n"

6,171,"Maximum residual"
6,172,"Import"
6,173,"You must select a projected CRS"
6,174,"Current projected CRS cannot be deleted"
6,175,"Are you sure that you want to delete selected projected CRS?"
6,176,"Central Meridian"
6,177,"Origin Latitude"
6,178,"False Easting"
6,179,"False Northing"
6,180,"Scale Factor"
6,181,"UTM Zone"
6,182,"Hemisphere"

6,183,"Select origin coordinates to compute local system"
6,184,"Current Position"
6,185,"Get Coordinates"
6,186,"Next >"
6,187,"Error getting base coordinates"
6,188,"Select local coordinates to compute local system"
6,189,"< Previous"
6,190,"Name for new local system"
6,191,"Finish"

6,192,"Current Local System"
6,193,"Max. Horizontal Error"
6,194,"Max. Vertical Error"
6,195,"Use Current Displacements"
6,196,"You must enter at least one point"
6,197,"Points listing not found"
6,198,"Are you sure you want to delete selected point?"
6,199,"Point already exists"
6,200,"Current displacements:\nX: %0.3lf\nY: %0.3lf\nZ: %0.3lf\nDo you want to continue?"

7,1,"File type"
7,2,"Coordinate type"
7,3,"Error reading stations file"
7,4,"Error reading points file"
7,5,"You must enter a value"
7,6,"Stations file is empty"
7,7,"Cannot find station in file"
7,8,"Points file is empty"
7,9,"Cannot find point in file"
7,10,"You must select a point or station"

7,11,"There are no stations for selecting"
7,12,"There are no points for selecting"
7,13,"Storing style files not found"
7,14,"Working style files not found"
7,15,"Option not implemented"
7,16,"Error computing projected coordinates"
7,17,"Error adding record"

7,18,"Ready"
7,19,"Assign"
7,20,"There are no styles for editing"
7,21,"There are no styles for copying"
7,22,"There are no styles for deleting"
7,23,"Error removing style"
7,24,"There are no styles for renaming"

7,25,"Saving paused"
7,26,"Active file does not exist. You must configure GNSS receiver"
7,27,"Saving resumed"
7,28,"Active working style does not exist"
7,29,"Saving finished"

7,30,"Start Job"
7,31,"Default"
7,32,"Place in Local System"
7,33,"Define Local System"
7,34,"ATTENTION!\nCurrent displacement will be removed\nX: %0.3lf\nY: %0.3lf\nZ: %0.3lf\nDo you want to continue?"
7,35,"Local system not defined for this project"
7,36,"ATTENTION!\nLocal system and displacements will be removed\nSC: %s\nX: %0.3lf\nY: %0.3lf\nZ: %0.3lf\nDo you want to continue?"

7,37,"Geoid %s"
7,38,"Invalid UTM data"
7,39,"Unable to update settings file"
7,40,"y"
7,41,"n"

7,42,"You must specify a file name"
7,43,"you must specify a point name"
7,44,"GNSS receiver has no available memory to record data"
7,45,"GNSS receiver is saving data. Do you want to quit?"
7,46," S\0"
7,47," E\0"
7,48,"%d Point stored"
7,49,"%d Points stored"
7,50,"LevCinematico"
7,51,"Error getting GNSS receiver files"
7,52,"File already exists in receiver"

7,53,"0 sec. of %d"
7,54,"0 seconds"
7,55,"You must enter a point name"
7,56,"%d seconds"
7,57,"%d sec. %d"
7,58,"Predefined time finished. Do you want to finish saving?"
7,59,"LevEstatico"
7,60,"Error when saving point in the file"

7,61,"Warning: Insuficient Accuracy"
7,62,"Information"
7,63,"HP"
7,64,"VP"
7,65,"PDOP"
7,66,"Ignore"
7,67,"Stop saving"
7,68,"Do not ask again"

7,69,"Azimuth / Distance"
7,70,"Ref. Point"
7,71,"Hght. Dif."
7,72,"Point recorded"
7,73,"You must select a reference point"
7,74,"Error when measuring distance"
7,75,"You must select a points file"
7,76,"Code database does not exist"
7,77,"Current points file is empty. \n%s"

7,78,"Distances / Points"
7,79,"P1"
7,80,"P2"
7,81,"P3"
7,82,"D"
7,83,"Sol"
7,84,"Lft of P2"
7,85,"Rg of P2"
7,86,"There is not solution"
7,87,"There are not solutions"
7,88,"Point recorded"
7,89,"You must select the point 1"
7,90,"You must select the point 2"
7,91,"The points 1 and 2 must be different"
7,92,"You musts select the point 3"
7,93,"The points 1 and 3 must be different"
7,94,"The points 2 and 3 must be different"

7,95,"Distance (P2)"
7,96,"Hght. Dif. (P2)"
7,97,"The points must be different"

7,98,"Displaced points"
7,99,"Polar to Rectangular"
7,100,"Input Data"
7,101,"X Coord."
7,102,"Y Coord."
7,103,"Z Coord."
7,104,"You must enter a point number"

7,105,"Radio Channels"
7,106,"Frecuency Table"
7,107,"Channel Listing"
7,108,"Set Channel"
7,109,"Invalid Channel"
7,110,"Error getting channel information"
7,111,"You must enter a channel"

7,112,"Out of local system"
7,113,"Do not show this message again"
7,114,"SieteParametros"
7,115,"Helmert3D"

7,116,"Alignment Height"
7,117,"Inc."
7,118,"Aut."
7,119,"Pt."
7,120,"You must select graphic mode"
7,121,"Nearest"
7,122,"Exclude Set Out"

7,123,"Error readign point file"
7,124,"You must select stakeout point"
7,125,"Selected initial point not found in file"
7,126,"You must enter a code"
7,127,"Cannot find any point with the given code in file"
7,128,"Cannot find individual point selected in file"
7,129,"Cannot find result file in project"
7,130,"Error checking stakeout status of selected point"
7,131,"The point is already set out.\nContinue?
7,132,"Result file not found in project"
7,133,"Error checking stakeout status of selected station"
7,134,"Station is already staked out.\nContinue?"
7,135,"Cannot find result file in project"
7,136,"Error checking stakeout status of point selected"
7,137,"Cannot find result file for checking points"
7,138,"There are no points for stakeout"
7,139,"Initial point does not exist in file"
7,140,"Final point does not exist in file"
7,141,"Given point not found in file"

7,142,"Reference Height"
7,143,"Automatic"
7,144,"Optional Slopes"
7,145,"No cross-sections files in the project"
7,146,"Error reading cross-section file"
7,147,"Cannot find station in cross-section file"
7,148,"Platform width"
7,149,"Origin height"
7,150,"Slope type"
7,151,"Slope"
7,152,"Cut"
7,153,"Fill"

7,154,"Line 1"
7,155,"Line 2"
7,156,"Point 1"
7,157,"Point 2"
7,158,"Points not read"
7,159,"Error: Cannot find intersection between lines"

7,160,"Lines Intersection"
7,161,"C."
7,162,"H. Offset"
7,163,"Error gettwing initial and end alignment station"
7,164,"There is no cross-section file in current project"
7,165,"X1"
7,166,"Y1"
7,167,"Z1"
7,168,"X2"
7,169,"Y2"
7,170,"Z2"
7,171,"N1"
7,172,"N2"
7,173,"Point does not exist"

7,174,"Point 1 (P1)"
7,175,"Point 2 (P2)"
7,176,"Distance to origin(DO)"
7,177,"Distance to line(DR)"
7,178,"Initial point not selected"
7,179,"Final point not selected"

7,180,"Stakeout Types"
7,181,"Polyline selected has less than 2 vertices"
7,182,"Error converting polyline to alignment"
7,183,"You must select a DXF file in project"
7,184,"B_%s"
7,185,"Error getting point from drawing"
7,186,"You must enter a point number"
7,187,"P_%s"
7,188,"You must enter a station name"
7,189,"Reference Line"

7,190,"You must select start point of reference line"
7,191,"You must select end point of reference line"
7,192,"Points must be different"
7,193,"One way"
7,194,"Round Trip"
7,195,"Parallels"
7,196,"Staggered"
7,197,"Side Offset"
7,198,"Direction"
7,199,"Points between lines"
7,200,"MSE"

7,201,"Reading Source File..."
7,202,"Writing Target File..."
7,203,"Error when opening source file"
7,204,"Source file is empty"
7,205,"Error when creating target file"
7,206,"Target File Created"
7,207,"%ld Points Read"
7,208,"%ld Points Transformed"

7,209,"Guiding over Alignment"
7,210,"H. Alignment"
7,211,"Save Data File"
7,212,"From project"
7,213,"Select file"
7,214,"From polilyne"
7,215,"Defined by 2 points"
7,216,"By time"
7,217,"By distance"
7,218,"Seconds"
7,219,"Meters"
7,220,"The project doesn't include Shape or DXF cartography files"
7,221,"You must select the data file"
7,222,"You must select an horizontal alignment"

8,1,"Sonar Height"
8,2,"%d (%dGPS + %dGLO)"
8,3,"No Comm."
8,4,"%d  North"
8,5,"%d  South"
8,6,"G%d"
8,7,"R%d"
8,8,"G"
8,9,"R"
8,10,"Az:%d  Elev:%d  SNR:%d "
8,11,"Azimuth: %d"
8,12,"Elevation: %d"
8,13,"SNR.L1:%d  L2:%d"
8,14,"Bad state"

8,15,"Low elevation"
8,16,"Weak signal"
8,17,"Not used"
8,18,"L1"
8,19,"L2"
8,20,"Normal"
8,21,"N"
8,22,"Az"
8,23,"Status"
8,24,"Satellites: %d/%d"
8,25,"SNR"

8,26,"Real time system restarted"
8,27,"Error restarting real time system"
8,28," (s)"
8,29,"Fixed"
8,30,"Restart"
8,31,"Cannot read project settings"
8,32,"ERROR: You must select a projected CRS"

8,33,"etiq1"
8,34,"Poligon Sec"
8,35,"Nokta Secimi"
8,36,"COM%d"
8,37,"Port must be different of %d"
8,38,"Port must be different of %d and %d"
8,39,"Cannot find sonar drivers"

8,40,"Start Code"
8,41,"N Epochs"
8,42,"TdContinua"
8,43,"Point %s"
8,44,"TdAuto"
8,45,"Td"
8,46," S"
8,47," E"
8,48,"Cannot find points in project.\nDo you want to select one?"
8,49,"Ortho. H."
8,50,"Ellip. H."
8,51,"Error saving point"
8,52,"Current point file is empty.\n%s"
8,53,"Error creating new point file"

8,54,"TdManual"
8,55,"Cannot create a new profile file"
8,56,"Profile information does not exist"
8,57,"TdLon"
8,58,"Profile file is empty.\n%s"
8,59,"Profile file not found in project.\nDo you want to create one?"
8,60,"Error creating new profile file"
8,61,"Station %0.3lf Dpl %0.3lf"
8,62,"Error opening point file"
8,63,"Error opening profile file"
8,64,"Error saving profile vertex"

8,65,"You must enter a command"
8,66,"Token too long"
8,67,"Dosya acilirken hata olustu"
8,68,"Kaydetme tarihi yok"
8,69,"Dosya olusturuldu"

8,70,"Survey Station"
8,71,"TomarBase"
8,72,"Error saving station"
8,73,"Station already exists"
8,74,"Add Position Type to Code"
8,75,"You must select at least an option"

8,76,"Error creating alignment file"
8,77,"Survey Alignment"
8,78,"On Sta  Off %0.2lf"
8,79,"Fwd %0.2lf  Off %0.2lf"
8,80,"Bcw %0.2lf  Off %0.2lf"
8,81,"Hgt %0.3lf  NV %d"
8,82,"Out of tolerance and offset"
8,83,"Out of tolerance"
8,84,"Out of offset"
8,85,"Offset > %d m"

8,86,"Cross-Section without data"
8,87,"NV 0 Lft 0.0 Rgt 0.0"
8,88,"NV %d Lft %0.1lf Rgt %0.1lf"
8,89,"Error when reading cross-section file"
8,90,"Error analyzing point read"
8,91,"Ħ ATTENTION ! \nOut of tolerance and offset\n"
8,92,"Ħ ATTENTION ! \nOut of tolerance\n"
8,93,"Ħ ATTENTION ! \nOut of offset\n"
8,94,"Do you want to save data?"
8,95,"Point Code"
8,96,"TTRA"
8,97,"TTRA_%s_%0.3lf_%0.3lf_%s"
8,98,"TomarTra"
8,99,"Cross-section vertices not found"

8,100,"Error getting initial and final station"
8,101,"Cross-section files do not exist.\nDo you want to create one?"
8,102,"Error when creating cross-section file"
8,103,"Current Alignment: %s"
8,104,"Station Interval"
8,105,"Left Width"
8,106,"Right Width"
8,107,"Current Alignment: Test.eje"
8,108,"Reference Cross-Section"
8,109,"Left Exc."
8,110,"Right Exc."
8,111,"Error reading reference cross-sections"
8,112,"Reference file does not contain data for station"

8,113,"Define by 2 points ref. 0"
8,114,"Points File"
8,115,"--None--"
8,116,"Local system applied"
8,117,"Projected CRS applied"
8,118,"No points found in GPS data file"
8,119,"Origin and target files are different"
8,120,"0 common points found. File not created"
8,121,"Local system applied"

8,122,"Traslation (m)"
8,123,"Rotation (sec)"
8,124,"Scale (ppm)"
8,125,"Datum"
8,126,"Identification"
8,127,"ID"

8,128,"Define by 1 Point"
8,129,"You must get position"
8,130,"Local Coordinates"
8,131,"Rx"
8,132,"Ry"
8,133,"Rz"
8,134,"Disp. X"
8,135,"Disp. Y"
8,136,"Disp. Z"
8,137,"Error computing local system"
8,138,"You must compute local system"
8,139,"Do you want to apply local system?"
8,140,"You must select a name for local system"
8,141,"You must select origin point"
8,142,"You must select target point"
8,143,"PtInicial"
8,144,"PtFinal"
8,145,"Error computing inverse local system"

8,146,"Insert"
8,147,"Error getting GNSS receiver data"
8,148,"You must get current position"
8,149,"You must select local coordinates"
8,150,"Description"
8,151,"Semi-axis"
8,152,"Major"
8,153,"Minor"
8,154,"Other"
8,155,"Flattening"
8,156,"Inv.Flattening"

8,157,"You must select an element from list"
8,158,"Are you sure you want to delete selected element?"
8,159,"Parallel 1"
8,160,"Parallel 2"
8,161,"Projected CRS"
8,162,"Center"
8,163,"Origin"

8,164,"You must select planimetry, altimetry or both"
8,165,"GPS Coordinates"
8,166,"Point Pairs"
8,167,"H Control"
8,168,"V Control"
8,169,"Seven Parameters"
8,170,"Residuals"
8,171,"Control"

8,172,"X Residual"
8,173,"Y Residual"
8,174,"Z Residual"
8,175,"You must insert at least 2 pairs of points"
8,176,"ATTENTION!\nRound Mean Square: %0.4lf\n Continue?"
8,177,"You must enter a name for local system"
8,178,"Source file is empty"
8,179,"Error when creating source coordinates file"
8,180,"Error when reading source coordinates file"

8,181,"Target coordinates file is empty"
8,182,"Error when reading target coordinates file"
8,183,"The distance between target points %s and %s is less than 1 cm. Remove same points from file"
8,184,"The distance between source points %s and %s is less than 1 cm. Remove same points from file"
8,185,"%d common points found. Must exists at least 2"
8,186,"%d common points found. Must exists at least 3"
8,187,"%d common points found. Must exists at least 4"
8,188,"Error opening local system report file"
8,189,"SEVEN PARAMETER LOCAL TRANSFORMATION\n"
8,190,"Station\tX.Origin\tY.Origin\tZ.Origin\tStation\tX.Target\tY.Target\tZ.Target\n"

8,191,"Station\tStation\tRes.X\tRes.Y\tRes.Z\n"
8,192,"RESULTS\n"
8,193,"X = s * (m11 * x + m12 * y + m13 * z) + tx\n"
8,194,"Y = s * (m21 * x + m22 * y + m23 * z) + ty\n"
8,195,"Z = s * (m31 * x + m32 * y + m33 * z) + tz\n\n"
8,196,"PARAMETER\n"
8,197,"Scale\t\tS: %0.10lf\n"
8,198,"Displacement\t\tX: %0.3lf\tY: %0.3lf\tZ: %0.3lf\n"
8,199,"Angles\t\tOmega: %0.4lf\tTita: %0.4lf\tKappa: %0.4lf\n"
8,200,"Standard Desviation: %0.4lf\n"
8,201,"Waiting for data from radio modem"
8,202,"Configuring radio modem"
8,203,"Base Id."
8,204,"Any"

8,205,"C"
8,206," C"

8,207,"RTK Fixed"
8,208,"RTK Floating/OmniHP/OmniXP"
8,209,"DGPS/OmniVBS"
8,210,"Autonomous"
8,211,"Virtual Port"

8,212,"ATTENTION!\nGeoid has changed. Points stored with previous geoid.\nDo you want to continue?"
8,213,"Error when copy NTR file"
8,214,"Error when copy TXT file.\nżDo you want to continue?"
8,215,"The local system file already exists.\nżDo you want to overwrite it?"
8,216,"Activate Open mode"
8,217,"Activate Forest mode"
8,218,"Query state"
8,219,"Environmental condition"

9,1,"Current displacements:\nX: %0.3lf\nY: %0.3lf\nZ: %0.3lf\nDo you want to work with them?"
9,2,"(%s) D %0.2lf MH %0.2lf\n"
9,3,"(%s) P %s D %0.2lf MH %0.2lf\n"
9,4,"MH"
9,5," Line + (Right)"
9,6," Line - (Left)"
9,7,"(%s) L %d DO %0.2lf\nD %0.2lf MH %0.2lf\n"
9,8," Right Side"
9,9," Left Side"
9,10," New Station"
9,11," New Offset"
9,12,"Sta %0.2lf Dpl %0.2lf"
9,13,"Sta %0.2lf MH %0.2lf\n"
9,14," New Code"
9,15,"Sta %0.2lf Dpl %0.2lf Hdif ?"
9,16,"Error when creating vertical alignment file"
9,17,"Files created"
9,18,"Disconnect NTRIP"
9,19,"Activate/Deactivate Satellites"
9,20,"Sta %0.2lf Dpl %0.2lf MH %0.2lf"
9,21,"Camera"
9,22,"Error when initializing camera"
9,23,"Day"
9,24,"Night"
9,25,"Auto"
9,26,"You must select X1 zoom"
9,27,"Error when capturing image"
9,28,"Save this image?"
9,29,"Capture"
9,30,"Brightness"
9,31,"Sharpness"
9,32,"Zoom"
9,33,"Error when creating image folder"
9,34,"Error when creating PHT file"
9,35,"You must save a point"
9,36,"Error when opening PHT file"
9,37,"Image %s already exists.\nDo you want to overwrite it?"
9,38,"Image Viewer"
9,39,"LOG File"
9,40,"Baslat"
9,41,"Stop"
9,42,"Continue"
9,43,"Station: %0.3lf\nSlope: %0.3lf\n"
9,44,"L: %0.3lf\nHeight: %0.3lf\n"
9,45,"Station: %0.3lf\nHeight: %0.3lf\n"
9,46,"Station: %0.3lf\nHeight: %0.3lf\nSlope: %0.6lf\n"
9,47,"DX"
9,48,"DY"
9,49,"DZ"
9,50,"Semi-Major Axis"
9,51,"The selected projected CRS is being used"
9,52,"Do you wish to delete the projected CRS"
9,53,"The selected ellisoid is being used"
9,54,"The selected datum is being used"
9,55,"Do you wish to delete the ellipsoid"
9,56,"Do you wish to delete the datum"
9,57,"You must set the ellipsoid code"
9,58,"Only 2 characters codes are valid"
9,59,"You must set the ellipsoid name"
9,60,"%s ellipsoid already exists"
9,61,"dX"
9,62,"dY"
9,63,"dZ"
9,64,"Rx"
9,65,"Ry"
9,66,"Rz"
9,67,"dS"
9,68,"You must set the datum code"
9,69,"You must set the datum name"
9,70,"The datum code must be of 8 characters as maximum"
9,71,"%s datum already exists"
9,72,"Projected CRS Type"
9,73,"False Easting (m)"
9,74,"False Northing (m)"
9,75,"Grid"
9,76,"You must set the projected CRS name"
9,77,"%s projected CRS already exists"
9,78,"You must select a NTv2 grid file"
9,79,"Zone (1-60)"
9,80,"UTM Zone must be between 1 and 60"
9,81,"View Observations File"
9,82,"#Projected CRS: %s  Vertical CRS(Geoid): %s  Local System: %s  Distances:%s  Angles: %s\n"
9,83,"Distance > %d"
9,84,"Offset > %d"
9,85,"You must select a datum"
9,86,"You must select a local system file"
9,87,"Error when creating local system file"
9,88,"All"
9,89,"Filter using File"
9,90,"Export to *.w84 File"
9,91,"Convert *.w84 File"
9,92,"Origin and target geoids must be the same"
9,93,"Navigator"
9,94,"Ni_Nj"
9,95,"Scale (GPS d./Local d.)"
9,96,"GPS H.dif.-Local H.dif."
9,97,"GPS Az.-Local Az."
9,98,"Standard Desviation"
9,99,"Ambiguity Level"
9,100,"Low"
9,101,"Medium"
9,102,"High"
9,103,"_V_ALIGNMENT"
9,104,"_SUPERELEVATIONS"
9,105,"_THEORETICAL_POINT"
9,106,"_QUICK_PROFILE"
9,107,"_AREA"
9,108,"VAH"
9,109,"SH"
9,110,"Show Vertical Alig. Height"
9,111,"Show Surface Height"
9,112,"You must select a horizontal alignment or a surface"
9,113,"Basic"
9,114,"Manage"
9,115,"Current cross section"
9,116,"Semi-Major Axis must be greater than 0.0"
9,117,"Inverse Flattening must be greater than 0.0"
9,118,"Group"
9,119,"Direct"
9,120,"Inverse"
9,121,"Source Ellipsoid"
9,122,"Target Ellipsoid"
9,123,"Direction"
9,124,"NTv2 Grid"
9,125,"3 Parameters to WGS84"
9,126,"7 Parameters to WGS84"
9,127,"Error when reading datums file"
9,128,"The datum shift of current projected CRS doens't exist"
9,129,"Source and target datum shifts must be the same"
9,130,"Slopes"
9,131,"Manual Cross Sections"
9,132,"Ref. Station"
9,133,"New WGS84 Ref. Station"
9,134,"Move Coordinates"
9,135,"You must select a reference station"
9,136,"You must select a initial point"
9,137,"You must select a final point"
9,138,"Create HTML report"
9,139,"HTML report created"
9,140,"Sat."
9,141,"WGS84 h"
9,142,"Show Meas."
9,143,"Initial C."
9,144,"Final C."
9,145,"Setting Out by Codes"
9,146,"Code %s does not exist"
9,147,"x"
9,148,"y"
9,149,"z"
9,150,"H"
9,151,"h"
9,152,"E"
9,153,"N"
9,154,"Source CRS"
9,155,"Target CRS"
9,156,"Ellipsoidal"
9,157,"Orthometric"
9,158,"Datum Shift"
9,159,"Geodesy"
9,160,"Datum Shifts"
9,161,"Projected CRSs"
9,162,"Ef - Ei"
9,163,"Nf - Ni"
9,164,"hf - hi"
9,165,"Hf - Hi"
9,166,"xf - xi"
9,167,"yf - yi"
9,168,"zf - zi"
9,169,"Offsets"
9,170,"Geographic WGS84"
9,171,"Coordinate Reference System"
9,172,"Compound"
9,173,"Local"
9,174,"Vertical CRS"
9,175,"Projected CRS"
9,176,"CRS Type"
9,177,"Local System"
9,178,"Geo.Dat.Shift"
9,179,"Ver.Dat.Shift"
9,180,"CRSs"
9,181,"Geographic CRSs"
9,182,"Geocentric CRSs"
9,183,"Vertical CRSs"
9,184,"Geodetic Datums"
9,185,"Vertical Datums"
9,186,"Geo. Datum Shifts"
9,187,"Ver. Datum Shifts"
9,188,"Geodetic"
9,189,"Vertical"
9,190,"Geographic"
9,191,"Geocentric"
9,192,"Vertical"
9,193,"Projected"
9,194,"User"
9,195,"EPSG"
9,196,"Data Source"
9,197,"Search By"
9,198,"Area"
9,199,"Prime Meridian"
9,200,"Unsupported CRS"
9,201,"Unsupported Datum Shift"
9,202,"Source Datum"
9,203,"Target Datum"
9,204,"You must select a geodetic datum shift"
9,205,"You must select a vertical CRS"
9,206,"You must select a vertical datum shift"
9,207,"Geocentric"
9,208,"Geographic"
9,209,"Projected"
9,210,"You must select a geodetic CRS"
9,211,"Source Data"
9,212,"Target Data"
9,213,"Geographic CRS"
9,214,"Geocentric CRS"
9,215,"Invalid source data"
9,216,"Invalid target data"
9,217,"Information Source"
9,218,"Base N."
9,219,"Rover N."
9,220,"New Local System"
9,221,"Edit Local System"
9,222,"Import Local System"
9,223,"Delete Local System"
9,224,"Error when deleting WMS server"
9,225,"Error when creating WMS server"
9,226,"Error when editing WMS server"
9,227,"Are you sure you want to delete the current WMS server?"
9,228,"You must select at least one layer"
9,229,"Error when updating NTRIP servers file"
9,230,"Error when updating operators file"
9,231,"Error when reading NTRIP servers file"
9,232,"Error when reading operators file"
9,233,"Error when creating NTRIP servers file"
9,234,"Error when creating operators file"
9,235,"Other"
9,236,"Save operator data..."
9,237,"Save NTRIP server data..."
9,238,"NTRIP Server"
9,239,"Delete current NTRIP server"
9,240,"Delete current operator"
9,241,"Are you sure you want to delete current NTRIP server?"
9,242,"Are you sure you want to delete current operator?"
9,243,"Convert NMEA GGA File..."
9,244,"GGA File"
9,245,"Projected C. File"
9,246,"You have exceeded the time limit in demo mode. The application will close"
9,247,"You have exceeded the number of points recorded in demo mode. The application will close"
9,248,"Favorites"
9,249,"Favorite"
9,250,"This command is not available in DEMO version"
9,251,"The horizontal alignment length must be lower than 100m"
9,252,"You must select the type of local system"

10,1,"Activate Near Point"
10,2,"Desactivate Near Point"
