[    ]//Status Bar
[Durum Çubuğu]
[   Radius]
[   Yarıçap]
[   Turn]
[   Dön]
[  BaseOccups: ]//log message
[]
[ - disable]//log message
[ - aktif değil]
[ - failed to filtering]//log message
[]
[ (!!!Sentinel driver is not installed.)]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->Codes list title (warning)
[]
[ (Ignored for fixed point)]//log message
[]
[ (Obs N %d)]
[]
[ (Occup N %d)]
[]
[ (Recovered) ]//TTools;TLink; window title; additional part to file name, when file was recovered
[ (Kurtarıldı) ]
[ : no Cross Sections]//TTools->CoGo; Convert road to DTM
[]
[ : no Points]//TTools->CoGo; Convert road to DTM
[]
[ : no Vertical Profiles]//TTools->CoGo; Convert road to DTM
[]
[ + Azimuth Absence]//TTools; Adjustment; diagnistic message
[]
[ C/A]//TT->Residiul view window->legend window
[]
[ Conditional]//TTools; Adjustment; diagnistic message
[]
[ Constraint]//TTools; Adjustment; diagnistic message
[]
[ did not receive HORZ coordinates]//TTools; Adjustment; diagnistic message
[]
[ did not receive VERT coordinates]//TTools; Adjustment; diagnistic message
[]
[ failed to load : %s]//error message
[]
[ Inner]//TTools; Adjustment; diagnistic message
[]
[ Minimal]//TTools; Adjustment; diagnistic message
[]
[ points]//TTools; Adjustment; diagnistic message
[]
[ RMS=%.3f ]//message
[]
[ RoverOccups: ]//log message
[]
[ tag]
[]
[ x=%.3f y=%.3f z=%.3f]//message
[]
[#]//TTools, TLink; Tab View; DL tab; field ordinal number |TL and TT->TSObs tab->right and left panel->index number; Tape Dimensions tab->index number;
[]
[#User]//TTools and TLink, default name for new anonymous point created by Add Point
[]
[%]//TT->X-Section Templates tab->right panel->X-Section segment properties->field name
[]
[%d Iterations are not enough. Subnetwork Adjustment failed]//TTools;  error message under Adjustment
[]
[%d Point(s) are out of Adjustment]//TTools; diagnostic message during Adjustment
[]
[%d points are NOT adjusted by %s due Control absense or Errors]//TTools; Adjustment; diagnostic message
[]
[%d points are NOT adjusted by %s due Control absense or Unresolved resections]//TTools; Adjustment; diagnostic message
[]
[%d Points did not receive Coordinates]//TLink, rcdefs.h; diagnostic message during Compute coordinate
[]
[%d Points did not receive Vert-coordinates]//TLink, rcdefs.h; diagnostic message during Compute coordinate
[]
[%d pt]//message|TTools->Layer properties->Line width->list box content|TT->Linework tab->Line properties->Line width->list box content
[]
[%s %s: unknown value %s = %s]
[]
[%s Blunders, UWE = %.2lf]//TTools; Adjustment; diagnistic message
[]
[%s, Constraint]//TTools; Adjustment Report, Output use
[]
[%s, Inner constraint]//TTools; Adjustment Report, Output use
[]
[%s, Minimal constraint]//TTools; Adjustment Report, Output use
[]
[%sPoint %s has bad %s attachment]//TTools;   error message under Adjustment
[]
[%u points without code cannot be exported to SHP]//message box
[]
[&&]
[]
[&3D View]//TTools menu View
[]
[&About Topcon Link...]
[&Topcon Link Hakkında...]
[&About Topcon Link...\nDisplays the program information and copyright\nAbout Topcon Link]//TL->Tool Bar->Help->About Topcon Tools
[&Topcon Link Hakkında...\nProgram bilgisi ve telif hakkı görüntüleme\nTopcon Link Hakkında]
[&About Topcon Tools...]
[]
[&About Topcon Tools...\nDisplays the program information and copyright\nAbout Topcon Tools]//TT->Tool Bar->Help->About Topcon Tools
[]
[&Add\\&Add to Surface\nAdd Points and Lines to Surface\nAdd Points and Lines to Surface]//TT->Tool Bar->Edit->Add->Add to Surface
[]
[&Add\\&Append Points to Line\nAppend Points to Line\nAppend Points to Line]//TT->Tool Bar->Edit->Add->Append Points to Line
[]
[&Add\\&Insert Points to Line\nInsert Points to Line\nInsert Points to Line]//TT->Tool Bar->Edit->Add->Insert Points to Line
[]
[&Add\\Arc]//TTools->Tool bar->Edit->Add Arc
[]
[&Add\\Area]//TTools->Tool bar->Edit->Add Area
[]
[&Add\\DistAz Offset Point...]//for internal use only
[]
[&Add\\Layer...]//TTools, main menu
[]
[&Add\\Line]//TTools, main menu
[]
[&Add\\Manual DL Run...]//TTools, main menu
[]
[&Add\\Manual TS Occupation...]//TTools, main menu
[]
[&Add\\New DynaUser...]
[]
[&Add\\Point...]//TTools and TLink, main menu
[&Ekle\\Nokta...]
[&Add\\PTL Offset Point...]//for internal use only
[&Ekle\\PTL Ofset Noktası...]
[&Add\\Road...]//TTools, main menu
[]
[&Add\\Surface...]//TTools, main menu
[]
[&Add\\X-Section Template]//TTools, main menu
[]
[&Adjustment]//1) Menu bar; Process (TTools spec.); menu item  2) Menu bar; Process (TTools spec.); Process Properties dialog, page name
[]
[&Antennas List]//TTools -> Tabular View -> View menu set
[]
[&Arrange &Icons]
[&İkonları &Sırala]
[&Arrange Icons\nArrange icons at the bottom of the window\nArrange Icons]//TL->Tool Bar->Window|TT->Tool Bar->Window
[&İkonları Sırala\nPencerenin altına ikonları sırala\nİkonları Sırala]
[&Background Images...\nRun Background Images dialog\nBackground Images]//TT->Tool Bar->View->Background Images
[]
[&CAD View]//TTools->Menu Bar->View
[&ÇİZİM Ekranı]
[&Cascade]
[]
[&Cascade\nArrange windows so they overlap\nCascade Windows]//TL->Tool Bar->Window|TT->Tool Bar->Window
[&Basamakla\nÇakışma pencereleri sıraya koyun\nPencereleri Basamakla]
[&Close Job]
[]
[&Close Job\nClose the job\nClose Job]//TT->Tool Bar->Job->Close Job
[&İşi Kapat\nİşi kapat\nİşi Kapat]
[&COGO]//TL->Tool Bar (for internal use)|TT->Tool Bar
[&KOGE]
[&Compare Surfaces...]//TTools->CoGo->Compare Surfaces
[]
[&Compute Coordinates]//Menu bar; Process (TLink spec.); menu item
[&Koordinatları Hesapla]
[&Configuration...\nOpen Configuration Dialog\nConfiguration]//TL->Open Configuration window(TL->Tool Bar->File->Configuration)
[&Konfigürasyon...\Konfigürasyon Menüsü Aç\nKonfigürasyon]
[&Configuration...\tCtrl+F2]
[&Konfigürasyon...\tCtrl+F2]
[&Context Help]
[&Yardım Menüsü]
[&Context Help\nShow context help on a specified item\nContext Help]//TL->Tool Bar->Help->Context Help|TT->Tool Bar->Help->Context Help
[]
[&Copy]
[&Kopyala]
[&Copy\nCopy the selection and put it on the Clipboard\nCopy]//TL->Tool Bar->Edit->Copy|TT->Tool Bar->Edit->Copy
[&Kopyala\nPanoda seçili olanı kopyala\nKopyala]
[&Copy\tCtrl+C]//TTools; CoGoLine; Pop-up menu item|Ttools->Layers Control->Layers Combo box->Pop-up menu item|TTools and TLink->Menu Bar->Edit|TTools and TLink->Import from Device->Pop-up menu item|TTools and TLink->Cad View and Map View->Pop-up menu item|TT->Codes window->Pop-up menu item|TT->Occupation View window->Pop-up menu item on occupation|TT->Residiul View window->Pop-up menu item on Residiul|TTools and TLink->Menu Bar->Edit
[&Kopyala\tCtrl+C]
[&Customize...]
[&Özelleştir...]
[&Delete\nErase the selection\nErase]//TL->Tool Bar->Edit->Delete|TT->Tool Bar->Edit->Delete
[&Sil\nSeçileni sil\nSil]
[&Delete\tDel]//TTools; CoGoLine; Pop-up menu item|Ttools->Layers Control->Layers Combo box->Pop-up menu item|TTools and TLink->Menu Bar->Edit|TTools and TLink->Import from Device->Pop-up menu item|TTools and TLink->Cad View and Map View->Pop-up menu item|TT->Codes window->Pop-up menu item|TT->Occupation View window->Pop-up menu item on occupation|TT->Residiul View window->Pop-up menu item on Residiul|TTools and TLink->Menu Bar->Edit
[&Sil\tDel]
[&DGPS PostProcessing]//????hint text in the Status Bar
[]
[&Disable\tCtrl+D]
[&Aktif değil\tCtrl+D]
[&Edit]//TL->Tool Bar|TT->Tool Bar
[&Düzelt]
[&Enable\nEnable the selected object(s)\nEnable object(s)]//TT->Tool Bar->Edit->Enable
[]
[&Enable\tCtrl+E]
[&Aktif\tCtrl+E]
[&Export...]//TTools->Menu Bar->Job->menu item
[]
[&Feedback\\&Question To Support...\nSend question to support by E-mail\nQuestion To Support]//TL->Tool Bar->Help->FeedBack->Question To Support
[]
[&Feedback\\&Question To Support...\nSend question to support by E-mail\nQuestion To Support...]//TT->Tool Bar->Help->FeedBack->Question To Support
[]
[&Feedback\\&Send Bug Report...\nSend bug report by E-mail\nSend Bug Report]//TL->Tool Bar->Help->FeedBack->Send Bug Report
[]
[&Feedback\\&Send Bug Report...\nSend bug report by E-mail\nSend Bug Report...]//TT->Tool Bar->Help->FeedBack->Send Bug Report
[]
[&Feedback\\&Topcon on Web...\nVisit Topcon web site\nTopcon on Web]//TL->Tool Bar->Help->FeedBack->Topcon on Web
[]
[&Feedback\\&Topcon on Web...\nVisit Topcon web site\nTopcon on Web...]//TT->Tool Bar->Help->FeedBack->Topcon on Web
[]
[&File]//TL->Tool Bar
[&Dosya]
[&File properties...]
[&Dosya özellikleri...]
[&File Properties...\nDisplay properties of the current file\nFile Properties]//TL->Open File properties window(TL->Tool Bar->File->File Properties)
[&Dosya Özellikleri...\nGeçerli dosyanın özelliklerini göser\nDosya Özellikleri ]
[&Filters...]
[&Filitreler...]
[&Filters...\nSet miscellaneous filters\nFilters]//TT->Tool Bar->View->Filters
[]
[&GPS+ PostProcessing]//TT->Tool Bar->Process->GPS+ PostProcessing
[]
[&Help]//TL->Tool Bar|TT->Tool Bar
[&Yardım]
[&Help Topics]
[]
[&Help Topics...\nDisplay help topics\nHelp Topics]//TT->Tool Bar->Help->Help Topics
[]
[&Intersection...]//TTools; Menu Bar; COGO; menu item Intersection...
[]
[&Invert Selection]//TT->Tool Bar->Select->command name
[]
[&Job]//TT->Tool Bar
[]
[&Job Configuration...\nOpen Job Configuration Dialog\nJob configuration]//TT->Tool Bar->Job->Job Configuration
[]
[&Job configuration...\tCtrl+F2]
[]
[&Layers]//TTools -> Menu Bar -> View -> Layers
[&Tabakalar]
[&Loop Closures]//TT->Tool Bar->Process-> Loop Clousures command
[]
[&Map View]//TTools->Menu Bar->View
[&Harita Görünümü]
[&Messages]
[]
[&New Code]//TT->Codes window->Pop-up menu item
[&Yeni Kod]
[&New Job...]
[&Yeni İş...]
[&New Job...\nCreate a new job\nNew Job]//TT->Tool Bar->Job->New Job
[]
[&Occupation View Options...]
[]
[&Open File...\nOpen an existing file\nOpen File]//TL->Opening a file(Tool Bar->File->Open File)
[&Dosya Aç...\nVarolan dosya açık\nDosya Aç]
[&Open File...\tCtrl+O]
[&Dosya Aç...\tCtrl+O]
[&Open Job...]
[&İş Aç...]
[&Open Job...\nOpen an existing job\nOpen Job]//TT->Tool Bar->Job->Open Job
[]
[&Paste\nInsert Clipboard contents\nPaste]//TL->Tool Bar->Edit->Paste|TT->Tool Bar->Edit->Paste
[&Yapıştır\nPano içeriklerini ekleyin\nYapıştır]
[&Paste\tCtrl+V]//Ttools->Layers Control->Layers Combo box->Pop-up menu item|TTools and TLink->Menu Bar->Edit|TTools and TLink->Import from Device->Pop-up menu item|TT->Codes window->Pop-up menu item|TTools and TLink->Menu Bar->Edit
[]
[&Point In Direction...]//TTools; Menu Bar; COGO; menu item Point In Direction...
[]
[&Print]
[]
[&Print...\nPrint the active document\nPrint]//TL->Tool Bar->File->Print|TT->Tool Bar->Job->Print
[&Yazdır...\Aktif dokümanı yazdır\nYazdır]
[&Print...\tCtrl+P]
[&Yazdır...\tCtrl+P]
[&Process]//TL->Tool Bar|TT->Tool Bar
[&Proses]
[&Redo\nRedo the previously undone action\nRedo]//TL->Tool Bar->Edit->Redo|TT->Tool Bar->Edit->Redo
[&Yenile\nÖnceden yapılmamış uygulamaları yenile\nYenile]
[&Redo\tCtrl+Y]
[&Yenile\tCtrl+Y]
[&Remote Users...\nOpen Remote Users Dialog\nRemote Users]//TT->Tool Bar->Job->Remote Users Managment
[]
[&Report]//TTools; CoGoLine; Pop-up menu item|not used|TL->Tool Bar (for internal use)|TT->Tool Bar
[]
[&Report Configuration]//TT->Tool Bar->Report->command name
[]
[&Restore All]
[]
[&Save File...\tCtrl+S]
[]
[&Save File\nSave the active file\nSave File]//TL->Saving a file(Tool Bar->File->Save File)
[&Dosyayı Kaydet\nAktif dosyayı kaydet\nDosyayı Kaydet]
[&Save Job]
[]
[&Save Job\nSave the job\nSave Job]//TT->Tool Bar->Job->Save Job
[]
[&Select]//TL->Tool Bar (for internal use)|TT->Tool Bar
[&Seç]
[&Select All]
[]
[&Status Bar]
[&Durum Çubuğu]
[&Status Bar\nShow or hide the status bar\nToggle StatusBar]//TL->Tool Bar->View->Status Bar|TT->Tool Bar->View->Status Bar
[&Durum Çubuğu\nDurum Çubuğunu göster ya da gizle\nDurum Çubuğunu Değiştirme]
[&Tabular View Options...]
[&Tablo Görünüm Seçenekleri...]
[&Tabular View\nShow or hide tabular view window\nTabular view window]//TT->Tool Bar->View->Tabular View
[&Tablo Görünümleri\nTablo Görünüm penceresini göster yada gizle\nTablo görünüm penceresi]
[&Tabular view\tCtrl+T]
[&Tablo Görünümleri\tCtrl+T]
[&Toolbar]
[]
[&Toolbar\nShow or hide the toolbar\nToggle Toolbar]//TL->Tool Bar->View->Tool Bar
[&Araç Çubuğu\Araç Çubuğunu göster ya da sakla\nToogle Araç Çubuğu]
[&Tools]//TL->Tool Bar (for internal use)|TT->Tool Bar->for internal use
[&Araçlar]
[&Traverse...]//TTools; Menu Bar; COGO; menu item Traverse...
[]
[&Undo\nUndo the last action\nUndo]//TL->Tool Bar->Edit->Undo|TT->Tool Bar->Edit->Undo
[&Geri Al\nSon uygulamayı geri al\nGeri Al]
[&Undo\tCtrl+Z]
[&Geri Al\tCtrl+Z]
[&View]//TL->Tool Bar|TT->Tool Bar
[&Görünüm]
[&Window]//TL->Tool Bar|TT->Tool Bar
[&Pencere]
[&Zoom]
[&Zoom]
[&Zoom\\&Restore All\nFit all elements to the graphic view\nRestore All]//TL->Tool Bar->Edit->Zoom->Restore All|TT->Tool Bar->Edit->Zoom->Restore All
[&Zoom\\&Tümünü Göster\nGrafik ekranda tüm objeleri göster\nTümünü Yenile]
[&Zoom\\Zoom &Back\nZoom the graphic view back to it's previous state\nZoom Back]//TL->Tool Bar->Edit->Zoom->Zoom Back|TT->Tool Bar->Edit->Zoom->Zoom Back
[&Zoom\\Yaklaştır &Geri\nGrafik ekranı geri al\Geri Al]
[&Zoom\\Zoom &In\nZoom the graphic view in\nZoom In]//TL->Tool Bar->Edit->Zoom->Zoom In|TT->Tool Bar->Edit->Zoom->Zoom In
[&Zoom\\Yaklaş\nGrafik görüntüde yaklaş\nYaklaş]
[&Zoom\\Zoom &Out\nZoom the graphic view out\nZoom Out]//TL->Tool Bar->Edit->Zoom->Zoom Out|TT->Tool Bar->Edit->Zoom->Zoom Out
[&Zoom\\Uzaklaş\nGrafik görüntüde uzaklaş\nUzaklaş]
[(c) Topcon Positioning Systems]//for internal use only|log message
[(c) Topcon Positioning Systems]
[(channel)]
[]
[(delta time)]
[]
[(disabled), ]//log message
[(aktif değil),]
[(polynom degree)]
[]
[(satellite)]
[(uydu)]
[*.??D;*.??G;*.??N]//Compact RINEX file extensions
[]
[*.??O;*.??G;*.??N]//RINEX file extensions
[]
[*.dl;*.lev;*.txt]//TTools; Import, Export; Format name; extensions
[]
[*.rw5;*.raw]//Import,Convert: Format Extensions
[]
[, TS Obs ]//diagnostic message during Compute coordinate
[]
[...]//TTools; Inverse; for diagnistic message  |TLink->Convert File dialog->button name|TT->Startup dialog->buttom name
[]
[; Command: ]//Tools&link - message in message log on command execution|Tools&link - message in message log on command execution|TL->log message|TT->log message
[]
[[Default (%s)]]//default value for advanced import/export options
[]
[[Default]]//default value for advanced import/export options
[]
[\r\n  Point %s is absent]//TTools; CoGo; error message
[]
[\r\nContinue ?]//diagnostic message during Adjustment and Compute coordinate     
[]
[_]//TLink; Resect Export, Empty Measurement
[]
[<<]//TTools->Export->Cut Sheet  user-defined format->button|TTools and TLink->Tabular View->Options->button|TTools; Background images dialog;|TTools->File->Remote Users->button
[]
[<< Back]//TTools and TLink->Export to Device and Import from Device->button name
[]
[<<Prev]
[]
[> in dialog ]//log message
[]
[> in Tabular View]//log message
[]
[>>]//TTools->Export->Cut Sheet  user-defined format->button|TTools and TLink->Export files and Convert File->Custom format properties->button|TTools and TLink->Tabular View->Options->button|TTools; Background images dialog;|Resolve Duplicate Points dialog|TTools->File->Remote Users->button
[]
[1/f]//for internal use only
[]
[1:n]//TT->X-Section Templates tab->left panel->part of the column name
[]
[1D]//TTools; Adjustment; objects description
[]
[1st Azimuth is Absent]//diagnostic message during Adjustment and Compute coordinate     
[]
[1st Station has'nt Coordinates]//diagnostic message during Adjustment and Compute coordinate       
[]
[2D]//TTools; Adjustment; objects description      
[]
[3D]//TTools; Adjustment; objects description
[]
[3D View]//TTools->Window title
[]
[68%]//TTools; Process Properties dialog (TTools spec.);Adjustment page,  radio button
[]
[95%]//TTools; Process Properties dialog (TTools spec.);Adjustment page,  radio button
[]
[99%]//TTools; Process Properties dialog (TTools spec.);Adjustment page,  radio button
[]
[a]//for internal use only
[]
[A configuration name cannot contain any of the following characters: ]//Configuration name dialog (Job configuration->Save configuration)
[]
[A curve with the given parameters can not be created, so it is converted to a 2-point curve]
[]
[A curve with zero radius can not be created]
[]
[Abbreviation of agency]//TLink; DL BlueBook Export Options, Order and class of survey input field name
[]
[Abbreviation of Submitting Organization]//TLink; GPSDataTransfer Export Options, Processing  Agency Code input field name|TLink; BlueBook Export Options, Processing  Agency Code input field name
[]
[Abort operation in progress?]//message box
[]
[Abort sending only current file?]//Sending file dlg->Cancel button->text of Msg box
[]
[Aborted by user]//TTools and TLink; message|log message during Convert File
[]
[About Topcon Link]//TL->Tool Bar->Help->About Topcon Link
[]
[About Topcon Tools]//TT->Tool Bar->Help->About Topcon Tools
[]
[Absent]//TTools and TLink -TabView->GPSObs Tab-> possible value in the Orbit column
[]
[Absolute]//TT->Point tab->Properties for Point->Offset tab->radio button name
[]
[Accepted Blunder Equations: ]//TTools;  error message under Adjustment
[]
[Access C&odes...\nDisplays Access Codes Dialog\nAccess Codes]//TT->Tool Bar->Help->Access Codes
[]
[Access Code]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->column name
[]
[Access Code is available from Topcon Sales Support]//TT->Enter Access Code dialog->text under the upper panel
[]
[Activate Task List]//not used
[]
[Active]//TT->Tool Bar->View->Layers->Column name
[]
[Active layer cannot be invisible]//TT->error message
[]
[Add]//TTools; Codes; Menu Attribute properties; button|TTools and TLink->Custom Antennas List->button name|TTools and TLink->Custom Cameras List->button name|TT and TL->Job Configuration->Coordinate Systems->Geoid List->button name|TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument->button name
[Ekle]
[Add a new arc to the linework\nAdd an arc]//TTools->Add Arc->hint text
[]
[Add a new closed line to the job\nAdd closed line]//TTools->Add Area->hint text
[]
[Add a new distance&azimuth offset point to the current job\nAdd DistAz Offset Point]//for internal use only
[]
[Add a new DL Obs Run to the current job\nAdd Manual DL Run]//tooltip for Add DL Run menu item
[]
[Add a new DL Obs to the current job\nAdd Manual DL Obs]//tooltip for Add DL Obs menu item
[]
[Add a new horizontal element to the road\nAdd line to road]//tooltip for Add Horz. Element dialog
[]
[Add a new layer to the current job\nAdd Layer]//TTools, tooltip
[]
[Add a new line to the current job\nAdd Line]//TTools, tooltip
[]
[Add a new point to the current job\nAdd Point]//TTools and TLink, tooltip
[]
[Add a new PTL offset point to the current job\nAdd PTL Offset Point]//for internal use only
[]
[Add a new road to the current job\nAdd Road]//tooltip for Add Road dialog
[]
[Add a new surface to the current job\nAdd Surface]//TTools, tooltip
[]
[Add a new TS Obs to the current job\nAdd Manual TS Obs]//tooltip for Add TS Obs menu item
[]
[Add a new TS Occupation to the current job\nAdd Manual TS Occupation]//tooltip for Add TS Run menu item
[]
[Add a new vertical element to the road\nAdd vertical element to road]//TT->Roads tab
[]
[Add a new X-Section template to the current job\nAdd X-Section template]//tooltip for Add X-Section template dialog
[]
[Add a new X-Section to the road\nAdd X-Section to road]//tooltip for Add X-Section dialog
[]
[Add Arc]//TTools->Tool bar->Edit->Add->Arc
[]
[Add Area]//TTools->Tool bar->Edit->Add->Area
[]
[Add background image(s) to job]//Ttools->view->Background images->Undo operation name
[]
[Add code]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->button name
[]
[Add Converted Background Image(s)]
[]
[Add DistAz Offset Point]//for internal use only
[]
[Add DynaUser]
[]
[Add DynaUser\nAdd DynaUser]
[]
[Add files]//not used
[]
[Add Group]//Remote users dlg->button caption
[]
[Add Horz Element]//TT->Roads tab->left panel->Add Horz. Element
[]
[Add image]//TTools; Background images dialog;
[]
[Add Image Measured Point]//action name for undo|name for undo operation after point creation based on image measurements
[]
[Add Image Measurement]//CAD View window, dialog caption (when adding image measurements)
[]
[Add Kinematic fan %s->%s to processing]//log message
[]
[Add Layer]//TTools -> Menu Bar -> View -> Layers -> Layers window -> Pop-up menu item
[]
[Add Line]//Toolbar with parameters for Add Line command
[]
[Add Manual DL Obs]//TTools, caption of Add DL Obs dialog
[]
[Add Manual DL Run]//TTools, caption of Add DL Run dialog
[]
[Add Manual TS Obs]//TTools, caption of Add TS Obs dialog
[]
[Add Manual TS Occupation]//TTools, caption of Add TS Run dialog
[]
[Add New Device]//TTools and TLink->Export to Device and Import from Device->Pop-up menu item
[]
[Add new Offset to X-Section Template\nAdd new Offset]//TT->X-Section Templates tab->right panel->hint text
[]
[Add Next Element]
[]
[Add Next Obs]
[]
[Add Next Offset]
[]
[Add Next X-Section]
[]
[Add Offset]//TT->X-Section Templates tab->right panel->Pop-up menu item
[]
[Add Photo Note]//TT and TL->Tab View->Point properties->Photo Notes tab->button name
[Foto Notu Ekle]
[Add Plot]
[Çizim Ekle]
[Add Point]//TTools; TLink; Localization window; button name|TTools and TLink, caption of Add Point dialog
[Nokta Ekle]
[Add points and lines to Surface from list\nAdd Points and Lines to Surface]//TTools, tooltip
[]
[Add PTL Offset Point]//for internal use only
[DADB Noktası Ekle]
[Add Road]//TTools, caption of Add Road dialog
[Yol Ekle]
[Add Static vector %s->%s to processing]//log message
[]
[Add Stop&Go fan %s->%s to processing]//log message
[]
[Add Stop&Go vector %s->%s to processing]//log message
[]
[Add Surface]//TTools, caption of Add Surface dialog
[]
[Add to Azimuth]//TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Compute Azimuth->field name
[]
[Add to group...]//TTools->File->Remote users->User prop.->button
[]
[Add to Surface]//TTools, after choosing "Add to Surface" in context menu for points/lines if there is more then 1 Surface in the job
[]
[Add to this Surface]//TTools,context menu on Surface object
[]
[Add User]//Remote users dlg->button caption
[]
[Add user...]//TTools->File->Remote users->group prop.->button
[]
[Add Vert Element]//TT->Roads tab
[]
[Add X-Section]//TT->Roads tab->left panel->Add X-Section
[]
[Add X-Section Template]//TT->X-Section Templates tab->left panel->Pop-up menu item
[]
[Added modules: ]//Access codes dialog
[]
[Adding background image to job]//TTools; Background images;
[]
[Adding report]//message box
[]
[Adj Dimension]//TTools; Adjustment;   objects description
[]
[Adjust Dimension]//TTools; Adjustment; objects description
[]
[Adjust network\nAdjust network]//Menu bar; Process menu(TTools spec.); hint text in the Status Bar          
[]
[Adjusted]//TTools; Adjustment; diagnistic message|TTools; DL Obs Properties dialog; Adjustment Page; field Adjustment Status; field text|TTools and TLink->GPS Obs Properties->Adjust Page->field Adjustment Status->possible value|TTools->Map View->Legend window->point type|not used|TT->Compare Point Report Options->part of the column name|Name Of Vector Type|TT->Point summary Report Options->radio button name|TT->Tool Bar->Select->Select Points->Point type list box->value|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->Adjustment Status list box->value
[]
[Adjusted points filter\nAdjusted points filter]//for internal use only
[]
[Adjusted Subnetworks Count: ]//TTools; Adjustment; diagnistic message
[]
[Adjusted Type]//not used
[]
[AdjustedObj]//TTools;   objects description for Adjustment
[]
[Adjustment]
[]
[Adjustment CANNOT continue without changing]//TTools; Adjustment; diagnistic message
[]
[Adjustment Diagnostic]//TTools; Adjustment; Table header
[]
[Adjustment has NO effect]//TTools; Adjustment; diagnostic message
[]
[Adjustment in Global Coordinates]//TTools; Adjustment; diagnostic message
[]
[Adjustment in Local Coordinates]//TTools; Adjustment; diagnostic message
[]
[Adjustment Report]//TTools; Adjustment Report Options,internal use
[]
[Adjustment Report Options]//TTools; Adjustment Report Options,internal use
[]
[Adjustment residuals]//not used
[]
[Adjustment Result]//TTools; Adjustment; Table header
[]
[Adjustment Status]//TTools, DL Obs Properties dialog; Adjustment Page, field name|TTools and TLink->GPS Obs Properties->Adjust Page->field name|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->list box name
[]
[Adjustment Template]//TTools; Adjustment Report Options,Template name
[]
[Adjustment Type]//TTools; Adjustment; Button name
[Dengeleme Tipi]
[Advanced]
[]
[Advanced GIS]//name of module, in Autorizations dialog and in About
[]
[Advanced options]//TTools and TLink->Import and Export files-Check box
[Gelişmiş seçenekler]
[Advanced Options]//for internal use only
[]
[Albers Equal Area]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[]
[Alias]//TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name|not used
[]
[All]//TT->Loop Closure Report Options window->radio button name|Selection Case|TT->Point summary Report Options->radio button name
[]
[All Diagrams are EMPTY]
[]
[All files]//Send files dlg group caption
[Tüm Dosyalar]
[All files (*.*)]//TTools and TLink -> Import, Export, Convert file-> file format|not used
[Tüm Dosyalar(*.*)]
[All files (*.*)|*.*]//not used
[]
[All files|*.*]//TT and TL->format tree item|not used
[]
[All groups and users will be removed]//Remote users dlg->warning dlg->text
[]
[All methods]//TT->Tool Bar->Select->Select GPS Occup.->Method list box->value
[]
[All points]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[All rights reserved]//TL->Tool Bar->Help->About Topcon Link window->text|TT->Tool Bar->Help->About Topcon Tools window->text
[Tüm hakkı saklıdır]
[All types]//TT->Tool Bar->Select->Select GPS Obs.->Solution type list box->value
[]
[All Users]//Remote users dlg->root item caption
[]
[All vectors]//TT->Repeated Observations Report Options->radio button name
[]
[Allowable deviation]//(select two or more points on MapView window)->(click right button of mouse)->dialog.
[]
[Allowed]//TTools; DL Obs Properties dialog; Adjustment Page; list box AutoReject; list box text|TTools and TLink->GPS Obs Properties->Adjust Page->list box AutoReject->possible value|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->AutoReject list box->value
[]
[Along Line]//TT->Point tab->Properties for Point->Offset tab
[]
[Along Meas.Line]//TT->Point tab->Properties for Point->Offset tab
[]
[Alt]//Shortcut Description
[]
[Always Backup]//TTools->Job Configuration->Save->Backup files from devices->possible value
[]
[Analyse Identical Points]//TTools; Adjustment; Button name
[]
[Analyse Repeated Observations]//TTools; Adjustment; Button name
[]
[and minimum observation duration (h)]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[and/or suffix]//TT and TL->Points tab->Pop-up menu item Rename Points->Points renaming window->text
[]
[Angle]//TTools->CoGo->Traverse; field Name
[]
[Angle Balance]//Process Properties dialog(TLink spec.), page Compute Coordinates;  List box Adjustment type
[]
[Angle format:]//TT ->in advanced import/export options->for internal use
[]
[Angle Left]//TTools->CoGo->Traverse
[]
[Angle Right]//TTools->CoGo->Traverse
[]
[Angle type]//TTools->CoGo->Traverse
[]
[Angles]//TTools->Job Configuration and TLink->Configuration ->Angles tab name
[]
[Angles (Dec.degrees)]//TTools->Job Configuration->Display->Precisions
[Açılar (Dec.derece)]
[Angles (seconds)]//TTools->Job Configuration->Display->Precisions
[Açılar (saniye)]
[Angular Unit]//TTools->Job Configuration->Units->Angular Unit list box name
[]
[Angular unit:]//TT ->in advanced import/export options->list box name (for example export FC5 Raw)
[]
[Anonymous]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Ant Height Method]//TTools and TLink -> Tabular View ->GPS Occupations Tab, column name
[Ant.Yüks.Ölçü Metodu]
[Antenna]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab name
[Anten]
[Antenna calibration set]
[]
[Antenna East Offset]//not used
[]
[Antenna File]
[]
[Antenna height]//TT->Tool Bar->Select->Select GPS Occup.->list box name
[]
[Antenna Height]//TTools and TLink -> Tabular View ->GPS Occupations Tab, column name
[Anten Yüksekliği]
[Antenna North Offset]//not used
[]
[Antenna Serial Number]//for internal use only
[]
[Antenna Type]//TTools and TLink -> Tabular View ->GPS Occupations Tab  -> column name
[Anten Tipi]
[Antenna Vertical Offset]//not used
[]
[Antennas List]//TTools and TLink -> Tabular View -> Antenna list window caption name
[Antenler Listesi]
[APA Coordinates]//TTools and TLink->Import, Export, Convert->Format name;
[]
[APA TS Obs]//for internal use only
[]
[Append a point to the selected line\nAppend Points to Line]//TTools, tooltip
[]
[Append Point(s) to Line]//TTools,context menu for lines
[]
[Append points to the selected line\nAppend Points to Line]//TTools, tooltip
[]
[Apply]//button name|TTools; Filters dialog; button name|button name
[]
[Arc End]//for internal use
[]
[Arc Long Section]//TT->Roads tab->Vert. element->type of the element
[]
[Arc Start]//for internal use
[]
[Are you sure you want to delete these files/folders?]//message box
[]
[Are you sure you want to send job '%s' to the Recycle Bin?]//TT->Sturtup dialog->Delete job->message
[]
[Area]//properties for Surface; column name in Surface tab and in options|TTools->CoGo->Compare Surfaces|for internal use(feature)
[Alan]
[Area: %s sq. %s]//TTools->Map View  and Cad View->trxt in the Status Bar during selecting the area
[]
[Arrange tables by selection]//TT->Tool Bar->Select->Select None->hint text in the Status Bar
[]
[ASCII [TSV]]//not used
[]
[Ask]//TTools; Background images dialog;
[]
[Asterisk (*)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[AT Job Configuration]//TTools TLink internal use only
[]
[AtmosphericCorrection]//for internal use
[Atmosferik Düzeltme]
[Attribute]//TTools; Codes; Atribuite Properties; Caption|TTools->Point Properties->CAD tab->right panel->column name
[Öznitelik]
[Attribute Name]//TTools and TLink->Object name (Attribuite Properties dialog)
[Öznitelik İsmi]
[Attributes]//not used
[]
[Australian Geoid Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Auto]//TTools; Adjustment; Button name|TTools->GPS Vectors Import   |TT and TL->Layers window->Breakline type column ->value|for internal use only|TL->Convert File->Advanced options->radio button name
[]
[Auto correlation]//not used
[]
[Auto Fixing: First & Last Points]//Process Properties dialog, Tlink spec, Compute Coordinates page, field
[]
[Auto Fixing: First & Last Points, First & Last Azimuthes]//Process Properties dialog, Tlink spec, Compute Coordinates page, field
[]
[Auto Fixing: First Point, First & Last Azimuthes]//Process Properties dialog, Tlink spec, Compute Coordinates page, field
[]
[Auto generate job name]//for internal use only
[]
[Auto saving file: ]//TTools;TLink; message  when autosaving a file
[]
[Auto topo occupations]//TT->Occupation View window->Legend window
[]
[Auto Update]//TTools, properties for Surface
[]
[Automatic Blunder Rejection]//TTools; Adjustment; Button name
[]
[Automatic Tests]//for internal use only
[]
[Autonomous]//TTools and TLink->GPS Occupations->Method->possible value
[]
[AutoReject]//TTools, DL Obs Properties dialog; Adjustment Page, list box name name|TTools and TLink->GPS Obs Properties->list box name|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->list box name
[]
[AutoRejected]//TTools; DL Obs Properties dialog; Adjustment Page; field Adjustment Status; field text|TTools and TLink->GPS Obs Properties->Adjust Page->field Adjustment Status->possible value|TT->Tab View->Quality control tab->message|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->Adjustment Status list box->value
[]
[Auto-Rejected]//Name Of Vector Type
[]
[AutoRejected Only]//Selection Case
[]
[Autosave completed, operation returns: ]//TTools; write message in log during the job autosaving
[]
[Autosave Interval (min)]//TTools (Job Configuration) and TLink (Configuration)->Save node->spin control name
[Otomatik Kayıt (dakika)]
[Autosave was aborted by user]
[]
[AutoTopo]//TTools and TLink ->Properties for Occupation->field Method->possible field content
[]
[Autotopo\\Obs\\Disabled]//TTools; Filters window
[]
[Autotopo\\Obs\\Enabled]//TTools; Filters window
[]
[Autotopo\\Occupations]//TTools; Filters window
[]
[Autotopo\\Points]//TTools; Filters window
[]
[Available columns]//TTools and TLink->Tabular View->Options->group box name
[Mevcut sütunlar]
[Available images:]//TTools; Background images dialog;
[Mevcut resimler:]
[Available modules:]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->text in the upper part of the window
[Mevcut modüller:]
[Available report templates:]//TT->Report Configuration->left panel name
[]
[Avg Job Height]//TTools; TLink ->Job Configuration->Coordinate Systems; Grid to Ground window -> field name; or Convert file dialog -> Grid to Ground
[]
[Axis azimuth]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[]
[Azimuth]//TTools spec.; diagnostics about errors under Adjustment when bad connected network|TTools->CoGo->Traverse|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name|TTools and TLink ->GPS Obs tab-> column name|TT->Point tab->Properties for Point->Offset tab->field name|TT->Roads tab->Horz. element->right panel->column name|TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Azimut]
[Azimuth 1]//TTools; CoGo;Intersection
[]
[Azimuth 2]//TTools; CoGo; Intersection
[Azimut 2]
[Azimuth Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[Azimut Kaba Hatası]
[Azimuth Rotation]//TTools; TLink ->Job Configuration->Coordinate Systems; Grid to Ground window -> field name; or Convert file dialog -> Grid to Ground
[Azimut Dönüklüğü]
[Azimuth, Distance, dHt]//for internal use only
[]
[Azimuth, Distance, Elevation Angle]//for internal use only
[]
[Azimuth: %s]//TTools->Map View  and Cad View->trxt in the Status Bar during selecting the area
[]
[Back Sight]//not used
[]
[Back Sights]//not used
[]
[Back Sights List\nBack Sights List]//not used
[]
[BackBearing-Name]//TLink; Resect Export, Header Field name
[]
[Background images]//TTools; Background images dialog; caption
[]
[Background map drawing is not allowed by selected datum]//error message
[]
[Background Map File]//TTools - Map view options and CAD View options
[]
[Backsight Angle]//not used
[]
[Backsight Point]//not used
[]
[Backsight Setting]//TLink->Compute Coordinates->Backsight dialog(for TS measurments)->caption
[BN Ayarları]
[Backspace]//Shortcut Description
[]
[Backup files from devices]//TTools->Job Configuration->Save->list box name
[]
[Backward Azimuth]//TTools; Inverse window; bottom pane and Properties window
[]
[Bad covariance matrix for: ]//TTools; error message under Adjustment
[]
[Bad data on station %s]//diagnostic message during Adjustment and Compute coordinate
[]
[Bad Distance = %.1lfm on TS Obs %s]//diagnostic message during Compute coordinate
[]
[Bad header line: ]//log message
[]
[Bad instrument Ht = %.3lfm on Station %s]//diagnostic message during Compute coordinate
[]
[Bad Inv PTL]//TTools->CoGo;Inv PTL
[]
[Bad reflector Ht = %.3lfm on TS Obs %s]//diagnostic message during Compute coordinate
[]
[Balance]//TTools, TLink; DL Occupation Properties dialog; field name
[]
[Bar (|)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[Base]//TTools and TLink ->Properties for Occupation->field Method->possible field content
[]
[Base Antenna Height]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Base Antenna Type]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Base[%s:%d]: x=%.3f y=%.3f z=%.3f Rover[%s:%d]: x=%.3f y=%.3f z=%.3f]//log message
[]
[Bases]//not used
[]
[Bases\\Occupations]//TTools; Filters window
[]
[Bases\\Points]//TTools; Filters window
[]
[BBFF]//TTools, TLink; DL Occupation Properties dialog; field Type; text
[]
[Bearing]//TTools->CoGo->Traverse|for internal use only???
[]
[Begin a Group]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[Begin Line]//TT and TL->Point Properties->Control code
[]
[Belgium Geoid Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[BenchMark]//for internal use only
[]
[Benchmark Point]//not used
[]
[Best Fit Alignment]//string in the progress bar that shown during the best fit alignment calculating
[]
[Best Fit Alignment Options]//not used! (select two or more points on MapView window)->(click right button of mouse)->dialog->Caption.
[]
[Best Fit Alignment\nBest Fit Alignment]
[]
[BFFB]//TTools, TLink; DL Occupation Properties dialog; field Type; text
[]
[Bitmap files (*.bmp)|*.bmp||]//TT and TL->Map View, Cad View, Occupation View, Residual View->Pop-up menu item Save View to File->Save as->file type
[]
[Bitmap files (*.bmp)|*.bmp|JPEG files (*.jpg)|*.jpg||]//TT and TL->Map View, Cad View, Occupation View, Residual View->Pop-up menu item Save View to File->Save as->file type
[]
[BKB]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[]
[Black]//TTools->attribute properies->color list box->possible value
[]
[BLH]//TTools and TLink->Export files and Convert File->Custom format properties->Coordinate system list box->possible value
[]
[Blue]//TTools->attribute properies->color list box->possible value
[]
[BlueBook]//TLink; GPSDataTransfer Export Options, Name Of Export Filter|TLink; BlueBook Export Options, Name Of Export Filter
[]
[BlueBook Export]//TLink; GPSDataTransfer Export Options,internal use|TLink; BlueBook Export Options,internal use
[]
[BlueBook Sheet]//TLink; GPSDataTransfer Export Options, Name Of Export Filter|TLink; BlueBook Export Options, Name Of Export Filter
[]
[Body Template]//TTools->Report->report Configuration->Localization Report Options->template name
[]
[Both]//TTools; Adjustment; Column name|TTools and TLink->Point Properties->General tab->list box Control->possible value|not used
[]
[Both prefix and suffix are empty. Renaming will have no effect.]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[]
[Both surfaces do not have unical unique projection]//TTools; CoGo; Compare surfaces, error message
[]
[Bottom right corner - X]//Ttools->view->Background images->left panel (Available images)->field name
[]
[Bottom right corner - Y]//Ttools->view->Background images->left panel (Available images)->field name
[]
[Boundary]//TT and TL->Layers window->Breakline type column ->value
[]
[Bounds]//TTools; Adjustment; Column name
[]
[BPW files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[Breakline]//TT and TL->Layers window->Breakline type column ->value
[]
[Breakline Type]//TT and TL->Layers window->Breakline type column ->value
[]
[Broadcast]//TTools and TLink -TabView->GPSObs Tab-> possible value in the Orbit column
[]
[Browse]//TTools - Map view options and CAD View options
[]
[Browse for Device]
[]
[Browse...]//TT->Startup dialog->button name
[]
[BS]//TTools, TLink; DL Obs Properties dialog; General Page, Type, field content|TTools->DL Obs Report -> Options dialog ->  column name|TT and TL->Properties for TS Obs->General tab->Type list box->value
[]
[BS Azimuth]//TTools->CoGo->Traverse
[]
[BS Bearing]//TTools->CoGo->Traverse
[]
[BS Point]//TTools->CoGo->Traverse	
[]
[Build date is: %#x]//TL->Tool Bar->Help->About Topcon Link window->text|TT->Tool Bar->Help->About Topcon Tools window->text
[Sürüm tarihi: %#x]
[build July 25, 2002]//log message
[]
[build November 17, 2000]//for internal use only
[]
[Button appearance]//Ttools; Customize toolbars window; Button settings dialog; text for radio button group
[]
[Button name]//Ttools; Customize toolbars window; Button settings dialog; field name
[]
[Button Settings]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[By Code]//TT->Filters window->tab name
[]
[By QAQC]//TTools->Filters
[]
[By Quality Control]//Process Properties dialog, Ttools spec., Adjustment page,  radio-button
[]
[By Time]//TT->Filters window->tab name
[]
[By Type]//Ttools; Filter dialog; Page name
[]
[BYCODE]//TTools->Linework->Properties of Line|TT->Tab View->Layer column->possible value
[]
[BYLAYER]//TTools->Linework->Properties of Line|TT->Codes->Properties->Plotting styles->list box content
[]
[bytes]//units of files size - send file dialog
[]
[C&odes]//TTools; Tool Bar; View; Codes
[]
[CAD]//TTools and TLink->Point Properties->Cad tab->tab name|not used
[CAD]
[CAD View]//TTools->Window title
[CAD Görünümü]
[CAD View Item]//for internal use only
[CAD Görünüm Item]
[CAD View Item Options]
[]
[CAD View Options]//TTools->window name|header of "CAD View Options" dialog (View->CAD View Options)|header of "CAD View Options" dialog (View->CAD View Options)
[]
[Calc]//TTools; Inverse window; Calculate button
[]
[Calculate]
[]
[Calculate coordinates of the point in given direction\nPoint In Direction]//TTools, hint text in Status Bar
[]
[Calculate coordinates of the traverse points\nTraverse]//TTools, hint text in Status Bar
[]
[Calculate nearest distance from the given point to the given line\nInverse Point to Line]//TTools, hint text in Status Bar
[]
[Calculate parameters of distance and azimuth between two points\nInverse]//TTools, hint text in Status Bar
[]
[Calculate the coordinates of the intersection point(s) of the rays and spheres\nIntersection]//TTools; hint text in the Status Bar
[]
[Camera]//internal use
[Kamera]
[Camera point]//image property name
[Kamera noktası]
[Camera positions are too close. Stereopair cannot be created]//TTools->Stereopairs tab->message
[]
[Can not compute datum transformation parameters: not enough points in list]//TTools; TLink; Datum Transformation; message box while updating Datum Transformation
[]
[Can not compute localization: not enough local point coords]//TTools; TLink; Localization; message box while localization
[]
[Can not compute localization: not enough points in list]//TTools; TLink; Localization; message box while localization
[]
[Can not compute localization: not enough WGS point coords]//TTools; TLink; Localization; message box while localization
[]
[Can not create control window for processing]//log message
[]
[Can not create TPD export session]//log message
[]
[Can not export occupation: ]//log message
[]
[Can not export to same RINEX file occupations that were made by different receivers]//log message
[]
[Can not export to same TPD file occupations that were made by different receivers]//log message
[]
[Can not export to the same file occupations that were made by different receivers]//error message
[]
[Can not open file]//TLink; GPSDataTransfer Export Options, Message on file open failer|TLink; BlueBook Export Options, Message on file open failer
[Dosya açılamıyor]
[Can not overwrite predefined datum]//TTools; TLink; Datum Transformation; message box while saving parameters
[]
[Can not process any of %d vectors]//log message
[]
[Can not process any rays]//log message
[]
[Can not rename points]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[Noktalar yeniden adlandırılamıyor]
[Can not update localization: horizontal localization only]//TTools; TLink; Localization; message box while localization
[]
[Can not update localization: vertical localization only]//TTools; TLink; Localization; message box while localization
[]
[Canadian Geoid Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Cancel]//TTools; Adjustment; Button name|TTools->CoGo; Intersect + PointInDirection + ...|button name|TTools->Export->Cut Sheet  user-defined format->button|Ttools->Map View->Options>MrSid Background file activation->Password window->button name|Cnacel Button|Cancel button|TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Compute Azimuth->button name|TTools->Occupation view->Merge GPS Occupations dialog and Split GPS Occupations dialog->button name|Drag'n'drop menu item|TTools and TLink->Import from Device; Device Properties and Open for Convert->button name|button name|TT->Tool Bar->Process-> Loop Clousures->Loop Clousures window->button name|TT->Tool Bar->Select->Select Points, GPS Obs, TS Obs and etc.->button name|TL->button name|TT->button name|TT->Grid to Ground dialog (from Job configuration for example)->button name|Ttools->Map View->Options>MrSid Background file activation->Password window->button name|Send files dlg button
[Çıkış]
[Cannot add new code: the maximum number of access codes reached. Please, remove unusable codes.]//Access codes dialog->message
[]
[Cannot be deleted]//error message
[]
[Cannot connect to the device]//error message
[]
[Cannot continue Blunder Treatment]//TTools;   error message under Adjustment
[]
[Cannot continue Subnetwork Adjustment]//TTools;  error message under Adjustment
[]
[Cannot delete file on the controller]//TT and TL->Export to Device->log message
[Kontrol Ünitesindeki dosya silinemiyor]
[Cannot detect center]//for internal use only
[]
[Cannot detect corner]//for internal use only
[]
[Cannot open file]//TL->Opening a file->error message|TT->Open recent files->error message
[]
[Cant allocate memory]//error message
[]
[Cant find lib files]//error message
[]
[Cant open file]//error message
[]
[Cant open job history file]//error message
[]
[Cant tranform cs]//error message
[]
[Cant use elevation]//error message
[]
[Cap (^)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[CarrierFixed]//log message
[]
[CarrierFloat]//log message
[]
[Cassini-Soldner]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[]
[Category]
[]
[CE Based Total Station]
[]
[Center]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[Merkez]
[Center detection]//detection type in thumbnail/stereopair view options|for internal use only
[]
[Central meridian]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Merkez meridyen]
[Chain]//for internal use
[KM]
[Chainage]//TT->Job Configuration->Display->Roads tab->Display CL Pos as list box->possible value
[Kilometre]
[Chains]//for internal use only
[KM'ler]
[Chains List\nChains List]//for internal use only
[KM Listesi\nKM Listesi]
[Change the window position]//Command Move for Window; text in the Status Bar
[Pencere pozisyonunu değiştirin]
[Change the window size]//Command Size for Window; text in the Status Bar
[Pencere boyutunu değiştirin]
[Checking license file...]//TT->log message
[]
[Chord]//TT->Roads tab->Horz. element->Properties for Curve, Intersection->field name
[]
[Circular Arc]//TT->Roads tab->Vert. element->type of the element
[]
[CL Positions]//TT->Roads tab->Vert. element->Graphic->axis name
[]
[Cl&ose]
[Ka&pat]
[Class not found]//log error message
[Class bulunamadı]
[Cleaning files...]//log message
[Dosyalar siliniyor...]
[Clear changed status]
[]
[Clear changed status\nClear changed status]
[]
[Clear current selection]//TT->Tool Bar->Select->Select GPS OBS,GPS Occup, Points, TS Obs, TS Occup->check box name
[]
[Clear QC status]//for internal use ??
[]
[Clear QC status and message\nClear QC status and message]//for internal use ??
[]
[Client]//TT->for future release
[]
[CLIP]//TTools->Export->Format name
[]
[Close]//TTools; Inverse window; Close button|button name|TTools; Filters dialog; button name|TTools; TLink; Localization window; button name|TTools and TLink->Custom Antennas List->button name|TTools and TLink->Custom Cameras List->button name|TLink->Convert File dialog->button name|TTools; Background images dialog;|TT and TL->Job Configuration->Coordinate Systems->Geoid List->button name|TT->Report configuration->button name|TT->Startup dialog->button name and Configuration list->button name|TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument->button name|TTools->File->Remote Users->button|Send files dlg button
[Kapat]
[Close Al&l]
[Tümünü Kapat]
[Close Al&l\nClose all open windows\nClose All]//TL->Tool Bar->Window
[Tümünü Kapa&t\nTüm açık pencereleri kapat\nTümünü Kapat]
[Close print preview mode\nCancel Preview]//Close in Print Preview mode; text in the Status Bar
[]
[Close tab]//Msg session dialog->Tab context menu item
[]
[Close the active window and prompts to save the documents]//Command Close for Window; text in the Status Bar
[]
[Close\nClose the window\nClose]//TL->Tool Bar->Window
[Kapat\nPencereyi Kapat\nKapat]
[Code]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TTools and TLink->Export files and Convert File->Custom format properties->field in the left panel|TTools->Linework->Properties of Line|not used|TTools->thumbnail/stereopair view options->Labels tab->Check box|TTools->Map View options and Cad View options->Labels tab->Check box|Resolve Duplicate Points dialog|TT->X-Section Templates tab->right panel->X-Section segment properties->list box name|TT->Tool Bar->Select->Select Points->field name|TT and TL->Properties for TS Obs->General tab->list box name
[Kod]
[Code Diff]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Kod Farkı]
[Code Library]//TTools; Export to File; Format name
[Kod Kütüphanesi]
[Code Smoothing]//TTools->Export(Advanced options for Rinex files)->check box name
[]
[Code status]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->field name
[]
[CodeDiff]//log message
[KodFarkı]
[CodeDiffSmooth]//log message
[]
[Codes]//TTools; Window title|TTools->Menu bar->Edit->Add->Add Line|TTools and TLink->Point Properties->CAD tab->group box name
[Kodlar]
[Codes to filter:]//TT->Filters window->By Code tab->field name
[]
[Code-String combinations can not be repeated]//message box
[]
[Codestrings doesnt exists]//error message
[]
[Coefficient]//for internal use only
[Katsayı]
[cogo]//TTools; CoGo;  Intersection
[koge]
[COGO]//TTools->Map View->Legend window->point type
[KOGE]
[CoGo]
[KoGe]
[COGO points filter\nCOGO points filter]//for internal use only
[]
[CoGoInvPTL]//TTools; CoGo; Inverse PTL, ComObj name(internal use)
[]
[CoGoLine]//TTools; CoGo; Object description; for internal use
[]
[CogoPoint]//TTools; CoGo; Intersection; ComObj name(internal use)
[]
[CogoTraversePoint]//not used
[]
[Color]//TTools->Linework->Properties of Line|TT and TL->Tab View->Point properties->Cad tab->field name
[Renk]
[Combi NDF]//TTools;  objects description for Adjustment
[]
[Combi UWE]//TTools;  objects description for Adjustment
[]
[Combined Grid to Ground Scale Factor]//TTools->Tab View->Point tab ->column name|TT->Point summary Report Options->column name
[]
[Combined Ground to Grid Scale Factor]//TT->Point summary Report Options->column name
[]
[Comma]//TTools and TLink->Export files and Convert File->Custom format properties->Delimeters list box->possible value
[Virgül]
[Comma (,)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[Command executed: ]//Tools&link - message in message log on command execution|Tools&link - message in message log on command execution|TL->log message|TT->log message
[Komut uygulandı:]
[Command execution returns error: ]//Tools&link - message in message log on command execution|Tools&link - message in message log on command execution|TL->log message|TT->log message
[Komut uygulanırken hatayla dönüştü:]
[Command execution returns OK; Command: ]//Tools&link - message in message log on command execution|Tools&link - message in message log on command execution|TL->log message|TT->log message
[Komut uygulanırken OK ye dönün;Komut:]
[Command properties]//for internal use|for internal use
[Komut özellikleri]
[Command Properties]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[Komut Özellikleri]
[Commands]//Tools&link - message in message log on command execution|Tools&link - message in message log on command execution|TL->log message|TT->log message
[Komutlar]
[Comment]//properties for Surface; column name in Surface tab and in options|TT->Job Info->field name
[Açıklama]
[Common Format Image File]//File format description
[]
[Common image files]//for internal use
[]
[Common Image Import Filter]//for internal use
[]
[Common Image Import Filter\nCommon Image Import Filter]//for internal use
[]
[Common Options]//TL->for internal use|TT->for internal use
[]
[Compact RINEX]//Import,Export,Convert Format Name
[Birleşik RINEX]
[Compare Both]//TTools and TLink->Point Properties->General tab->list box Control->possible value|TT->Tab View->Point tab->Control column->possible value
[İkini Uygula]
[Compare Horz]//TTools and TLink->Point Properties->General tab->list box Control->possible value|TT->Tab View->Point tab->Control column->possible value
[Yty'a Uygula]
[Compare Point Report]//TT->Compare Point Report Options window->tooltip
[]
[Compare Point Report Options]//TT->Compare Point Report Options window name
[]
[Compare Points]//TT->Job Configuration->Quality Control->Automatic Tests->check box name
[]
[Compare Points QC filter\nCompare Points QC filter]//internal use
[]
[Compare Surfaces]//TTools->CoGo; DTM compare               
[]
[Compare Surfaces...]//TTools->CoGo->Compare Surfaces
[]
[Compare Surfaces\nView]//TTools->CoGo; DTM compare    
[]
[Compare two surfaces or compare a surface and a horizontal plane\nCompare Surfaces]//TTools->CoGo->Compare Surfaces
[]
[Compare Vert]//TTools and TLink->Point Properties->General tab->list box Control->possible value|TT->Tab View->Point tab->Control column->possible value
[]
[Comparing Surface is corrupt]//TTools->CoGo->Compare Surfaces
[]
[Comparing Surface is not performed]//TTools->CoGo->Compare Surfaces
[]
[Compass Rule]//Process Properties dialog(TLink spec.), page Compute Coordinates;  List box Adjustment type
[]
[Composite Objects]//not used
[]
[Compute Azimuth]//TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Compute...->dialog caption
[]
[Compute Coordinates]//Process properties dialog (TLink spec.); page name
[Koordinatları Hesapla]
[Compute Coordinates has NO effect]//TLink; Compute Coordinates; diagnostic message
[Kootdinatlar Hesaplanmaz. Etkisi yok.]
[Compute coordinates of points\nCompute coordinates of points]//Menu bar; Process menu(TLink spec.); hint text in the Status Bar           
[]
[Compute DOPs]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Compute localization Failed]//TTools; TLink; Localization; message box while localization
[Lokalizasyon hesabı başarılamadı]
[Compute parameters]//TTools; TLink; Localization window; button name
[Hesaplama parametreleri]
[Compute...]//TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Button name
[]
[Confidence Level]//TTools Process Properties dialog (TTools spec.);Adjustment page, caption of the radio button group
[]
[Configuration]//TL->Tool Bar->File->Configuration
[Seçenekler]
[Configuration '%s' already exists]//TT->Enter Configuration->message
[]
[Configuration '%s' already exists. Overwrite?]//TT->Save Configuration->message
[]
[Configuration name ]//TT->Job Configuration->Save Configuration->Enter configuration name window->field name
[]
[Configuration name is empty]////Configuration name dialog (Job configuration->Save configuration)
[]
[Configurations list]//TT->Job Configuration window->List configurations->Configurations list window caption
[]
[Configurations:]//TT->Creare a new job->list box name
[]
[Configure Reports\nConfigure Reports]//TT->hint text
[]
[Constants]
[]
[Constrained %dD Adjustment]//TTools;  error message under Adjustment
[]
[Continue]//TTools; Adjustment; Button name
[]
[Contour Lines]//Contour lines dialog->Caption
[]
[Contr.Horz]//AdjObj.cpp,rcdefs.h;  objects description for Adjustment
[]
[Contr.Vert]//AdjObj.cpp,rcdefs.h;  objects description for Adjustment
[]
[Control]//TT and TL->in advanced import/export options and open file->Point type list box->value|TT->Point summary Report Options->radio button name
[Kontrol]
[Control Code]//TT->Properties for point->String tab->list box name and TTools->Tab View->Line work->field name|TT and TL->Properties for TS Obs->String tab->field name
[Kontrol Kodu]
[Control Code 2]//TTools->Tab View->Line work->field name
[Kontrol Kodu 2]
[Control Code2]//TT and TL->Properties for TS Obs->String tab->field name
[Kontrol Kodu2]
[Control Point is not linked with network]//message
[]
[Control points filter\nControl points filter]//for internal use only
[Kontrol noktlr filitrele\nKontrol noktlr filitrele]
[Control Tie Analysis]//TTools; Adjustment; Button name
[Kontrol Tie Analizi]
[Control Tie Analysis: Success]//TTools; Adjustment; Column name
[Kontrol Tie Analizi: Başarılı]
[Control Tie Analysis: Unfixed Points]//TTools; Adjustment; Table header
[Kontrol Tie Analizi: Noktalar Fix değil.]
[Control Tie Test failed]//TT->QC message
[Kontrol Tie Testi Başarısız]
[ControlCode]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[Kontrol Kodu]
[ControlCode2]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[Kontrol Kodu2]
[Convergence]//TTools->Tab View->Point tab ->column name|TT->Point summary Report Options->column name
[]
[Convert]//TLink->Convert File dialog->button name
[Dönüştür]
[Convert file]//not used
[]
[Convert File]//Conver dialog name
[Dosya Dönüştür]
[Convert File...]//TLink->Menu Bar->File->menu item
[Dosya Dönüştür...]
[Convert files between formats\nConvert files between formats]//TLink->Convert files->text in the Status Bar
[Formatlar arasında dosyaları dönüştür\nFormatlar arasında dosyaları dönüştür]
[Convert image]//TTools->View->Background Images...->select one of the image files in the left pane of dialog->click on button "Convert image" ->message|TTools; Background images dialog;
[]
[Convert image to job coordinate system]//TTools; Background images dialog;
[]
[Convert Options]//for internal use only
[Dünüştürme Seçenekleri]
[Convert road to lines]//TTools->Convert road to Lines
[]
[Convert road to points]//TTools->Convert road to points
[]
[Convert road to surface]//TTools->CoGo; Convert road to DTM
[]
[Convert road to surface\nConvert road to surface]
[]
[Convert\\To Lines]//TTools->Convert road to Lines menu name
[]
[Convert\\To Points]//TTools->Convert road to points menu name
[]
[Convert\\To Surface]//TTools->CoGo; Convert road to DTM
[]
[Coordinate order]//TLink->Open TS Raw Data Files and TTools Import->list box name
[Koordinat düzeni]
[Coordinate order:]//coordinate order in advanced import/export options
[Koordinat düzeni:]
[Coordinate point]//for internal use only
[Nokta Koordinatı]
[Coordinate system]//TTools and TLink->Export files and Convert File->Custom format properties->list box name|Ttools->view->Background images->left panel (Available images)->field name
[Koordinat sistemi]
[Coordinate System]//for internal use only|for internal use only
[Koordinat Sistemi]
[Coordinate system of the background image file and coordinate system of the job are different. The image will not be shown unless you change the coordinate system of the job or convert the image.]//Ttools->view->Background images->Message box when adding an image to job
[]
[Coordinate system:]//coordinate system in advanced import/export options
[]
[Coordinate Systems]//TTools->Job Configuration and TLink->Configuration->left panel->node name
[Koordinat Sistemleri]
[Coordinate type]//TTools->Job Configuration->Coordinate System->List box
[]
[Coordinate type:]//coordinate type in advanced import/export options
[]
[Coordinates]//TTools and TLink->Import, Open, Convert file->Format name
[Koordinatlar]
[Coordinates are unfound]//TTools; CoGo; Traverse, error message
[]
[Coordinates Expansion]//diagnostic message during Compute coordinate
[]
[Coordinates Expansion, Method: %s]//diagnostic message during Compute coordinate
[]
[Coordinates files]//TTools->Export->Format name
[]
[Coordinates(N,E)]//TTools->Job Configuration->Display->Precisions
[Koordinatlar(X,Y)]
[Coordinates\\Grid]//TTools and TLink->Point Properties->Coordinate tab->group box name
[Koordinatlar\\Grid]
[Coordinates\\Ground]//TTools and TLink->Point Properties->Coordinate tab->group box name
[Koordinatlar\\Yer]
[Coordinates\\Lat,Lon]//TTools and TLink->Point Properties->Coordinate tab->group box name
[Koordinatlar\\Enl,Boy]
[Coordinates\\WGS84]//TTools and TLink->Point Properties->Coordinate tab->group box name
[Koordinatlar\\WGS84]
[Copy]//for internal use only|Context menu item on history of messages dlg
[Kopyala]
[Copy Button Image]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[Copy here]//Drag'n'drop menu item
[]
[Copy key]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->button name
[]
[Copy report as ...]//TT->Report Configuration->button name
[]
[Copy View to Clipboard]
[]
[Copyright \251 2003-2006]//TL->Tool Bar->Help->About Topcon Link window->text|TT->Tool Bar->Help->About Topcon Tools window->text
[Tüm Hakkı Saklıdır\ 2003-2007]
[Corner]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[Köşe]
[Corner detection]//detection type in thumbnail/stereopair view options|for internal use only
[]
[Corr NE]//for internal use only
[]
[Corr(X,Y)]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Corr(X,Z)]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Corr(Y,Z)]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[CorrXY]//for internal use only
[]
[CorrXZ]//for internal use only
[]
[CorrYZ]//for internal use only
[]
[CORS Coordinates]//TTools; Import and Export from files; format name; TLink->Convert files->format name
[]
[Could not create the file!]//message box
[]
[Could not load format definition from: ]//for internal use only log message
[]
[could not open file %1]//error message
[]
[Could not open input file: ]//for internal use only log message
[]
[Cov(X,Y)]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[]
[Cov(X,Z)]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[]
[Cov(Y,Z)]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[]
[Covariance Matrix]//for internal use only
[]
[CR5]//TTools; Import; Export; Format name
[]
[CR5 Data File]//not used
[]
[Crandall]//Process Properties dialog(TLink spec.), page Compute Coordinates;  List box Adjustment type
[]
[Create a new job]//TT->Startup dialog->New job->window caption
[]
[Create new folder]//for internal use only|for internal use only
[]
[Create Offset Lines]//TTools->Convert road to Lines
[]
[Create Offset Points]//TTools->Convert road to points
[]
[Create Scan Surface]//Ttools->Scan Session tab->left panel->Pop-up menu item
[]
[Create shortcuts here]//Drag'n'drop menu item
[]
[Create Stereopair]//Images tab, left pane
[]
[Create Stereopair\nCreate Stereopair]//Images tab, left pane
[]
[Create temporary processing files in %s]//message
[]
[Create Turn Points]//TTools->Convert road to points
[]
[Created]//TT->Startup dialog->column name
[]
[Created %d %s object(s)]
[]
[Created by]//TT->Job Info->field name
[]
[Creates Surface from the scanned points\nCreate Surface from Scan Session]//tooltip
[]
[Creating component filter...]//TL->log message|TT->log message
[]
[Cross Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[Çapraz Kaba Hata ]
[CS to SC]//TT->Roads tab->Add Horz. Element: Spiral window->Spiral Dir list box->value
[]
[CS to ST]//TT->Roads tab->Add Horz. Element: Spiral window->Spiral Dir list box->value
[]
[Ctrl]//Shortcut Description
[]
[Ctrl Flag]//TT->Compare Point Report Options->column name
[]
[Cu&t\nCut the selection and put it on the Clipboard\nCut]//TL->Tool Bar->Edit->Cut|TT->Tool Bar->Edit->Cut
[Ke&s\nEkranda seçilen yerleri kes\nKes]
[Cu&t\tCtrl+X]//Ttools->Layers Control->Layers Combo box->Pop-up menu item|TTools and TLink->Menu Bar->Edit|TTools and TLink->Import from Device->Pop-up menu item|TTools and TLink->Cad View and Map View->Pop-up menu item|TT->Codes window->Pop-up menu item|TT->Occupation View window->Pop-up menu item on occupation|TT->Residiul View window->Pop-up menu item on Residiul|TTools and TLink->Menu Bar->Edit
[Ke&s\tCtrl+X]
[Cub.%s]//template for making abbreviated cubic unit name out of regular linear unit name
[]
[Cubic %s]//template for making cubic unit name out of regular linear unit name
[]
[Current file]//Send files dlg group caption
[]
[Curve]
[]
[Curve by 2 points]
[]
[Curve by 3 points]
[]
[Custom]//camera property name
[Özel]
[Custom Antennas List]//TTools and TLink->GPS Occupation Properties->Antenna Tab->Custom Antennas List, dialog name
[Özel Antenler Listesi]
[Custom Cameras List]//TTools and TLink->Image Properties->Camera Tab->Custom Cameras List, dialog name
[Özel Kameralar Listesi]
[Custom color]//for internal use only
[Özel renk]
[Custom Datums List]//TT and TL->Custom datum list window name
[Özel Datun Listesi]
[Custom Format not saved properly]//log message
[Özel Format uygun şekilde kayıtedilemedi]
[Custom format properties]//TTools and TLink->Export files and Convert File->Custom format properties dialog name
[Özel format özellikleri]
[Custom Projections List]//TT and TL->Custom Projections List window name
[Özel Projeksiyon Listesi]
[Custom Text Format]//TTools and TLink->Import and Export files, Convert File->format name
[Özel Text Formatı]
[Custom TS Instrument List]//TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument->window caption
[]
[custom vector format properties]//TTools and TLink->Export files and Convert File->Custom format properties dialog name  
[özel vektör format özellikleri]
[Custom..]//TTools and TLink->GPSOccupation Properties->Antenna tab->button name|button name|TT->TS Obs tab->Properties for TS Occupation->button name
[Özel..]
[Custom...]//TTools and TLink->Image Properties->Camera tab->button name
[Özel..]
[Customi&ze...\nCustomize toolbars\nCustomize]//TL->Tool Bar->View (for internal use)|TT->Tool Bar->View->Customize
[Özelleşt&ir...\nAraçÇubuğunu Özelleştir\nÖzelleştir]
[Customize]//TTools, "Customize" dialog
[]
[Customize toolbars]//TTools; Tool Bar; View; Customize; Customize toolbars window; caption
[]
[Cut]//TTools->CoGo->Compare Surfaces|TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[]
[Cut Object(s)]//TTools and TLink->Menu Bar->Edit->menu item after object cutting
[Obje(leri)Kes]
[Cut Sheet]//TTools->Export->Format name|TT and TL - tab name in Properties for staked points
[Kazı Tabakası]
[Cut Sheet Report]//TT->Report->Report Configuration->Cut Sheet Report->Options->hint text(for internal use)
[Kazı Tabakası Raporu]
[Cut Sheet Report Options]//TT->Report->Report Configuration->Cut Sheet Report->Options(for internal use)
[Kazı Tabakası Rapor Seçenekleri]
[Cut Sheet Standard]//TTools->Export->Format namem
[Kazı Tabakası Standart]
[Cut Sheet User-Defined]//TTools->Export->Format name
[Kazı Tabakası Kullanıcı Tanımlı]
[Cut Sheet User-Defined format properties]//TTools->Export->Cut Sheet  user-  defined format->dialog caption
[Kullanıcı Tanımlı Kazı Tabakası Format Özellikleri]
[Cut Slope]//TT->X-Section Templates tab->Properties->field name
[Kazı Eğimi]
[Cut(Fill)]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TT and TL - on Cut Sheet tab in properties for staked points|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[Kazı(Dolgu)]
[Cut/Fill]//TT->X-Section Templates tab->right panel->Graphic View->text under cursor
[Kazı(Dolgu)]
[CX]//camera property name
[]
[CY]//camera property name
[]
[Cycles]//TT->Residiul view window->axis name
[]
[D&isable\nDisable the selected object(s)\nDisable object(s)]//TT->Tool Bar->Edit->Disable
[]
[Dark Blue]//TTools->attribute properies->color list box->possible value
[Koyu Mavi]
[Dash]//TTools->attribute properies->Outline tab->Style list box->possible value
[Kesikli]
[Dash-Dot]//TTools->attribute properies->Outline tab->Style list box->possible value
[Kesik-Nokta]
[Data Base Object is locked]//error message under Adjustment and Compute  Coordinates
[]
[Data does not fit in element]//for internal use only log message
[]
[Date]//TTools, TLink; Tab View; DL tab; DL Occupation Properties;  field name|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools->Codes->New Attribute->possible attribuite type|TL->File properties->Session tab->field name
[Gün]
[Date created]//TT->Job Info->field name
[Gün oluşturuldu]
[Date/Time]//TTools; Codes; New Attribute; Pop-up menu command|TLink; Resect Export, Header Field name
[Gün/Zaman]
[Datum]//TTools; ->Job Configuration->Coordinate Systems ->Datum Properties dialog-> caption|TTools->Job Configuration->Coordinate Systems->List box name
[Datum]
[Datum already exists. Overwrite it?]//TTools; TLink; Datum Transformation; message box while saving parameters
[Datun zaten mevcut. Üzerine yazılsın mı?]
[Datum Lat, Lon, Elevation]//TTools (Job Configuration and list box in the Status Bar)and TLink (list box in the Status Bar)->possible value
[]
[Datum Lat, Lon, Ell.H]//TTools (Job Configuration and list box in the Status Bar)and TLink (list box in the Status Bar)->possible value
[]
[Datum Transformation]//TTools; TLink; Command name
[Datum Transformasyonu]
[Datum:]//TT and TL->in advanced import/export options, convertation and open file->list box name
[Datum:]
[Day]//TTools->Occupation view->Split GPS Occupations dialog->Split by list box->value
[]
[days]//TT->Tool Bar->Select->Select GPS Occup and GPS Obs->Duration->spin edit name
[günler]
[DBF Code Library]//TTools; Codes; Export to file; file format
[DBF Kod Kütüphanesi]
[dd mm sss]//Ttools(Job Configuration) and TLink(Configuration)->Display->Angles tab->angles list box and Lat,Lon list box->possible value
[dd mm sss]
[dd%smm'ss.s"]//Ttools(Job Configuration) and TLink(Configuration)->Display->Angles tab->angles list box and Lat,Lon list box->possible value
[dd%smm'ss.s"]
[dd.ddd]//Ttools(Job Configuration) and TLink(Configuration)->Display->Angles tab->angles list box and Lat,Lon list box->possible value
[dd.ddd]
[dd.mmsss]//Ttools(Job Configuration) and TLink(Configuration)->Display->Angles tab->angles list box and Lat,Lon list box->possible value
[dd.mmsss]
[dE]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink ->GPS Obs tab-> column name|TT and TL - on Cut Sheet tab in properties for staked points|TT->Compare Point Report Options->column name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[dD]
[Default absolute]//antenna type set name : TTools and TLink -> Job Configuration(Equipment) -> Import Antenna -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> Set combobox selectable case   
[Mutlak varsayalın]
[Default meteo param at height:]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Default relative]//antenna type set name : TTools and TLink -> Job Configuration(Equipment) -> Import Antenna -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> Set combobox - selectable case
[Göreceli varsayılan]
[Default Value]//TTools; Codes; Attribute properties; field name|TTools->Attribute properties->Default value
[Geçerli Değer]
[Deflection]//TTools->CoGo->Traverse	
[]
[Deflection East]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Sapma Doğu]
[Deflection North]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Sapma Kuzey]
[Deg Chord]//TT->Roads tab->Horz. element->Properties for Curve, Spiral, Intersection->field name
[]
[Deg Curve]//TT->Roads tab->Horz. element->Properties for Curve, Spiral, Intersection->field name
[]
[Del]//Shortcut Description
[Sil]
[Delete]//TTools; Customize toolbars window; Toolbars Page; button mame|TTools and TLink; command|TT->Job Configuration window->List configurations->Configurations list window->button name|Context menu item on history of messages dlg
[]
[Delete Button]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[Delete code]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->button name
[]
[Delete from line(s)]//TTools->Cad View->delete point from line->Pop-up menu item
[]
[Delete from Surfaces]//TTools, context menu on points and lines belonging to Surface
[]
[Delete job]//TT->Sturtup dialog->button name
[]
[Delete point from lines\nDelete from lines]//TTools->Cad View->delete point from line->hint text
[]
[Delete report]//TT->Report Configuration->button name
[]
[Delete selected object from Surfaces\nDelete from Surfaces]//TTools,tooltip
[]
[Delev]//TTools; Inverse;
[]
[Delimiters]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box name|TTools and TLink->Export files and Convert File->Custom format properties->list box name
[]
[Delta]//TT->Roads tab->Horz. element->Curve->Properties->General page->field name
[]
[Delta East]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Delta Elevation]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Delta Ell.H]//TTools; Inverse window; bottom pane and Properties window
[]
[Delta H]//TTools; Inverse window; bottom pane and Properties window
[]
[Delta North]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Demo Mode]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->button name
[]
[Demo mode points]//message box
[]
[Demo mode roads]//not used
[]
[Description]//not used|not used|TTools->File->Remote users->add group->prop. name
[]
[Description:]//Send files dlg group caption
[]
[Design]
[Dizayn]
[Design East]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Design Elevation]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Design files]//TTools->Export->Format name|TTools->Export->Format name
[]
[Design North]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Design Point]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|???for internal use only
[]
[Design points filter\nDesign points filter]//for internal use only
[]
[Destination]//TLink->Convert File->Right Panel->list box name
[Hedef]
[Destination type]//not used
[Hedef tipi]
[Destination:]//TLink->Convert File dialog->list box name
[Hedef:]
[Detail]//TTools; Adjustment; Column name
[]
[Details]//not used
[]
[Detection type]//TTools->thumbnail/stereopair view options->Image Measurements tab->Combo box name                
[]
[Dev Az(&quot;)]//TT->Repeated Observations Report list->column name
[]
[Dev E]//TTools; Adjustment; Column name|TT->Repeated Observations Report list->column name
[]
[Dev H]//TTools; Adjustment; Column name
[]
[Dev HA(&quot;)]//TTools; Adjustment; Column name|TT->Repeated Observations Report list->column name
[]
[Dev N]//TTools; Adjustment; Column name|TT->Repeated Observations Report list->column name
[]
[Dev SD]//TTools; Adjustment; Column name|TT->Repeated Observations Report list->column name     
[]
[Dev U]//TT->Repeated Observations Report list->column name
[]
[Dev VA(&quot;)]//TTools; Adjustment; Column name|TT->Repeated Observations Report list->column name
[]
[Device]//TTools and TLink->Export from Device and Import toDevice->panel name
[Cihaz]
[Device properties:]//not used
[]
[Devices]//TTools and TLink->Import from Device
[Cihazlar]
[Devices:]//for internal use only
[]
[DGN/ISFF]//TTools->Export->Format name
[]
[DGPS]//TTools and TLink->GPS Obs Properties ->Method, possible value
[DGPS]
[DGPS Go]//TTools and TLink->GPS Obs Properties ->Method, possible value|Solution Name
[DGPS Go]
[DGPS Kin]//TTools and TLink->GPS Obs Properties ->Method, possible value
[DGPS Kin]
[DGPS Kinematic]//TTools->Map View->Legend window->point type|Solution Name
[]
[DGPS Kinematic Horizontal Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name(when PP module is disabled)
[]
[DGPS Kinematic Precisions]//TT->Job Configuration->Quality Control->Automatic Tests tab->check box name(when PP module is disabled)
[]
[DGPS Kinematic Vertical Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name(when PP module is disabled)
[]
[DGPS Non-processed Kinematic]//TTools->MapView->legend window
[]
[DGPS Non-processed Static]//TTools->MapView->legend window
[]
[DGPS Non-processed Stop]//TTools->MapView->legend window
[]
[DGPS PostProcessing]//????hint text in the Status Bar
[]
[DGPS Static]//TTools->Map View->Legend window->point type|Solution Name
[]
[DGPS Static Horizontal Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name(when PP module is disabled)
[]
[DGPS Static Precisions]//TT->Job Configuration->Quality Control->Automatic Tests tab->check box name(when PP module is disabled)
[]
[DGPS Static Vertical Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name(when PP module is disabled)
[]
[DGPS Stop]//TTools and TLink->GPS Obs Properties ->Method, possible value|TTools->Map View->Legend window->point type|Solution Name
[DGPS Stop]
[dH]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TT->Compare Point Report Options->column name
[dH]
[dHt]//TTools and TLink ->GPS Obs tab-> column name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[dYk]
[dHz]//TLink; Resect Export, Header Field name|TT->Loop Closure Report->Column name
[dYty]
[dHz (ppm)]//TT->Loop Closures Report->column name
[]
[dHz relative]//TT->Loop Closures Report->column name
[]
[Digital Level]//not used
[]
[Digital Level filter\nDigital Level filter]//not used
[]
[Digital Level observations]//not used
[]
[Digits after decimal]//for internal use only
[Ondalık sayı hanesi]
[Dimensions: %s %s x %s %s]//TTools->Map View  and Cad View->trxt in the Status Bar during selecting the area
[]
[Dim-Type]//TLink; Resect Export, Header Field name
[Byt-Tipi]
[Direct3D cannot work with this videocard settings!]//TT->3D View->error message
[]
[Direction]//TTools->CoGo; Intersect|not used|Message prop. name
[]
[Direction is not found]//TTools; CoGo; Point In Direction, error message
[]
[Directory:]//Receive file dlg
[Dizin:]
[Disable]//TTools and TLink->Tab View->Points Tab->Pop-up menu item and Menu Bar->Edit->menu item|TT->Occupation View window->Pop-up menu item|TT->Residiul view window->pop-up menu
[Aktif değil]
[Disable objects\nDisable objects]//TTools and TLink->text in the Status Bar
[Objeleri kaldır\nObjeleri kaldır]
[Disabled]//TTools; DL Obs Properties dialog; Adjustment Page; field Adjustment Status; field text|TTools and TLink->GPS Obs Properties->Adjust Page->field Adjustment Status->possible value|//TTools->Map View->Legend window->line type|TT->Tool Bar->Select->Select Points, GPS Obs, TS Obs->Enabled for adjustment list box->value|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->Adjustment Status list box->value
[]
[Disabled from Adjustment]//Name Of Vector Type
[]
[Disabled points filter\nDisabled points filter]//for internal use only
[]
[Disabled svs/epochs]//TTools->Export(Advanced options for Rinex files)->check box name
[]
[Disabled TS filter\nDisabled TS filter]//TT->View->Filters->By Type
[]
[Display]//tab name in options dialog in Surface tab|TTools->CoGo; Options                   |TTools->Linework->Options->page name|TTools and TLink -> Tabular View ->GPS Occupations tab->Options->Tab name|for internal use|TTools(Job Configuration) and TLink(Configuration)->node name; TTools and TLink_>Tab View->Point tab->options->tab name|not used|TT->Roads view options dialog name (for internal use)|TSObs tab(TT and TL) and Tape Dimensions tab (TT)->Options->tab name
[Ekran]
[Display CL Pos as]//TT->Job Configuration->Display->Roads tab->list box name
[Aks Ekran Görünümü]
[Display Cross Sections]//TT->Roads tab->Options->tab name
[]
[Display Horizontal Elements]//TT->Roads tab->Options->tab name
[]
[Display Loop Closures for selected GPS Obs\nLoop Closures]//TT->tool tip
[]
[Display Mode]//TT->Occupation View Options window->Occupation View Options tab->group box name
[]
[Display roads]//not used
[]
[Display String and Control Code]//TT(Job Configuration) and TL(Configuration)->Display ->Strings tab->Check box name
[]
[Display Vertical Elements]//TT->Roads tab->Options->tab name
[]
[Display\\Angles]//TTools->Job Configuration and TLink->Configuration
[Ekran\\Açılar]
[Display\\Compare Surfaces]//TTools->CoGo; DTM compare, key word
[]
[Display\\Digits after decimal]//TTools(Job Configuration) and TLink(Configuration)->Display->Precisions tab ->group box name
[Ekran\\Ondalık hane sayısı]
[Display\\DL Obs]//TTools, TLink; DL Obs Tab; Options dialog; Page name
[Ekran\\DL Okuml.]
[Display\\DynaUser]
[]
[Display\\GPS Obs]//for internal use only
[Ekran\\GPS Gözlemleri]
[Display\\GPS Occupations]//for internal use only
[Ekran\\GPS Oturumları]
[Display\\Horizontal Road Elements]//TT->Roads tab->Options(for internal use)
[Ekran\\Yatay Yol Geometrisi]
[Display\\Image Measurements]//orientation points
[]
[Display\\Images]//for internal use
[Ekran\\Resimler]
[Display\\Intersection]//TTools->CoGo;Intersection, keyword
[]
[Display\\Inverse]
[]
[Display\\Inverse Point to Line]//TTools->CoGo;Inv PTL, key word
[]
[Display\\Lines]//TTools; Linework Tab; Options dialog
[Ekran\\Hatlar]
[Display\\Linework]//TT->Tabular View Optioms window
[]
[Display\\Point In Direction]//TTools->CoGo; Options
[]
[Display\\Points]//for internal use only
[Ekran\\Noktalar]
[Display\\Precisions]//TTools->Job Configuration and TLink->Configuration
[Ekran\\Hassasiyetler]
[Display\\Road Graphic Views]//TT->Roads tab(for internal use)
[Ekran\\Yol Grafik Görünümleri]
[Display\\Road X-Sections]//TT->Roads tab->Options(for internal use)
[Ekran\\Yol EnKesitleri]
[Display\\Roads]//TT->Job Configuration->Display->Roads tab
[Ekran\\Yollar]
[Display\\Scan Sessions]//TTools->Scan Sessions tab->Scan Session View options dialog->page name
[]
[Display\\Stereopairs]//for internal use
[Ekran\\StereoÇifti]
[Display\\Strings]//TTools (Job Configuration) and TLink (Configuration)
[Ekran\\Hatlar]
[Display\\Surfaces]//name in list and name of tab in Tabular View Options
[]
[Display\\Tape Obs]//TT and TL->Tabular View Options->Tape Obs
[Ekran\\Şerit Ölçs.]
[Display\\Time]//TTools->Job Configuration and TLink->Configuration    
[Ekran\\Zaman]
[Display\\TS Obs]//TT and TL->Tabular View Options->TS Obs
[Ekran\\TS Oturm]
[Display\\Vertical Road Elements]//TT->Roads tab->Options(for internal use)
[Ekran\\Düşey Yol Geometrisi]
[Display\\X-Section Templates]//TT->X-Section Templates tab
[Ekran\\En Kesit Şablonları]
[Dist]//TTools->CoGo; Intersect + PointInDirection
[]
[Dist is Ground]//TTools->CoGo;PointInDirection
[]
[Dist1 is Ground]//TTools->CoGo;IntersectPoint
[]
[Dist2 is Ground]//TTools->CoGo;IntersectPoint
[]
[Distance]//TTools spec.; diagnostics about errors under Adjustment when bad connected network|TTools; Inverse window; bottom pane|TTools, TLink; Tab View; DL tab; field name|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink ->GPS Obs tab-> column name|Resolve Duplicate Points dialog, column name|TT->Identical Points Report->column name|TT->Tabular View->Tape Dimensions tab->column name
[Mesafe]
[Distance 1]//TTools; CoGo; Intersection
[]
[Distance 2]//TTools; CoGo; Intersection
[]
[Distance between one or more adjacent points is less than doubled deviation: \neither reduce deviation value or remove abundant point from selection.]//(select two or more points on MapView window)->(click right button of mouse)->dialog->set required parameters->OK->message box with this text may appear
[]
[Distance from prev]
[Önceki Nok.dan Mesafe]
[Distance from start]
[Başlangıç Nok.dan Mesafe]
[Distance is]//TL->Convert File->Advanced options->right panel->group box name
[Mesafe]
[Distance mode:]//TT ->in advanced import/export options->Distance mode list box name (for example export TS Obs->FC5 Raw)
[]
[Distance residual (m.)]//TT->Misnamed Autotopo Rovers Report->column name
[]
[Distance: %s %s]//TTools->Map View  and Cad View->trxt in the Status Bar during selecting the area
[]
[Distances]//TTools->Job Configuration->Display->Precisions
[Mesafeler]
[Distortion, K]//camera property name
[]
[Distortion, P]//camera property name
[]
[Divide by 0]
[]
[Divide by zero]//TTools;  error message under Adjustment
[]
[DL BlueBook]//TLink; BlueBook Export Options, Report name
[DL BlueBook]
[DL Data File]//not used
[]
[DL export filter]//TTools; Export; message
[]
[DL from point %s%s to point %s%s]
[]
[DL import filter]//TTools; Import; message
[]
[DL Measurements]//????TTools->Map View->Legend window->point type
[]
[DL Obs]//TLink; File; File Properties dialog; caption
[]
[DL Obs List\nDL Obs List]//hint text; for internal use only
[DL Okum.List\nDL Okum.List]
[DL Obs Report]//for internal use only
[DL Okum.Raporu]
[DL Obs Report Options]//for internal use only
[DL Okum.Rapor Seçnklri]
[DL Precisions]//for internal use only
[DL Hassasiyeti]
[DL Run]//TTools, TLink; Tab View; DL tab; DL Occupation Properties dialog name;
[DL Run]
[DL Runs]//TTools, TLink; Tab View; DL tab; DL Occupation window name (for Print Priview);
[DL Runs]
[DL Sideshot]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[DL Sideshots filter\nDL Sideshots filter]//not used
[]
[DL Traverse]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[DL Traverse Points filter\nDL Traverse Points filter]//not used
[]
[DL Vertical Precision]//TT->Job Configuration->Quality Control->DL Obs Precisions tab->field name
[]
[DL-Export]
[]
[DLExport to ]//TTools; Export; message
[]
[DLL not found]//error message
[]
[DMS]//TLink; Resect Export, Angular Unit Name|TTools->Job Configuration->Units->Angular Unit list box->possible value; TTools and TLink->Status Bar->list box for angular units
[DMS]
[dN]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink ->GPS Obs tab-> column name|TT and TL - on Cut Sheet tab in properties for staked points|TT->Compare Point Report Options->column name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[dX]
[dN, dE, dHt]//for internal use only
[dX, dY, dZ]
[Do not Backup]//TTools->Job Configuration->Save->Backup files from devices->possible value
[]
[Do not show this dialog window again]//TTools; Background images;
[]
[Do not use]//TT->Tool Bar->Select->Select Points, GPS Obs, TS Obs and etc.->Std Dev Horizontal and Std Dev Vertical list boxes->value
[]
[Do not use the image]//TTools; Background images dialog;
[]
[Dongle]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->Key value->value
[]
[Dot]//TTools->attribute properies->Outline tab->Style list box->possible value
[]
[Double Sterographic]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[İkili Sterografik]
[Download file from TPS controller\nDownload file from TPS controller]
[]
[Download TopSURV job from device]//TT and TL->Import from Device->Progress bar text
[Cihazdan TopSURV iş dosyasını indir]
[Download\\TSV]
[]
[Downweighted Blunder Equations: ]//TTools;  error message under Adjustment
[]
[Drop element(s)]//Undo action name
[]
[Drop options]//TTools;Tlink; Drop options dialog; caption
[Bırakma seçenekleri]
[Dry temperature: (°C)]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[dS]//TLink; Resect Export, Header Field name
[dS]
[dU]//TT->Loop Closure Report->Column name
[]
[dU (ppm)]//TT->Loop Closures Report->column name
[]
[dU relative]//TT->Loop Closures Report->column name
[]
[Duration]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools->Occupation view->Split GPS Occupations dialog->field name|TT->Tool Bar->Select->Select GPS Obs.->list box name
[Süre]
[Duration of constant zenith path delay (h)]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[dV]//TLink; Resect Export, Header Field name
[dV]
[DWG]//TTools -> Import; Export; and Tlink-> Convert; Format name
[DWG]
[DWG Background Image File]//for internal use only
[DWG Arkaplan Resim Dosyası]
[DWG Data File]//not used
[]
[DWG DTM files]//for internal use only
[DWG DTM dosyası]
[DWG files]//TT->Map View options->Browse->Open dialog->Format name
[]
[DX]//TTools; TLink; Datum Transformation dialog; Datum parameter name|TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name
[DX]
[dX]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel|TTools and TLink -> Tabular View ->GPS Obs Tab ->Column name
[dX]
[dX, dY, dZ]//for internal use only
[dX, dY, dZ]
[DXF]//TTools -> Import; Export; and Tlink-> Convert; Format name
[DXF]
[DXF and DWG files]//for internal use only.
[DXF ve DWG dosyaları]
[DXF Background Image File]//for internal use only
[DXF Arkaplan Resim Dosyası]
[DXF Data File]//not used
[]
[DXF DTM Data File]//for internal use only
[DXF DTM Data Dosyası]
[DXF DTM files]//for internal use only
[]
[DXF files]//TT->Map View options->Browse->Open dialog->Format name
[]
[DY]//TTools; TLink; Datum Transformation dialog; Datum parameter name|TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name
[DY]
[dY]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel|TTools and TLink -> Tabular View ->GPS Obs Tab ->Column name
[dY]
[Dyna Users]
[]
[DynaSurv]//name of module, in Autorizations dialog and in About
[]
[DynaUser]//TTools and TLink -> Menu Bar->View->Tabular View Options->Tab name
[DynaUser]
[DynaUser List\nDynaUser List]//for internal use
[DynaUser List\nDynaUser List]
[DZ]//TTools; TLink; Datum Transformation dialog; Datum parameter name|TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name
[DZ]
[dZ]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel|TTools and TLink -> Tabular View ->GPS Obs Tab ->Column name
[dZ]
[dZA]//TLink; Resect Export, Header Field name
[dZA]
[E]//TTools; CoGo; Intersection|TTools and TLink->Tabular View, Longituide, part of BLH coordinate value (insted of +)|TTools and TLink->Tabular View, Latituide, part of coordinate value (insted of -)|TTools; part of coordinate value on axis|TTools; part of coordinate value on axis|TTools and TLink->Tabular View, Longituide, part of  coordinate value (insted of +)|not used
[D]
[E Residual]//TTools; TLink; Localization; Properties; field name
[D Farkı]
[E&xit]
[Ç&ıkış]
[E&xit\nQuit the application; prompts to save documents\nExit]//TL->Tool Bar->File->Exit|TT->Tool Bar->Job->Exit
[Ç&ıkış\nHazır belgeleri kaydedip uygulamadan çık\nÇıkış]
[East]//TLink; Resect Export, Header Field name|TT->3D View->left-bottom part of the window->axis name
[Doğu]
[East0]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Doğu0]
[Easting]//TTools and TLink->Export files and Convert File->Custom format properties->for Grid and Ground systems field in the left panel|TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name|not used|TTools->Map View and Cad View->axis name in Ground and Grid system|TT->Roads tab->Road properties->field name and Horz. Element properties->field name and Graphic View->axis name
[Sağa]
[Easting Offset]//TTools; TLink ->Job Configuration->Coordinate Systems; Grid to Ground window -> field name; or Convert file dialog -> Grid to Ground
[Sağa Ofset]
[Easting,Northing,Height]//TLink->Open TS Raw Data Files and TTools Import->list box Coordinate order->possible value
[Sağa, Yukarı, Yükselik]
[Eb]//units of files size - send file dialog
[]
[Edge Extracted]//TT and TL->Properties for TS Obs->Offset tab->Offset type->value
[Resim Ofseti]
[Edit]
[]
[Edit configuration]//TT->Creare a new job->button name
[]
[Edit Function]
[]
[Edit Parameters]
[]
[Edit Plot]
[]
[EDM]//Process properties dialog (TLink spec.); Compute Coordinates page; field EDM; caption |TT->Custom TS Instrument list->column name
[EDM]
[EDM, (mm)]//Process properties dialog (TLink spec.); Compute Coordinates page; field EDM (mm) accuracy factor
[EDM, (mm)]
[EDM, (ppm)]//Process properties dialog (TLink spec.); Compute Coordinates page; field EDM (ppm) accuracy factor
[EDM, (ppm)]
[EGM Coeff Correction File]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name for certain type of Canadian Geoids (in additional open dialog)
[EGM Coeff Düzeltme Dosyası]
[Element with ID='%s' not found]//for internal use only log message
[Elementi ID='%s' bulunamadı]
[Elementary]
[]
[Elev]//TT->3D View->left-bottom part of the window->axis name
[]
[Elevation]//TTools spec.; diagnostics about errors under Adjustment when bad connected network|TTools; CoGo; Intersection|TTools, TLink; DL Obs Properties dialog; Adjustment Page, field name|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name|TT->Roads tab->Road properties->field name and Vert. Element properties->field name and Vert. element->Graphic View->axis name
[Yükseklik]
[Elevation (Datum)]//TT->Point summary Report Options->column name
[Yükseklik (Datum)]
[Elevation Angle]//TTools and TLink ->GPS Obs tab-> column name
[Yükseklik Açısı]
[Elevation Mask]//TT->Process properties->GPS+Post Process tab->spin edit control name
[]
[Ell.Height]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[Elp.Yüsk.]
[Ell.height\Elevation]//TT->Compare Point Report Options->column name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item|TT->Point summary Report Options->column name
[]
[Ell.Ht\\Elevation]//TTools and TLink->Tab View->Point tab->Options->column name
[Elp.Yk.\\Yükseklik]
[Ellipsoid]//Ttools; ->Job Configuration->Coordinate Systems -> Custom Datum List-> column name or Properies dialog for datum
[]
[Ellipsoid:]//TTools; TLink; Datum Transformation dialog; Datum parameter name
[Elipsoid:]
[Empty password]//Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message|Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message
[]
[Empty report file name]//message box
[]
[Enable]//TTools and TLink->Tab View->Points Tab->Pop-up menu item and Menu Bar->Edit->menu item|TT->Occupation View window->Pop-up menu item|TT->Residiul view window->pop-up menu|Internal use
[Aktif]
[Enable continuous kinematic]//TT->Process properties->GPS+Post Process tab-> Check box name
[]
[Enable objects\nEnable objects]//TTools and TLink->text in the Status Bar
[Aktif objeler\nAktif objeler]
[Enabled]//TTools, TLink; Tab View; DL tab; DL Occupation Properties; Check box enabled|TTools and TLink -> Tabular View -> GPS obs tab -> GPS Obs Properties - Check box name and GPS Occupations tab -> GPS Occupations Properties - Check box name|not used|TT->Tool Bar->Select->Select TS Obs->list box name|TT->TSObs properties->Check box name
[Aktif]
[Enabled for adjustment]//TT->Tool Bar->Select->Select Points->list box name
[]
[Enabled for Adjustment]//TTools and TLink->Tab View->Point Properties->General tab->check box name
[Dengeleme içi Aktif]
[Enabled modules:]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->text
[]
[End 1]//TTools; CoGo; Intersection
[]
[End 2]//TTools; CoGo; Intersection
[]
[End Azimuth]//TT->Roads tab->Horz. element->Properties->End Position tab->field name
[Bitiş Azimutu]
[End Deg Chord]//TT->Roads tab->Horz. element->Properties for Spiral->field name
[]
[End Deg Curve]//TT->Roads tab->Horz. element->Properties for Spiral->field name
[]
[End Easting]//TT->Roads tab->Horz. element->Properties->End Position tab->field name
[Bitiş Y'si]
[End Grade]//TT->Roads tab->Vert. element->right panel->column name
[Eğim Sonu]
[End Line]//TT and TL->Point Properties->Control code
[Hat Sonu]
[End Northing]//TT->Roads tab->Horz. element->Properties->End Position tab->field name
[Bitiş X 'i]
[End Point]//for internal use only
[Bitiş Noktası]
[End Position]//TT->Roads tab->Horz. element->Properties->End Position tab name
[]
[End Radius]//TT->Roads tab->Horz. element->right panel->column name
[Bitiş Yarıçapı]
[End Sta/Chainage]//TT->Roads tab->Horz. element->Properties->End Position tab->field name
[Bitiş İstasyon/KM]
[End Time]//TTools->Occupation view->Split GPS Occupations dialog->field name
[Bitiş Zamanı]
[End time]//TT->Tool Bar->Select->Select GPS Occup.->list box name
[Bitiş zamanı]
[End Time Nanoseconds]//not used
[]
[End Time Seconds]//not used
[]
[EndPoint]//TTools; CoGo; Intersection
[]
[Endpoint has not coordinates]//diagnostic message during Adjustment and Compute coordinate
[]
[Engine Mode:]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Engine(s) is running: %s. Stop it and close job?]//TT->Close job->message
[]
[ENH]//TT and TL->in advanced import/export options, convertation and open file_>Coordiane order(for example SHP files)
[YXZ]
[Enlarge the window to full size]//Command Maxiniz for Window; text in the Status Bar
[]
[Enter]//Shortcut Description
[]
[Enter Access Code]//TT->Tool Bar->Help->Access Codes->dialog caption
[]
[Enter configuration name]//TT->Job Configuration->Save Configuration->Enter configuration name window caption
[]
[Entered password is incorrect]//Ttools->Map View->Options>MrSid Background file activation->Password window->message|Ttools->Map View->Options>MrSid Background file activation->Password window->message
[]
[Entry azimuth]
[Başlangıç Azimutu]
[Epochs]//TTools and TLink->GPS Obs Tab->Properties->field name
[Epoklar]
[Epochs Count]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[Epok Sayacı]
[Equal to]//TT->Tool Bar->Select->Select GPS Occup.->Antenna height list box->value and Select TS Occup.->Instrument height list box->value
[]
[Equations (Used/Rejected)]//TTools; Adjustment; Column name
[]
[Equipment]
[]
[Error]//not used
[]
[Error # %lx]//error message
[]
[Error Converting File]//TT and TL->Export to Device,Import from Device ->error message
[Dönüştürülen Dosyada Hata]
[Error in graphic building]
[]
[Error in parameter: ]//TTools; CoGo; error message
[]
[Error on line %d, position %d in '%S'.]//for internal use only log message
[]
[Error reading database]//TT and TL->Export to Device,Import from Device ->error message
[VeriTabanı okuma hatası]
[Error writing database]//TT and TL->Export to Device,Import from Device ->error message
[VeriTabanı yazma hatası]
[Errors]//TTools;TLink;log error message
[Hatalar]
[Esc]//Shortcut Description
[Çkş]
[Event]//for internal use|TTools->MapView->legend window|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Event points filter\nEvent points filter]//for internal use only
[]
[Events]//for internal use
[]
[Events List]//for internal use
[]
[Events List\nEvents List]//for internal use
[]
[Exchange XML]//Internal use
[]
[Exclamation (!)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[Exclusion]//TT and TL->Layers window->Breakline type column ->value
[Çıkart]
[Execute]//TT->Report Configuration->button name
[]
[Execute report ]//TT->Tool Bar->Report->hint text in the Status Bar
[]
[Existing]//TTools->CoGo->Compare Surfaces; Second Surface
[]
[Existing functions]
[]
[Exit azimuth]
[Bitiş Azimutu]
[Export]//TTools; Export; message|log message|log message|not used|log message|TTools and TLink; message|TTools->log message and Import dialog caption
[]
[Export &to Device...]//TLink ->Menu Bar->File(TLink) and Job(TTools)->menu item
[Cihaza& Aktar...]
[Export data to device\nExport to device]//TTool sand Tlink->Export to Device->text in the Status Bar
[Cihaza data aktar\nCihaza aktar]
[Export DL to XD\nExport DL to XD]
[]
[Export DXF and DWG Files]//for internal use only.
[DXF ve DWG Dosyalarını Aktar]
[Export DXF and DWG Files\nExport DXF and DWG Files]//for internal use only.
[]
[Export File Options]//for internal use only
[Dosya Aktarma Seçenekleri]
[Export files to external device\nExport to Device]//TLink->Export->text in the Status Bar
[]
[Export filters]//not used
[]
[Export is not supported for this device]//TLink->Export to Device->message
[Bu cihaz için aktarım desteklenmiyor]
[Export named vertices as points]//not used
[]
[Export Points to XD\nExport Points to XD]
[]
[Export points without code]//not used
[]
[Export to Coordinates Files]//for internal use only
[Koordinat Dosyasını Aktar]
[Export to D&evice...]//TTools and TLink->Menu Bar->File(TLink) and Job(TTools)->menu item
[Cihaza Akt&ar]
[Export to Device]//TLink->Export to Device dialog caption
[]
[Export to Device Options]//for internal use only
[Cihaza Aktarma Seçenekleri]
[Export to Device...]//TLink ->Menu Bar->File(TLink) and Job(TTools)->menu item
[Cihaza AKTAR...]
[Export to Device\nExport to Device]//TLink->Export->text in the Status Bar
[Cihaza Aktar\nCihaza Aktar]
[Export to DGN/ISFF format]//for internal use only
[DGN/ISFF formatı aktar]
[Export to DL Files]//TTools; Export; for internal use only
[]
[Export to DWG Files]
[]
[Export to DXF DTM Files]//for internal use only
[DXF DTM Dosyaları Aktar]
[Export to file\nExport to file]//TTools->Export->text in the Status Bar
[]
[Export to GFF Files]//TLink; for internal use only
[GFF Dosyaları Aktar]
[Export to LN3 format]//for internal use only
[]
[Export to RINEX files]//Export RINEX, Progress bar text
[]
[Export to Road Files]//for internal use only
[Yol Dosyaları Aktar]
[Export to Shape Files]//for internal use
[Shape Dosyaları Aktar]
[Export to Sheet files]//for internal use only
[Tabaka Dosyaları Aktar]
[Export to TDS Files]//not used
[]
[Export to TN3 Files]//TT->Export(for internal use)
[]
[Export to Topcon Japan file\nExport to Topcon Japan file]//for internal use only
[]
[Export to Topcon Japan Files]//for internal use only
[]
[Export to Topcon Tools Job\nExport to Topcon Tools Job]//for internal use
[]
[Export to TopSURV Database Files]
[]
[Export to TPD file]//Progress bar text
[]
[Export to XML Files]
[]
[Export Topcon Tools Job]//for internal use
[]
[Export TS to XD\nExport TS to XD]
[]
[Export Vectors to XD\nExport Vectors to XD]
[]
[Export World Files]//for internal use only.
[]
[Export World Files\nExport World Files]//for internal use only.
[]
[Exporting %d occupations...]//log message
[]
[Extend slopes to the surface]//TTools->CoGo; Road2DTM
[]
[External]//TT->Roads tab->Horz. element->Properties for Curve->field name
[Dışa]
[Failed]//TTools->Map View->Legend window->line type|not used
[]
[Failed PP Kinematic]//TTools->Map View->Legend window->line type
[]
[Failed to export file %s : %s]//not used
[]
[Failed to get Civil3D]//message box
[]
[Failed to import file %s : %s]//not used
[]
[Failed to match the desired precision]//TT->QC message
[]
[Failed to process]//error message during Process
[]
[Failed to register control message.\nNo communication with engines will be possible.\nYou will have to figure out when processing is finished.]//message box
[]
[Failure of epoch!]//log message
[]
[False East]//not used
[]
[False North]//not used
[]
[Fan[%d]: BasePoint[%s]: x=%.3f y=%.3f z=%.3f]//log message
[]
[Fan[%s:%d] BasePoint [%s:%d]: %d points]//log message
[]
[FC-4 Points]//TTools->Export->Format name
[FC-4 Noktaları]
[FC-5 Points]//TTools->Export->Format name
[FC-5 Noktaları]
[FC-5 Raw]//TTools->Export->Format name
[FC-5 Ham]
[Feature Code]//not used
[]
[Feature Code Library]//not used
[]
[Feature Filter Options]//for internal use only
[]
[Field cannot be saved]//error message
[]
[Field Orientation Data]//not used
[]
[Field Scan Data]//not used|not used
[]
[Fields list is empty]//TTools->Export->Cut Sheet  user-defined format->Export|message box
[]
[File]//Ttools->Map View->Options->MrSid Background file activation->Pasword window->text|not used|TTools and TLink; Import from device|Ttools->Map View->Options->MrSid Background file activation->Pasword window->text
[]
[File %1 is corrupted and cannot be read]//error message
[]
[File %1 is read-only]//error message
[]
[File %1 not found]//error message
[Dosya %1 bulunamadı]
[File %s already exists. Overwrite?]//messaage box|messaage box|TTools (Import from device) and TLink (Import from device and Export to Device)->message box
[]
[File %s is already in job]//Ttools->view->Background images->Message
[]
[File %s is already in list]//Ttools->view->Background images->Message
[]
[File Converted Successfully]//TLink->Convert File-> log message
[Dosya Dönüştürme Başarılı]
[File decoding error]//Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message|Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message
[]
[File decoding error (exception in LizardTech library)]//Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message|Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message
[]
[File exists. Overwrite?]//TT and TL->Export to Device,Import from Device ->message box
[Dosya mevcut. Üzerine yazılsın mı?]
[File extension]//TTools and TLink->Export files and Convert File->Custom format properties->field name
[]
[File format]//TLink->Convert File->list box name
[Dosya formatı]
[File Name]//TTools and TLink->Object name (File Properties dialog)
[Dosya Adı]
[File name]//Ttools->view->Background images->left panel (Available images)->field name
[]
[File name:]//TTools and TLink -> Open File dialog and etc.->field name
[Dosya Adı:]
[File not parsed completely. Parsed only %ld bytes of %ld]//for internal use only log message
[]
[File Recognition]//log message
[]
[File type]//not used
[]
[File:]//Send files dlg static
[]
[File: %s is not %s]//log message
[]
[File: %s successful export as %s]//log message
[]
[File: %s successful parsed as %s]//log message
[]
[Files]//for internal use only|for internal use only
[]
[Files List\nFiles List]//for internal use only
[]
[Files to import]//not used
[]
[Files:]//Send files dlg static
[]
[Fill]//TTools->CoGo->Compare Surfaces|TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[]
[Fill Area]//for internal use(feature)
[]
[Fill mode]//TT->3D View->click on the 3D View window->Pop-up menu item Fill mode
[]
[Fill Slope]//TT->X-Section Templates tab->Properties->field name
[Dolgu Eğimi]
[Filter]//for internal use only|Filter
[Filitre]
[Filter by Station or Surface]//TTools->Images tab->Options->Show tab->cCeck box nane
[]
[Filter displayed objects by time\nTime filter]//for internal use only
[]
[Filtering data]//message
[]
[Filters]//TTools; Filters dialog; caption
[]
[Find]//Button caption
[]
[Finish]//TTools; Adjustment; Button name|button name|TT->Tool Bar->Process-> Loop Clousures->Loop Clousures window->button name
[]
[First surface does not have unique HORZ projection]//TTools; CoGo; Compare surfaces, error message
[]
[Fix coordinates from header]//Advanced option name for import/export
[Başlıktan Fix koordinatlar]
[Fix Endpoint Coordinates]//Process Properties dialog(TLink spec.), page Compute Coordinates; 
[]
[fix/calculated]//TLink; Resect Export, Subfield name
[fix/hesaplandı]
[Fixed]//TTools; Adjustment; diagnistic message|TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Fixed]
[Fixed Time]//TT->Process properties->GPS+Post Process tab->Minimum duration group box->possible vaue
[Fixed Zamanı]
[Float]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Float]
[Float solution]//TT->TabView->Quality Control tab->message
[]
[Floating domain error]//TTools;  error message under Adjustment
[]
[Focal Length]//camera property name
[]
[Focus point]//TTools, properties for Surface
[]
[Focus point in Surface %s is excluded from triangulation points]//TTools, message box
[]
[Folder]
[]
[Folder %s does not exist, create?]//message box in Convert dialog|TT->New Job->message
[]
[Folder For Backup]//TTools->Job Configuration->field name
[]
[Folder name:]//TTools and TLink -> Open File dialog and etc.->field name
[Klasör ismi:]
[following points...]//TTools; Adjustment; diagnostic message
[]
[For Imported Files]//???
[]
[Format]//TTools and TLink; Import from device
[Format]
[Format %s not found in list of formats]//log message
[Format%s fot-rmatlar listesinde bulunamadı]
[Format extension must be in form *.???]//message box
[]
[Format name]//TTools and TLink->Export files and Convert File->Custom format properties->field name
[Format ismi:]
[Format name:]//TTools and TLink -> Open File dialog and etc.->field name|not used
[Format ismi:]
[Format name: ]//TTools;Tlink; Drop options dialog; field name
[Format ismi:]
[Format name: %s can not be used, because the format with the same prefix already exists. Please enter different format name.]
[]
[Format not supported]//error message
[Desteklenmeyen format]
[Format of file %1 was not recognized]//error message
[]
[Format or Format Group %1 not found]//error message
[]
[FormatParser: Type of element mismatch]//for internal use only log message
[]
[FormatParser: Unexpected end of file]//for internal use only log message
[]
[FormatParser: Unexpected end of line]//for internal use only log message
[]
[Formula]
[]
[Forward]//Context menu item on history of messages dlg
[]
[Forward Azimuth]//TTools; Inverse window; bottom pane and Properties window
[]
[Forward session]//Msg session dialog->caption of tab for forwarding
[]
[Free %dD Adjustment]//TTools;  error message under Adjustment
[]
[Free NDF]//TTools;  objects description for Adjustment
[]
[Free UWE]//TTools;   objects description for Adjustment
[]
[From]//TTools->CoGo;Inv PTL|TTools, TLink; Tab View; DL tab; field name|TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Compute Azimuth->list box name|TLink->Convert File dialog->right group box caption|TT->Tab View->Linework tab->Column name|Message prop. name
[dan]
[From 1]//TTools; CoGo; Intersection
[]
[From 2]//TTools; CoGo; Intersection
[]
[From Observation Line]//TT and TL->Properties for TS Obs->Offset tab->Offset type->value
[]
[From point]//TT->Tool Bar->Select->Select TS Obs->field name
[]
[From Point]//TTools->CoGo->Traverse|TT->Point tab->Properties for Point->Offset tab->list box name
[]
[From:]//TTools; Inverse window; left-upper pane name
[]
[FS]//TTools, TLink;  DL Obs Properties dialog; General Page, Type, field content|TT and TL->Properties for TS Obs->General tab->Type list box->value
[BN]
[Full name]//TTools->File->Remote users->add user->prop. name
[]
[Full Name of Submitting Organization]//TLink; BlueBook Export Options, Organization input field name
[]
[FullCodes]//TTools and TLink->Export files and Convert File->Custom format properties->field in the left panel
[TümKodlar]
[FullCodes include Code and Attribute]//TTools and TLink->Export files and Convert File->Custom format properties->check box
[]
[FullCodes include Code, String and ControlCode]//TTools and TLink->Export files and Convert File->Custom format properties->check box
[]
[G ]
[]
[Gb]//units of files size - send file dialog
[]
[GC3 Data File]//not used
[]
[General]//tab name, properties for Surface|TTools; CoGo; Inverse; Properties for CoGoLine; Page name|TTools, TLink; Tab View; DL tab; DL Occupation Properties; page name|TTools; Codes; Attribute properties; Page name|TTools; TLink; Localization; Properties; Page name|TTools; Tlink; -> Job Configuration (Configuration)->Coordinate Systems -> list for geoobjects (geoids, datums and etc.)-> Properties dialog for geoobject -. Page name|TTools and TLink -> Tabular View-> General tab name in Antenna Properties dialog, Occupation Properties dialog, Observation Properies dialog,|for internal use only|TTools and TLink->Device properties dialog->Tab name|MapDaigramFile's section name of properties|TTools and TLink->page General in Properties dialogs|for internal use only|for internal use|TTools->Report->report Configuration->Project Report Options name|TTools; Adjustment Report Options,internal use|for internal use only|TT->Report->Report Configuration->TS Obs report options->Page name(for internal use)|TT->Report->Report Configuration->Cut Sheet Report->Options->tab name(for internal use)|Section Name|for internal use only|for internal use only|TT->Roads tab and X-Section Templates tab->Properties dialog->General tab name|TL->File properties->page name; TT->Custom Instrument Properties->Page name; TT and TL->Properties for TS Obs and TS Occup->page name|TT->Job Info->tab name|for internal use only|TTools and TLink -> Tabular View-> General tab name in Antenna Properties dialog, Occupation Properties dialog, Observation Properies dialog,|for internal use only
[Genel]
[General\\Curve]//TT->Roads tab->Horz. element (except Line)->Properties->General page->group box name
[]
[General\\Length]//TT->Roads tab->Horz. element->Properties->General page->group box name
[]
[General\\Point]//TT->Roads tab->Horiz. Element->Intersection->for internal use
[]
[General\\Start Coordinates]//TT->Roads tab->Road properties->Page General->Group box name
[]
[General\\Troposphere]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[General\\Troposphere\\Estimate Zenith Troposphere Delay (for static only)]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[General\Kinematic]
[]
[General\Static]//TT->Process Propereties->group box name
[]
[General\Static\Minimum duration]//TT->Process properties->GPS+Post Process tab-> group box name
[]
[General\Stop&Go]
[]
[Generate lines from the alignment\nGenerate lines]
[]
[Generate points on the alignment\nGenerate points]
[]
[Geodetic Distance]//TTools; Inverse window; bottom pane and Properties window
[]
[Geodetic info incomplete]//error message
[]
[Geodetic info is incomplete]//error message
[]
[Geoid]//TTools; TLink -> Job Configuration (Configuration) -> Geoid; list box name|TT->Job Configuration->Coordinate Systems->list box name
[Jeoid]
[Geoid Boundaries]//for internal use only
[]
[Geoid Canadian95 pasport file( h*.slv)]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name for certain type of Canadian Geoids (in additional open dialog)
[]
[Geoid could not be loaded]//error message box
[]
[Geoid File]//TTiils; TLink ->   Convert File -> File format list box- text
[Jeoid Dosyası]
[Geoid model is not in the list. Elevation calculations will work incorrectly if you do not load this geoid]
[]
[Geoid Regional Model]//for internal use only
[]
[Geoid2003 Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Geoid99/Geoid2003 Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[GeoidDenmark Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[GeoidDutch Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[GeoidFrench98 RAF98 Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Geoids List]//TT and TL->Job Configuration->Coordinate Systems->Geoid List->window name
[Geoid Listesi]
[GeoidSwedish Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[GeoidSwiss2004 Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[GeoPoint Compare Points]
[]
[GeoTIFF Background Image File]//not used
[]
[GeoTIFF files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[GeoTIFF map not allowed with datum]//error message
[]
[GFW files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[GIS]
[]
[GIS\\Link DL Files]//TTools; Export; for internal use only
[]
[GLN ]//TT->Residiul view window->legend window
[]
[GLN Sat Count]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[]
[Global Geoid File]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Global Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[GLONASS]//Advanced option name for import/export
[GLONASS]
[GLONASS Satellites]//TTools and TLink->GPS Obs Tab->Properties->field name
[GLONASS Uyduları]
[Glonass sv = %d Time = %s\n]//not used
[]
[GMT%s]//TTools and TLink->template used to generate texts in Job Configuration->Display->Time->GPS Time Zone Offset combo box|TTools and TLink->template used to generate texts in occupation time axis|TTools and TLink->template used to generate texts in Residiul time axis
[]
[Go]//TTools and TLink->GPS Occupations->Method->possible value
[]
[Go back]//for internal use only
[Geri al]
[Go to parent folder]//for internal use only|for internal use only
[Üst klasöre git]
[Go to previous folder]//for internal use only
[Önceki klasöre git]
[Go\\Obs\\Disabled]//TTools; Filters window
[]
[Go\\Obs\\Failed]//TTools; Filters window
[]
[Go\\Obs\\Potential]//TTools; Filters window
[]
[Go\\Obs\\Processed]//TTools; Filters window
[]
[Go\\Occupations]//TTools; Filters window
[]
[Go\\Processed Points]//TTools; Filters window
[]
[Go\\Unprocessed Points]//TTools; Filters window
[]
[Goad && Goodman]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Gon]//TLink; Resect Export, Angular Unit Name
[Grad]
[Gons]//TTools->Job Configuration->Units->Angular Unit list box->possible value; TTools and TLink->Status Bar->list box for angular units
[]
[GPS]//TTools; Adjustment;|Advanced option name for import/export
[]
[GPS ]//TT->Residiul view window->legend window
[]
[GPS %s-%s ]
[]
[GPS Base Occupations]//not used
[]
[GPS Base Occupations List\nGPS Base Occupations List]//for internal use
[]
[GPS Go]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[GPS Kinematic]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[GPS misclosure]//TTools; Adjustment; Column name
[]
[GPS Non-processed Kinematic]//TTools->MapView->legend window
[]
[GPS Non-processed Static]//TTools->MapView->legend window
[]
[GPS Non-processed Stop]//TTools->MapView->legend window
[]
[GPS Obs]//TTools and TLink -> Menu Bar->View->Tabular View Options->Tab name
[GPS Gözl.]
[GPS Obs Report]//Report Hint
[]
[GPS Obs Report Options]//Report Options Name
[]
[GPS Observations]//for internal use only
[GPS Gözlemleri]
[GPS Observations List\nGPS Observations List]//for internal use
[]
[GPS Occupation]//for internal use only|not used
[GPS Oturumu]
[GPS Occupation View Options]//for internal use
[GPS Oturum Opsiyonlarını Göster]
[GPS Occupations]//TTools and TLink -> Tabular View->Tab name
[GPS Oturumları]
[GPS Occupations List\nGPS Occupations List]//TTools and TLink, tooltip
[]
[GPS Offset]//TTools->Map View->Legend window->point type
[]
[GPS Only]//TT->Process properties->GPS+Post Process tab->System list box->possible value
[]
[GPS PP Kinematic]//TTools->Map View->Legend window->point type
[]
[GPS PP Static]//TTools->Map View->Legend window->point type
[]
[GPS PP Stop]//TTools->Map View->Legend window->point type
[]
[GPS Precisions]//for internal use only
[]
[GPS Sat Count]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[]
[GPS Satellites]//TTools and TLink->GPS Obs Tab->Properties->field name
[GPS Uyduları]
[GPS Static]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[GPS Stop]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[GPS Time]//TT->Occupation view window->axis name|TT->Residiul view window->axis name
[]
[GPS Time Zone Offset]//TTools and TLink->Job Configuration->Display->Time
[GPS Zaman Bölge Ofseti]
[GPS vectors only]//TT->Repeated Observations Report Options->radio button name
[]
[GPS week,day]//TTools and TLink->GPS Occupations Properties->Page General->field name
[GPS haftası,günü]
[GPS/GLONASS measurements PostProcessing\nDGPS PostProcessing]//hint text in the Status Bar
[]
[GPS/GLONASS measurements PostProcessing\nGPS+ PostProcessing]//hint text in the Status Bar
[]
[GPS+]//TT->Process properties->GPS+Post Process tab->System list box->possible value
[]
[GPS+ PostProcess Options]//not used
[]
[GPS+ PostProcess: ]//log message
[]
[GPS+ PostProcessing]//TT->Tool Bar->Process->GPS+ PostProcessing
[]
[GPS+ Raw Data]//TTools and TLink -> Import file or Convert file ->Format name list box->file type
[GPS+ Ham Data]
[GPS-vectors are normired by UWE]//TTools;  error message under Adjustment
[]
[Grade]//TT->X-Section Templates tab->right panel->X-Section segment properties->field name
[Eğim]
[Gradient fill]//Contour lines dialog->gradient fill
[]
[Graphic]//TT->Roads tab->left panel->node name
[]
[Graphic Views]//TT->Roads tab and X-Section Templates tab->right panel->Options->page name
[]
[Graphic Views\\Labels]//TT->Roads tab and X-Section Templates tab->right panel->Options->Graphic Views->group box name
[Grafik Görnüm\\Etiketler]
[Gray]//TTools->attribute properies->color list box->possible value
[]
[Great angle misclosure]//diagnostic message during Adjustment and Compute coordinate
[]
[Greater than]//TT->Tool Bar->Select->Select Points, GPS Obs, TS Obs and etc.->Std Dev Horizontal and Std Dev Vertical list boxes->value
[]
[Green]//TTools->attribute properies->color list box->possible value
[]
[Grid]//TTools and TLink->Export files and Convert File->Custom format properties->Coordinate system list box->possible value|TTools (Job Configuration and list box in the Status Bar)and TLink (list box in the Status Bar)->possible value
[]
[Grid Azimuth]//TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name
[Grid Azimut]
[Grid Distance]//TTools; Inverse window; bottom pane and Properties window
[]
[Grid Easting]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[]
[Grid Northing]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[]
[Grid to Ground]//for internal use only
[]
[Grid, Ell.H]//TT and TL->in advanced import/export options, convertation and open file->Coordinate type->content
[Grid, Elp.H]
[Grid->Ground]//TT->Grid to Ground dialog (from Job configuration for example)->window caption
[]
[Grid->Ground Parameters]//TTools->Job Configuration; Grid->Ground Parameters window caption and TLink->Convert File; Grid->Ground Parameters
[Grid->Yer Parametreleri]
[Ground]//TTools and TLink->Export files and Convert File->Custom format properties->Coordinate system list box->possible value|for internal use only|coordinate system name for map diagram file|TTools (Job Configuration and list box in the Status Bar)and TLink (list box in the Status Bar)->possible value
[Yer]
[Ground Azimuth]//TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name
[Yer Azimutu]
[Ground Dist]//TTools->CoGo; Intersect + PointInDirection
[]
[Ground Distance]//TTools; Inverse window; bottom pane and Properties window|Resolve Duplicate Points dialog, column name
[]
[Ground Easting]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[Sağa Değer (Y)]
[Ground Northing]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[Yukarı Değer (X)]
[Ground Origin]//TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->radio button name|TT->Grid to Ground dialog (from Job configuration for example)->radio button name
[Yer Orjini]
[Ground Origin\\Ground North]//for internal use only
[Yer Orjini\\Yer Kuzeyi]
[GroundMeasure\\Link MULTI Files]//for internal use only
[Yer Ölçme\\Link ÇOKLU Dosyaları]
[Group]//TTools->File->Remote users->add group->dlg caption|Caption of prop. dlg
[]
[Group of close points: ]//TTools; Adjustment; diagnistic message
[]
[Groups]//TTools->File->Remote users->add user->add group->dlg caption
[]
[GTS-210/310-10 Points]//TTools->Export->Format name
[GTS-210/310-10 Noktaları]
[GTS-210/310-12 Points]//TTools->Export->Format name
[GTS-210/310-12 Noktaları]
[GTS-210_310 Raw]//TTools->Export->Format name
[GTS-210_310 Ham]
[GTS-6 Raw]//TTools->Export->Format name
[GTS-6 Ham]
[GTS-7 Points]//TTools->Export->Format name
[GTS-7 Noktaları]
[GTS-7 Raw]//TTools->Export->Format name
[GTS-7 Ham]
[GTS-7+ Raw]//TTools->Export->Format name
[GTS-7+ Ham]
[h]//TT->Tool Bar->Select->Select GPS Occup and GPS Obs->Duration->spin edit name
[]
[H]//TLink; Resect Export, HA Measurement         
[YA]
[H on Bench]//error message
[]
[H0]//for internal use only
[]
[HA misclosure(&quot;)]//TTools; Adjustment; Column name
[]
[HA Sigma, (sec)]//Process properties dialog (TLink spec.); Compute Coordinates page; field HA Sigma 
[Sigma YA,(sn) ]
[HAngle Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[YtyAçı Kaba Hatası]
[Hardware lock driver either is not installed or not working properly]//error message
[]
[HD]//TL->Convert File->Advanced options->right panel->radio button name
[]
[HDist Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[YM Kaba Hatası]
[HDOP]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink->GPS Obs Tab->Properties->field name
[]
[Height]//TTools; Adjustment;  diagnostic message|TTools and TLink->Export files and Convert File->Custom format properties->field in the left panel|TLink; Resect Export, Header Field name|not used|for internal use only???|TTools->thumbnail/stereopair view options->Labels tab->Check box|TTools->Map View options and Cad View options->Labels tab->Check box|TTools; Adjustment Report, Output use
[Yükseklik]
[Height is]//TT->Point tab->Properties for Point->Offset tab->group box name
[]
[Height/Elev]//TTools->CoGo; Options
[]
[Heights]//TTools->Job Configuration->Display->Precisions
[Yükseklikler]
[Help]//button name|not used|button name|not used
[]
[Hide]//for internal use only
[]
[Hide pane]//tooltip
[]
[History]//History dlg caption
[]
[Hor.Dist]//TTools; Inverse window; bottom pane
[]
[HorAngle]//dTTools spec.; diagnostics about errors under Adjustment when bad connected network
[]
[Horiz. Precision]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[Yatay Hassasiyet]
[Horizontal]//TTools; Adjustment; Column name|TTools; TLink; Localization window; Properties; field Use; field content|TT ->in advanced import/export options->Distance mode list box->value(for example export TS Obs->FC5 Raw)
[]
[Horizontal Adjustment will NOT be done ]//TTools; Adjustment; diagnistic message 
[]
[Horizontal Alignment]
[]
[Horizontal alignment]//TT->Roads tab->left panel->node name
[]
[Horizontal and Vertical]//TTools; TLink; Localization window; Properties; field Use; field content
[Yatay ve Düşey]
[Horizontal Circle]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel  |TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Yatay Hata]
[Horizontal circle, Horizontal distance, Vertical distance]//for internal use
[Yatay Hata, Yatay Mesafe, Düşey Mesafe]
[Horizontal circle, Vertical angle, Slope distance]//for internal use
[Yatay Hata, Düşey Açı, Eğik Mesafe]
[Horizontal circle, Zenith angle, Slope distance]//for internal use
[Yatay Hata, Başucu Açısı, eğik Mesafe]
[Horizontal Control]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Horizontal Distance]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Yatay Mesafe]
[Horizontal Level]//TL->Convert File->Advanced options->radio button name
[Yatay Seviye]
[Horizontal level]//TT and TL->in advanced import/export options and open file->Vertical angle mode list box->value
[Yatay seviye]
[Horizontal Precision]//TTools and TLink ->GPS Obs properties-> page Observation ->field name
[Yatay Hassasiyet]
[Horizontal Resection]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[Yatay Kestirme]
[Horizontal&Vertical Control]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Horz]//TTools; Adjustment; diagnistic message
[]
[Horz Control Points: ]//TTools; Adjustment; diagnistic message 
[]
[Horz Element]
[]
[Horz only]//TTools; Adjustment; diagnistic message
[]
[Horz Tolerance]//TT->Loop Closure Report->Column name
[]
[Horz Tolerance abs.]//TT->Loop Closures Report->column name
[]
[Horz Tolerance rel.(ppm)]//TT->Loop Closures Report->column name
[]
[Horz. Accuracy]//TT->Custom TS Instrument list->column name
[]
[Horz. Vertical]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[Yatay Düşey]
[Horz+Vert]//TTools; Adjustment; diagnistic message
[]
[Hour]//TTools->Occupation view->Split GPS Occupations dialog->Split by list box->value
[]
[Ht Residual]//TTools, DL Obs Properties dialog; Adjustment Page, field name|TTools; TLink; Localization; Properties; field name
[]
[Ht. Measurement]//TTools, TLink; Tab View; DL Obs Properties; Observation tab;
[Ht. Ölçümü]
[HTML]//TT->Report Configuration->Report format->radio button name
[]
[http://www.topconpositioning.com/]//www.topconpositioning.com/"//web address, opening from menu Help/Feedback/Topcon On Web|www.topconpositioning.com/"//web address, opening from menu Help/Feedback/Topcon On Web
[http://www.paksoyteknik.com.tr]
[Humidity]//for internal use only
[Nem]
[Humidity: (%)]//TT->Process properties->GPS+Post Process tab (advanced module)
[Nem: (%)]
[HV Control]//TTools->Map View->Legend window->point type
[]
[Hz]//TLink; Resect Export, Header Field name
[Yty]
[Hz angle]//TT->Tool Bar->Select->Select TS Obs->list box name
[]
[Hz Control]//TTools->Map View->Legend window->point type
[]
[Hz dist]//TT->Tool Bar->Select->Select TS Obs->list box name
[]
[Hz precision]//TT->Tool Bar->Select->Select GPS Obs.->list box name
[]
[Hz residual]//TT->Tool Bar->Select->Select TS Obs->list box name
[]
[Hz. Dist]//TT->X-Section Templates tab->right panel->X-Section segment properties->field name
[Yty.Mesafe]
[Hz. Offset from CL]//TT->X-Section Templates tab->right panel->X-Section segment properties->field name
[Aks dan Yty Ofset]
[I&mport...]//TTools->Menu Bar->Job->menu item
[]
[I&nverse Point to Line...]//TTools; Menu Bar; COGO; menu item Point In Direction...
[]
[Icon]//TTools and TLink->Tabular View->column header
[İkon]
[Identical Points]//TTools; Adjustment; Table header  |TT->Job Configuration->Quality Control->Automatic Tests->check box name
[]
[Identical Points List]//TTools; TLink; Localization; for internal use only
[Aynı Noktalar Listesi]
[Identical Points QC filter\nIdentical Points QC filter]//internal use
[]
[Identical Points Report]//TT->Identical Points Report Options window->tool tip
[]
[Identical Points Report Options]//TT->Identical Points Report Options window name
[]
[If image coordinate system is different from job coordinate system:]//TTools; Background images dialog;
[]
[if minimum observation length (km)]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Ignore first line]//TTools->Export->Cut Sheet  user-defined format->check box name|TTools and TLink->Export files and Convert File->Custom format properties->check box name
[]
[Ignore QC]
[]
[Illegal Circle = %.2lf\xB0 on TS Obs %s]//diagnostic message during Compute coordinate
[]
[Illegal expression]
[]
[Illegal function name]
[]
[Illegal Interval]//TTools->CoGo; Convert road to DTM
[]
[Illegal Name]//TTools->CoGo; Convert road to DTM
[]
[Illegal parameter type]
[]
[Illegal parameter value %s]
[]
[Illegal parameters number]
[]
[Illegal type]
[]
[Ima&ge View]//TTools->Menu Bar->View
[]
[Image]//TTools, properties for Surface|Ttools and TLink->Images tab->Proprties for image->page name|TT and TL->TS Obs properties->tab name
[]
[Image conversion is impossible due to inconsistent coordinate systems]//View->Background Images...->AddImage->Convert image->Save (message box that appears if the image conversion is impossible)
[]
[Image Import: ]//message for progress indicator in status bar
[]
[Image Measured]//not used
[]
[Image measured]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Image measured points filter\nImage measured points filter]//for internal use only
[]
[Image Measuremens]//CAD View window, image measurements diagram name
[]
[Image Measurement]//internal use
[]
[Image Measurement View Options]//orientation points
[]
[Image Measurements]//TTools->thumbnail/stereopair view options->Tab name
[]
[Image Transformation]//Ttools->Stereopairs tab->transformation from Orientation to Stereo View->text in the Status Bar
[]
[Image View]//Ttools and TLink->Images tab->Pop-up menu item for image|TTools->Window title
[Resme Bak]
[Image View Options]//Ttools->View->Options->Images View->dialog caption
[]
[Image(s) have no orientation. Stereopair cannot be created]//TTools->Stereopairs tab->message
[]
[Images]//Ttools and Tlinlk->Page name|TT and TL - tab name in Properties for TS points with telescopic images
[Resimler]
[Images used in this job:]//TTools; Background images dialog;
[]
[Images View Options]//header of "Images View Options" dialog (View->Images View Options)
[]
[Images View\nImages View]//tooltip
[]
[Imaging]//name of module, in Autorizations dialog and in About
[]
[Import]
[]
[Import antenna calibration]//import antenna type set button name : TTools and TLink -> Job Configuration(Equipment) -> Import Antenna
[]
[Import File Options]//for internal use only
[]
[Import files from device\nImport from device]//TTool sand Tlink->Import from Device->text in the Status Bar
[Cihazdan dosyaları yükle\nCihazdan yükle]
[Import files from external device\nImport from Device]//TTools sand Tlink->Import from Device->text in the Status Bar
[Cihazdan yükle\nCihazdan yükle]
[Import from &Device...]//TTools and TLink->Menu Bar->File(TLink) and Job(TTools)->menu item
[Cihazdan &Yükle...]
[Import from AutoCAD DTM file]//for internal use only
[AutoCAD DTM dosyalarını yükle]
[Import from Device]//TTools and TLink->log message and Import dialog caption
[Cihazdan YÜKLE]
[Import from Device Options]//for internal use only
[]
[Import from Device...]//TTools and TLink->Menu Bar->File(TLink) and Job(TTools)->menu item
[Cihazdan YÜKLE...]
[Import from Device\nImport from Device]//TTool sand Tlink->Import from Device->text in the Status Bar
[]
[Import from DGN/ISFF format]//for internal use only
[]
[Import from DL file]//TTools; Import; Text in The Status Bar during the importing of DL files
[]
[Import from files\nImport from files]//TTools->Import->text in the Status Bar
[]
[Import from LN3 format]//for internal use only
[LN3 formatında yükle]
[Import from RINEX files]//Import RINEX, Progress bar text
[]
[Import from Shape Files]//for internal use
[Shape Dosyalarından Yükle]
[Import from TDS file]//Progress bar text
[]
[Import from Topcon Tools Job\nImport from Topcon Tools Job]//for internal use
[]
[Import from TPD file]//Progress bar text
[]
[Import from TPS file]//log message
[]
[Import is not supported for this device]//TTools and TLink->Import from Device->message
[Bu cihazdan yükleme desteklenmiyor]
[Import JPS Files]//for internal use only
[JPS Dosyalarını Yükle]
[Import processing result from %s]//log message
[]
[Import Rinex Files]//for internal use only
[Rinex Dosyaları Yükle]
[Import stat: Agency:%s CoordSystem:%s SV:%d NEphem:%d]
[]
[Import Topcon Tools Job]//for internal use
[Topcon Tools İşi Yükle]
[Import Topcon XML Antenna files]
[]
[Import TopSURV Files]
[]
[Imported]//TTools and TLink->GPS Obs Properties ->Method, possible value
[Yüklendi]
[Imported %d RTK vectors]//not used|log message
[]
[Imported %d stations]//not used|log message
[]
[Imported total %d points, %d have Ground coord and %d have GPS coord]//not used|log message
[]
[Importing data]//text in the Status Bar
[Data Yükleniyor]
[In %d pos. literal '%s' not found]//for internal use only log message
[]
[In Demo Mode you can have not more then 5 elements per road]//TTools->Demo mode->Message Box
[]
[In Demo Mode you can have not more then 5 lines per job]//TTools demo mode->Convert road to points
[]
[In Demo Mode you can have not more then 5 points per job]//TT->Demo mode->Add DL Obs->message box|TTools->Demo mode->Message Box|TT-Demo mode->message box when creating kinematic points|TTools demo mode->Convert road to points|TT->Demo mode->Add TS Obs->message box
[]
[In Demo Mode you can have not more then 5 points, roads and elements in the road per job]//TT->Tool Bar->Help->Access Code dialog-Demo mode->message box
[]
[In Demo Mode you can have not more then 5 roads per job]//TTools->Demo mode->Message Box
[]
[In Demo Mode you can have not more then 5 vertices per line]//TTools demo mode->Convert road to points
[]
[In direction of]//TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name
[Doğrultusunda]
[In early specification of SP3 format version 'b' FileType in pos 1 (line:13)]
[]
[In this version, localization is recomputed automatically as you add or delete points. However, you can press OK to make absolutely sure they have been recomputed]//TTools; TLink; Localization; message box while localization
[Bu versiyonda lokalizasyon otomatik tekrar hesaplanır veya siz ilave ettiğiniz gibi, noktaları silin.Eminseniz OK ya basıp işleme devam edin.]
[In&verse...]//TTools; Menu Bar; COGO; menu item Inverse...
[Te&rsi...]
[Include GPS Occupations]
[]
[Include GPS PP Static Vectors]
[]
[Include Points]
[]
[Include RTK Obs]
[]
[Include TS Obs]
[]
[Included report items:]//TT->Report Configuration->right panel name
[]
[Incoming]//Direction
[Giren]
[Incorrect coordinate system for some objects]//error message
[Bazı objelerin koordinat sistemleri hatalı]
[Incorrect epoch line]//log message
[Epok çizgisi hatalı]
[Incorrect file format]//error message|error message
[Yanlış dosya formatı]
[Incorrect parameters use: ]
[]
[Incorrect time for split]//TTools->Occupation view->Split->message
[]
[Infinity looping]//for internal use only log message
[Kapanmalar çözümsüz]
[Inner Constraint %dD Adjustment]//TTools;  error message under Adjustment
[]
[Input file has null legnth]//for internal use only log message
[Giriş dosyalarının geçersiz uzunluğu var]
[Input Surfaces are corrupt]//TTools->CoGo->Compare Surfaces
[]
[Ins]//Shortcut Description
[Ekl]
[Insert a new DL Obs to the current job\nInsert Manual DL Obs]//tooltip for Add DL Obs menu item
[]
[Insert a new horizontal element to the road\nInsert line to road]//TT->Roads tab
[]
[Insert a new TS Obs to the current job\nInsert Manual TS Obs]//tooltip for Add TS Obs menu item
[]
[Insert a new vertical element to the road\nInsert vertical element to road]//TT->Roads tab
[]
[Insert Horz Element]//TT->Roads tab
[]
[Insert Manual DL Obs]//TTools, caption of Add DL Obs dialog
[Manuel DL Okuması Ekle]
[Insert Manual TS Obs]//TTools, caption of Add TS Obs dialog
[Manuel TS Okuması Ekle]
[Insert new Offset to X-Section Template\nInsert new Offset]//TT->X-Section Templates tab->right panel->hint text
[]
[Insert Offset]//TT->X-Section Templates tab->right panel->Pop-up menu item
[Ofset Ekle]
[Insert point to the selected line\nInsert Points to Line]//TTools, tooltip
[]
[Insert Point(s) to Line]//TTools,context menu for lines
[]
[Insert points to the selected line\nInsert Points to Line]//TTools, tooltip
[]
[Insert Vert. Element]//TT->Roads tab
[]
[Instr. height]//TLink; Resect Export, Header Field name
[Alet yüksekliği]
[Instruction]//TTools (Import from device) and TLink (Import from device and Export to Device)->bottom part of the window caption
[Talimat]
[Instrument]//TL->File properties->Session tab->field name
[Cihaz]
[Instrument Elevation]//TTools, TLink; Tab View; DL tab; field name
[Alet Kotu]
[Instrument Height]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TT and TL->TSObs tab->left panel->column name; TT and TL->TS  occupation properties->field name
[Alet Yüksekliği]
[Instrument height]//TT->Tool Bar->Select->Select TS Occup->Duration->list box name
[Alet yüksekliği]
[Instrument Point]//Ttools->Scan Session tab->Scan Session Property->General tab->field name
[Cihaz Noktası]
[Instrument Type]//TT->Properties for TS Occupation->tab name and list box name
[Cihaz Tipi]
[Insufficient disk space at the device]//TT and TL->Export to Device->error message
[Cihazda yetersiz disk alanı]
[Insufficient physical memory on the device. Try closing some applications on the controller or changing the memory settings]//TT and TL->Export to Device->error message
[ Cihazdaki yetersiz fiziksel bellek.  Kont.Ünitesinde bazı uygulamaları kapatmayı deneyin veya bellek ayarlarını  değiştirin.]
[Insufficient space on CF. There shall be free space on CF 3 times the size of your job]//TT and TL->Export to Device,Import from Device ->error message
[CF Kartta bellek yetersiz. İşinizin boyutunu küçültürseniz boş alan açılabilir.]
[Integer]//TTools; Codes; New Attribute; Pop-up menu command|TTools->Codes->New Attribute->possible attribuite type
[TamSayı]
[Interactive Blunder Rejection]//TTools; Adjustment; Button name
[]
[Internal Error on Observation ]//TTools; error message under Adjustment
[]
[Intersect Point]//TTools->CoGo;Intersection
[]
[Intersect Task Report]//TTools; CoGo; Intersection, report name
[]
[Intersection]//TTools->CoGo;Intersection|TT->Roads tab->type of the added horizontal element
[Kesişim]
[Intersection Pt]//TT->Roads tab->Add Horz. Element: Intersection window->list box name
[Some Noktası]
[Intersection...]//TTools; Menu Bar; COGO; menu item Intersection...
[Kesişim...]
[Intersection\nView]//TTools->CoGo;Intersection
[]
[Interval]//TTools->CoGo; Convert road to DTM|for internal use only|Contour lines dialog->Interval
[Aralık]
[Interval 1 - From:]//TT->Filters window->By Time tab->list box name
[Aralık 1 - den:]
[Interval 1 - To:]//TT->Filters window->By Time tab->list box name
[Aralık 1 - e:]
[Interval 2 - From:]//TT->Filters window->By Time tab->list box name
[Aralık 2 - den:]
[Interval 2 - To:]//TT->Filters window->By Time tab->list box name
[Aralık 2 - e:]
[Invalid]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->Code status->value
[Geçersiz]
[Invalid data]//TT and TL->Export to Device,Import from Device ->error message
[Geçersiz data]
[Invalid file %1]//error message
[Geçersiz dosya %1]
[Invalid file or directory name: %s]//message box
[]
[Invalid format]//not used (only in comments)
[Geçersiz format]
[Invalid input]//error message
[Geçersiz giriş]
[Invalid job name]//TT->New Job->message
[Geçersiz iş ismi]
[Invalid satellite number in line %d]
[]
[Inverse]//TTools->CoGo; Inverse
[Tersi]
[Inverse From]//TTools; for internal use only
[den Tersi]
[Inverse Point to Line]//TTools->CoGo;Inv PTL
[]
[Inverse Point To Line Task Report]//TTools; CoGo; Inverse PTL, report name    
[]
[Inverse Point to Line...]//TTools; Menu Bar; COGO; menu item Point In Direction...
[]
[Inverse Point to Line\nView]//TTools->CoGo;Inv PTL
[]
[Inverse Task Report]//TTools; CoGo; Inverse, report name
[]
[Inverse To]//TTools; for internal use only
[]
[Inverse...]//TTools; Menu Bar; COGO; menu item Inverse...
[]
[Inverse\nView]//TTools->CoGo; Inverse
[]
[Invert Selection]//TT->Tool Bar->Select->command name
[]
[Invert selection\nInvert selection]//TT->Tool Bar->Invert Selection->hint text in the Status Bar
[]
[inverted]//log message
[ters]
[Iono Free]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[]
[IonoFree]//TT->Residiul view window->legend window
[]
[is password protected. Enter the password:]//Ttools->Map View->Options>MrSid Background file activation->Password window->text|Ttools->Map View->Options>MrSid Background file activation->Password window->text
[şifre ile korunuyor.Lütfen şifreyi girin:]
[Is Zenital]//not used
[]
[ISPOL]//TTools->Export->Format name
[]
[JDD Topcon Feature File]//TTools; Export to File; Format name
[JDD Topcon Özelk.Dosyası]
[JGW files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[Job]//TLink; Resect Export, Header Field name|TL->File properties->Session tab->field name|Internal use
[İş]
[Job &info...]
[]
[Job &Info...\nDisplay properties of current job\nProperties]//TT->Tool Bar->Job->Job Info
[]
[Job code]//TLink; GPSDataTransfer Export Options, Processing  Agency Code input field name|TLink; BlueBook Export Options, Processing  Agency Code input field name
[İş kodu]
[Job configuration]//TTools; Job configuration dialog caption|TT->Tool Bar-Job->Job Configuration
[İş ayarları]
[Job location]//TT->Creare a new job->field name
[]
[Job name]//TT->Creare a new job->field name
[]
[Job path: ]//not used
[]
[Job Properties]//for internal use
[İş Özellikleri]
[Job type]//TT->for future release
[]
[Jobs list]//for internal use
[]
[JPEG Files (*.jpg)|*.jpg|Bitmap Files (*.bmp)|*.bmp||]//TT and TL->Tab View->Point properties->Photo Notes tab->file types
[]
[JPS -> TPD has not converted]//not used
[]
[Kalinnikov]//for internal use only
[]
[Kb]//units of files size - send file dialog
[]
[Keep Scale 1.000]//TTools;TLink -> ToolBar -> Process -> Localization -> check box name
[Ölçeği Sakla 1.000]
[Key]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->field name
[]
[Key Value]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->field name
[]
[Kinematic]//TTools and TLink ->Properties for Occupation->field Method->possible field content
[Kinematik]
[Kinematic Horizontal Precision]//TT->Job Configuration->Quality Control->Point Precisions tab->field name
[]
[Kinematic occupations]//TT->Occupation View window->Legend window
[]
[Kinematic vector]//for internal use only
[Kinematik vektör]
[Kinematic Vertical Precision]//TT->Job Configuration->Quality Control->Point Precisions tab->field name
[]
[Kinematic:]//for internal use only
[Kinematik:]
[Kinematic\\Obs\\Disabled]//TTools; Filters window
[]
[Kinematic\\Obs\\Failed]//TTools; Filters window
[]
[Kinematic\\Obs\\Potential]//TTools; Filters window
[]
[Kinematic\\Obs\\Processed]//TTools; Filters window
[]
[Kinematic\\Occupations]//TTools; Filters window
[]
[Kinematic\\Processed Points]//TTools; Filters window
[]
[Kinematic\\Unprocessed Points]//TTools; Filters window
[]
[L1]//Advanced option name for import/export|TT->Residiul view window->legend window
[]
[L1 Base offset(A1)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name   
[L1 Baz ofseti(A1)]
[L1 Easting offset(E1)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name    
[L1 Sağa Değer ofseti(E1)]
[L1 Northing offset(N1)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name   
[L1 Yukarı değer ofseti(N1)]
[L1 Plane offset(C1)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name    
[L1 Düzlem ofseti(C1)]
[L1&L2]//for internal use only
[L1&L2]
[L2]//Advanced option name for import/export|TT->Residiul view window->legend window
[L2]
[L2 Base offset(A2)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name  
[L2 Baz ofseti(A2)]
[L2 Easting offset(E2)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name         
[L2 Sağa Değer ofseti(E2)]
[L2 Northing offset(N2)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name         
[L2 Yukarı değer ofseti(N2)]
[L2 Plane offset(C2)]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name    
[L2 Düzlem ofseti(C2)]
[Labels]//TTools->Map View options and Cad View options->tab name
[Etiketler]
[Labels properties]//not used
[]
[Labels\\Kinematic points\\Show on cursor]//TTools->Map View options and Cad View options->Labels tab->Check box name
[]
[Labels\\Kinematic points\\Show on map]//TTools->Map View options and Cad View options->Labels tab->Check box name
[]
[Labels\\Kinematic points\\Show on status bar]//TTools->Map View options and Cad View options->Labels tab->Check box name
[]
[Labels\\Show on cursor]//TTools->thumbnail/stereopair view options->Labels tab->Check box name
[Etiketler\\Kursor da göster]
[Labels\\Show on map]//TTools->thumbnail/stereopair view options->Labels tab->Check box name
[Etiketler\\Harita da göster]
[Labels\\Show on status bar]//TTools->thumbnail/stereopair view options->Labels tab->Check box name
[Etiketler\\Durum çubuğunda göster]
[Labels\\Static points\\Show on cursor]//TTools->Map View options and Cad View options->Labels tab->Check box name
[Etiketler\\Statik noktalar\\Kursor da göster]
[Labels\\Static points\\Show on map]//TTools->Map View options and Cad View options->Labels tab->Check box name
[Etiketler\\Statik noktalar\\Harita da göster]
[Labels\\Static points\\Show on status bar]//TTools->Map View options and Cad View options->Labels tab->Check box name
[Etiketler\\Statik noktalar\\Durum çubuğunda göster]
[Lambert]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[Lambert]
[LandXML]//TTools->Export->Format name
[LandXML]
[LandXML Data File]//not used
[LandXML Data Dosyası]
[LandXML GPS Obs]//TTools->Export->Format name
[LandXML GPS Gözl.]
[LandXML Points]//TTools->Import and Export->Format name
[LandXML Noktaları]
[LandXML Roads]//TTools->Import and Export->Format name
[]
[LandXML TS Obs]//TTools->Export->Format name
[]
[Large Icons]//not used
[]
[Last accessed]//TT->Startup dialog->column name
[]
[Last Azimuth is Absent]//diagnostic message during Adjustment and Compute coordinate      
[]
[Last Epoch: ]//log message
[]
[Last Station has'nt Coordinates]//diagnostic message during Adjustment and Compute coordinate       
[]
[Lat, Lon format:]//TT ->in advanced import/export options->for internal use
[]
[Lat, Lon, Elevation]//TT and TL->in advanced import/export options, convertation and open file->Coordinate type->content
[Enl, Boy, Yükseklik]
[Lat, Lon, Ell.H]//TT and TL->in advanced import/export options, convertation and open file->Coordinate type->content
[Enl, Boy, Elp.Yük.]
[Lat, Lon, h]//TTools (Job Configuration and list box in the Status Bar)and TLink (list box in the Status Bar)->possible value
[Enl, Boy, h]
[Lat,Lon]//Ttools(Job Configuration) and TLink(Configuration)->Display->Angles tab->Lat,Lon list box name
[Enl, Boy]
[Lat,Lon (Dec.degrees)]//TTools->Job Configuration->Display->Precisions
[Enl,Boy (Derece)]
[Lat,Lon (seconds)]//TTools->Job Configuration->Display->Precisions
[Enl,Boy (saniye)]
[Lat0]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Enl0]
[Latitude]//TTools; CoGo; Intersection|TTools and TLink->Export files and Convert File->Custom format properties->for BLH system field in the left panel|not used|for internal use only???|TTools->Map View and Cad View->axis name|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[Enlem]
[Latitude/Northing]//TTools->CoGo; Options
[]
[Latitude\\Northing]//TTools and TLink->Tab View->Point tab->Options->column name
[Enlem\\Yukarı Değer]
[Latitude\Northing]//TT->Compare Point Report Options->column name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item|TT->Point summary Report Options->column name
[Enlem\Yukarı Değer]
[LatLon Format]//TTools and TLink->Export files and Convert File->Custom format properties->list box name
[EnlBoy Formatı]
[Layer]//TTools, properties for Surface|TTools->Linework->Properties of Line|Contour lines dialog->Layer|TT->Tool Bar->View->Layers->Column name|TT->Roads tab->Road Properties->list box name|TT->Tool Bar->Select->Select Points->field name
[Tabaka]
[Layers]//TTools -> Window title
[]
[Layers Control]//TTools->Customize toolbars->Commands->buton name
[]
[Least Squares]//Process Properties dialog(TLink spec.), page Compute Coordinates;  List box Adjustment type
[EnKüçük Kareler]
[Left]
[]
[Left 1]//TTools->CoGo;Intersection
[Sol 1]
[Left 2]//TTools->CoGo;Intersection
[Sol 2]
[Legend]//TTools; Legend window name(Map View and Occupation View)|TTools->Legend window name|TT->Occupation View window->Legend window name|TT->Residiul View window->Legend window name
[Lejant]
[Length]//TT->Linework tab->Line properties->field name|TT->Loop Closures Report->column name|TT->Roads tab->Horz and Vertical element->right panel->column name|TT->Tool Bar->Select->Select GPS Obs.->list box name
[Uzunluk]
[Less than]//TT->Tool Bar->Select->Select Points, GPS Obs, TS Obs and etc.->Std Dev Horizontal and Std Dev Vertical list boxes->value
[Daha az]
[Level]//TTools->CoGo->Compare Surfaces; Second Surface type|TTools, TLink; DL Occupation Properties dialog; field Type; text
[]
[Level Pt.]//TTools, TLink; DL Obs Properties dialog; General Page, Type, field content
[]
[Level Run]//TTools, TLink; Tab View; DL tab;  DL Occupation Properties; field name
[Başla Nivelman]
[Leveling ]//TTools; Adjustment;  diagnostic message
[]
[Leveling Failed]//TTools; Adjustment;  diagnostic message
[]
[License agreement:]//not used|not used
[]
[Line]
[]
[Line End]//TTools->CoGo;Inv PTL
[]
[Line length > Max: ]//log message
[Hat uzunlğ > Maks:]
[Line Segment]
[]
[Line Segments Table]//TTools; Linework; for internal use only
[]
[Line Start]//TTools->CoGo;Inv PTL
[]
[Line Style]//TTools->Linework->Properties of Line|TTools->attribute properies->Outline tab->list box name
[Hat Tipi]
[Line Width]//TTools->Linework->Properties of Line|TTools->attribute properies->Outline tab->list box name
[Hat Kalınlığı]
[Line:%d '%c%c...' field '%c%c' is missed]//not used|log message
[]
[Line:%d '%c%c...' Height of reflector is undefined (set to 0.0)]//not used|log message
[]
[Line:%d '%c%c...' Height of station is redefined from %f to %f ]//not used|log message
[]
[Line:%d '%c%c...' Height of station is undefined (set to 0.0)]//not used|log message
[]
[Line:%d '%c%c...' RTK Base is undefined for vector to %s]//not used|log message
[]
[Linear Unit]//???????????|TTools->Job Configuration->Units->Linear Unit list box name|TL->Convert Files->list box name
[Mesafe Birimi]
[Lines]//TTools->Linework->Properties of Line->window name|TTools->Map View ->Legend window
[Hatlar]
[Lines List\nLines List]//for internal use only
[Hatlar Listesi\nHatlar Listesi]
[Lines Tab View Options]//TTools->Linework->options(for internal use only)
[]
[Linework]//TT->Tabular View Optioms window->tab name
[]
[Linework Processor Options]//internal use
[Hatİşlemleri İşlemci Seçenekleri]
[List]//not used
[]
[List configurations]//TT->Job Configuration window->button name
[]
[List of parameters creates NO Diagrams]
[]
[LN3]//TTools->Export->Format name
[]
[Load]//TT->Job Configuration window->List configurations->Configurations list window->button name
[]
[Loading dynamic commands...]//log message
[]
[Loading Feature Code Library..]//not used
[]
[Loading license file...]//TL->log message|TT->log message
[Lisans dosyası yükleniyor...]
[Loading module: ]//log message
[Modül yükleniyor:]
[Loading modules...]//log message|TL->log message|TT->log message
[Modeüller yükleniyor...]
[Loading options...]//log message
[Seçenekler yükleniyor...]
[Local]
[]
[Local Point]//TTools; TLink; Localization; Properties; field name
[Lokal Nokta]
[Local System]//for internal use only|not used
[Lokal Sistem]
[Local time (%s)]//TT->Occupation view window->horizontal axis name (if GPS Time Zone offset)|TT->Residiul view window->horizontal axis name (if GPS Time Zone offset)
[Lokal zaman (%s)]
[Locali&zation]//TTools; TLink; Command name
[Lokali&zasyon]
[Localization]
[]
[Localization GC3]
[Lokalizasyon GC3]
[Localization not found]//error message
[]
[Localization parameters]//TTools; TLink; Localization; for internal use only
[Lokalizasyon parametreleri]
[Localization Points Report]//TT->tooltip
[Lokalizasyon Noktaları Raporu]
[Localization Points Report Options]//for internal use only
[Lokalizasyon Noktaları Raporu Seçenekleri]
[Localization Report]//TTools->Report->report Configuration->hint (for internal use)
[Lokalizasyon Raporu]
[Localization Report Options]//TTools->Report->report Configuration->Localization Report Options name
[]
[Location Name]//not used
[]
[Loging parsing file to: ]//log message(debug)
[]
[Lon0]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Boy0]
[Longitude]//TTools; CoGo; Intersection|TTools and TLink->Export files and Convert File->Custom format properties->for BLH system field in the left panel|not used|for internal use only ???|TTools->Map View and Cad View->axis name|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[Boylam]
[Longitude/Easting]//TTools->CoGo; Options
[Boylam/Sağa Değer]
[Longitude\\Easting]//TTools and TLink->Tab View->Point tab->Options->column name
[Boylam\\Sağa Değer]
[Longitude\Easting]//TT->Compare Point Report Options->column name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item|TT->Point summary Report Options->column name
[Boylam\Sağa Değer]
[Look in:]//for internal use only|TLink-> Export to Device (Export to Total Station from and etc.)->list box name
[Gözat :]
[Loop]//TT->Loop Closure Report->Column name
[Loop]
[Loop Closure Report]//TT->Tool Bar->Process->Loop Clouseres..->Loop Closure Report Options window->tab name
[Loop Kapanma Raporu]
[Loop Closure Report Options]//TT->Tool Bar->Process->Loop Clouseres..->Loop Closure Report Options window caption
[Loop Kapanma Raporu Seçenekleri]
[Loop Closures]//TT->Loop Closures report name
[Loop Kapanmaları]
[Loose of Precision: Matrix correction failed ]//TTools;  error message under Adjustment
[]
[m]//Contour lines dialog->m|TT->Tool Bar->Select->Select GPS Occup and GPS Obs->Duration->spin edit name
[m]
[M&essages\nShow or hide messages window\nMessages window]//TL->Tool Bar->View (for internal use)|TT->Tool Bar->View->for internal use
[M&esaj\nMesaj penceresini göster yada gizle\nMesaj penceresi]
[Magenta]//TTools->attribute properies->color list box->possible value
[Majenta]
[Major lines]//Contour lines dialog->Major lines
[]
[Make sure you have installed ActiveSync and connected to mobile device via ActiveSync.]
[]
[Make topmost]//for internal use only
[]
[Make topmost\nMake this diagram topmost]//not used
[]
[Manage layer visibility and set active layer\nManage layers]//Ttools->Layers Control->tooltip
[]
[Manual]//TTools->Map View->Legend window->point type|TT and TL->in advanced import/export options and open file->Point type list box->value|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Manual points filter\nManual points filter]//for internal use only
[Manuel noktaları filitrele\nManuel noktaları filitrele]
[Manufacturer]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page General-> field name|TT->Custom TS Instrument list->column name and and Properties for Instrument->General tab->field name->General tab->field name
[Üretici]
[Map &View Options...]
[Harita &Görünüm Seçenekleri...]
[MAP Background Image File]//for internal use only
[Harita Arkaplan Resim Dosyası]
[Map Files]//not used
[]
[Map View]//TTools->Window Title
[]
[Map View Item]//for internal use only
[Harita Görünüm Elemanı]
[Map View Item Options]
[]
[Map View Options]//TTools->window name|TT->Map View options window caption
[]
[Mapping Scale]//TTools; TLink ->Job Configuration->Coordinate Systems; Grid to Ground window -> field name; or Convert file dialog -> Grid to Ground
[Harita Ölçeği]
[Mathematical Error ]//TTools;  error message under Adjustment
[Matematiksel Hata]
[Max Satellites]//for internal use only
[Maks. Uydular]
[Max. Distance]//TT->Custom TS Instrument list->column name
[]
[Max.Easting]//properties for Surface; column name in Surface tab and in options
[]
[Max.Elevation]//properties for Surface; column name in Surface tab and in options
[]
[Max.Northing]//properties for Surface; column name in Surface tab and in options
[]
[Maximum]//for internal use only
[Maksimum]
[Maximum Latitude]//TTools; TLink ->   Convert File -> panel To ->File format Geoif file -> field name
[Maksimum Enlem]
[Maximum Length]//for internal use only
[Maksimum Uzunluk]
[Maximum Longitude]//TTools; TLink ->   Convert File -> panel To ->File format Geoif file -> field name
[Maksimum Boylam]
[Mb]//units of files size - send file dialog
[]
[Measure]//TTools, TLink; DL Occupation Properties dialog; field Type; text
[Ölçü]
[Measured]//not used
[]
[Measured Height Method]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name
[Yükseklik Ölçüm Metodu]
[Member Of]//TTools->File->Remote users->User prop.->tab caption
[]
[Member of]//TTools->File->Remote users->add user->prop. name
[]
[Members]//TTools->File->Remote users->Group prop.->tab caption
[]
[Memory allocation error]//Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message|Ttools->Map View->Options->MrSid Background file activation->Password Dialog (appears if MrSID file is password protected)->message
[]
[Menu]//TTools; Codes; New Attribute; Pop-up menu command|TTools->Codes->New Attribute->possible attribuite type
[]
[Menu Attribute]//not used
[]
[Menu Items]//for internal use only
[Menü Elemanları]
[Merge]//TTools->GPS Obs popup menu
[]
[Merge GPS Occupations]//TTools->Occupation view->Merge GPS Occupations dialog caption
[]
[Merge Lines]
[]
[Merge selected lines\nMerge selected lines]
[]
[Merge\nMerge Occupation]//TTools->GPS Obs popup menu
[]
[Merged GPS Occupation Name:]//TTools->Occupation view->Merge GPS Occupations dialog->field name
[]
[Merged GPS Occupations should be belonged to the same points]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same antenna height type]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same antenna offsets]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same antenna serial number]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same antenna type]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same epoch interval]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same method]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same reciever id]//TTools->Occupation view->Merge->message
[]
[Merged GPS Occupations should have the same type of raw measurements]//TTools->Occupation view->Merge->message
[]
[Message]//Conext menu item
[Mesaj]
[Message center]//Command name and dlg caption
[Mesaj merkezi]
[Messages]//messages window
[Mesajlar]
[Messages window\nMessages window]//message window
[Mesajlar penceresi\Mesajlar penceresi]
[Meteo]//not used
[]
[Meteo Measurement]//for internal use only
[Meterolojik Ölçüm]
[Method]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink -> Tabular View ->GPS Occupations tab -> column name|TT->Tool Bar->Select->Select GPS Occup.->list box name
[Metod]
[Method %s is not available: %s]//TLink;  diagnostic message during Compute coordinate
[Metod %s aktif değil: %s]
[Method Least Squares is not inapplicable. We can apply Method %s]//diagnostic message during Compute coordinate
[]
[Metric Unit]//for internal use only
[Metrik Birim]
[Metric unit:]//metric unit in advanced import/export options
[Metrik birim:]
[Metric units]//Ttools->view->Background images->left panel (Available images)->field name
[Metrik birimler]
[Mexican Geoid97 Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[Meksika Jeoid97 Dosyaları]
[Microsoft Excel]//TT->Report Configuration->Report format->radio button name
[Microsoft Excel]
[Microsoft Word]//TT->Report Configuration->Report format->radio button name
[Microsoft Word]
[Mid Ord]//TT->Roads tab->Horz. element->Properties for Curve->field name
[]
[Might be recursion]
[]
[Mils]//TLink; Resect Export, Angular Unit Name|TTools->Job Configuration->Units->Angular Unit list box->possible value; TTools and TLink->Status Bar->list box for angular units
[Mil]
[Min. obs. time(sec)]//TT->Process properties->GPS+Post Process tab->spin edit control name
[Min.gözl.zamanı(sn)]
[Min.Easting]//properties for Surface; column name in Surface tab and in options
[]
[Min.Elevation]//properties for Surface; column name in Surface tab and in options
[]
[Min.Northing]//properties for Surface; column name in Surface tab and in options
[]
[Minimum]//for internal use only
[Minimum]
[Minimum Latitude]//TTools; TLink ->   Convert File -> panel To ->File format Geoif file -> field name
[Minimum Enlem]
[Minimum Longitude]//TTools; TLink ->   Convert File -> panel To ->File format Geoif file -> field name
[Minimum Boylam]
[Minor lines]//Contour lines dialog->Minor lines
[Yardımcı hatlar]
[Minors per major]//Contour lines dialog->Minors per major
[Yardımcılar vasıtasıyla asıl]
[Misnamed Autotopo Rovers]//TT->Job Configuration->Quality Control->Automatic Tests->check box name
[]
[Misnamed Autotopo Rovers QC filter\nMisnamed Autotopo Rovers QC filter]//internal use
[]
[Misnamed Autotopo Rovers Report]//TT->Misnamed Autotopo Rovers Report->tool tip
[]
[Misnamed Autotopo Rovers Report Options]//TT->Misnamed Autotopo Rovers Report Options window name
[]
[Misnamed GPS Occupation Report Options]//TT->Misnamed GPS Occupation Report Options name
[]
[Misnamed GPS Occupations]//TT->Job Configuration->Quality Control->Automatic Tests->check box name
[]
[Misnamed GPS Occupations QC filter\nMisnamed GPS Occupations QC filter]//internal use
[]
[Misnamed GPS Occupations Report]//TT->Misnamed GPS Occupation Report Options window->tool tip
[]
[MLM]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[DADB]
[mm]//Process properties dialog (TLink spec.); Compute Coordinates page; field EDM  measurment unit mm|measurement unit, displayed in Custom Antenna list and Custom Antenns Properties
[mm]
[mm GPS]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[mm GPS]
[mm.]//TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument list->EDM column->measurment units
[mm.]
[mmHg]//TLink; Resect Export, Subfield name
[mmHg]
[Modified]//TTools and TLink; Import from device
[Yenilendi]
[Module]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->column name
[Modül]
[Modules]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->field name
[Modüller]
[Modules included: ]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->for internal use
[Modülleri içerir:]
[More...]//TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Origin Point list box->list box item|TTools and TLink; tree node, for example when we set curremt projectiom system|TTools and TLink; tree node, for example when we set curremt projectiom system
[Diğer...]
[Move]//for internal use only
[Oynat]
[Move Down]//TTools->Export->Cut Sheet  user-defined format->button|TTools and TLink->Export files and Convert File->Custom format properties->button|TTools and TLink->Tabular View->Options->button|TT->Report Configuration->button name
[Aşağı İndir]
[Move here]//Drag'n'drop menu item
[Burada oynat]
[Move horizontal element(s)]//Undo action name
[Yatay oynatma eleman(ları)]
[Move offset(s)]//Undo action name
[Oynatma ofset(leri)]
[Move Up]//TTools->Export->Cut Sheet  user-defined format->button|TTools and TLink->Export files and Convert File->Custom format properties->button|TTools and TLink->Tabular View->Options->button|TT->Report Configuration->button name
[Yukarı Kaldır]
[Move vertical element(s)]//Undo action name
[Düşey oynatma eleman(ları)]
[Move X-Section template(s)]//Undo action name
[]
[Move X-Section(s)]//Undo action name
[]
[MrSID Background Image File]//for internal use only
[MrSID Arkaplan Resim Dosyası]
[MrSID files]//TTools->Map View options->Browse->Open dialog->Format name
[MrSID dosyaları]
[ms.]//Ttools and Tlink->GPS Time dialogs->time units
[ms.]
[MULTI Data File]//for internal use only
[ÇOKLU Data Dosyası]
[MultiBS computation on station %s failed]//TLink->Compute Coordinates->message
[ÇokluDN isyasondaki hesaplama %s başarısız]
[Multiple]//multiple choice in style combo boxes (color etc)
[Çoklu]
[Multiple Observations (thick line)]//TTools->Map View->Legend window->line type
[]
[MXMOSS Filter]//TTools->Export->Format name
[]
[MXMOSS Points]//TTools->Export->Format name
[MXMOSS Noktaları]
[MXMOSS Roads]//TTools->Export->Format name
[]
[MXMOSS TS Obs]//TTools->Export->Format name
[]
[MXMOSS X-Section Templates]//TTools->Export->Format name
[]
[My Computer]//TLink->Exporting Files to TPS Controllers or CE-based Total Station->Export to Device->left panel
[Bilgisayarım]
[N]//TTools; CoGo; Intersection|TTools and TLink->Tabular View, Latituide, part of BLH coordinate value (insted of +)|TTools and TLink->Tabular View, Longituide, part of coordinate value (insted of -)|TTools; part of coordinate value on axis|TTools; part of coordinate value on axis|TTools and TLink->Tabular View, Longituide, part of coordinate value (insted of -)|not used
[X]
[N Residual]//TTools; TLink; Localization; Properties; field name
[X Farkı]
[Name]//properties for Surface; column name in Surface tab and in options|TTools; Adjustment; Column name|TTools->CoGo;Inv PTL|column name|TTools; Tlink; -> Job Configuration (Configuration)->Coordinate Systems ->field Name in the lists for geoobjects (geoids, datums and etc.)and Properties dialogs for geoobjects.|TTools->Occupation view->Split GPS Occupations dialog->field name|TTools->thumbnail/stereopair view options->Labels tab->Check box|TTools and TLink->Device properties dialog->field name|TTools->Map View options and Cad View options->Labels tab->Check box|for internal use only|Resolve Duplicate Points dialog|TT->Loop Closure Report Options window->field name|TT->Repeated Observations Report list->column name|TTools->Report->report Configuration->Project Report Options->field name|TTools; Adjustment Report Options, field name|TT->Report->Report Configuration->TS Obs report options->field name|TT->Report->Report Configuration->Cut Sheet Report->Options->field name|internal string|TT->Point summary Report Options->field name|TTools->DL Obs Report -> Options dialog -> Field name|(select two or more points on MapView window)->(click right button of mouse)->dialog.|TT->Tool Bar->Select->Select Points->field name|TT->Custom TS Instrument list->column name and Properties for Instrument->General tab->field name|TTools->File->Remote users->add group->prop. name|TT->Localization summary Report Options->field name
[İsim]
[Name can not be empty]//TTools; TLink; Datum Transformation; message box while saving parameters
[İsim boş olamaz]
[Name cannot be changed]//error message
[İsim değiştirilemiyor]
[Name is too long]//error message
[İsim çok uzun]
[Name must be unique]//error message
[İsim tek olmalıdır]
[Name of Submitting Organization]//TLink; GPSDataTransfer Export Options, Organization input field name
[Kuruluş Göndermenin İsmi]
[Name#$Point]//TTools and TLink->Object name (Point Properties dialog)
[Nokta İsmi]
[Name:]//TTools; TLink; Datum Transformation dialog; Datum parameter name
[İsim:]
[Names List is empty]
[İsim Listesi Boş]
[Narrow Lane]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Narrow Lane]
[NarrowLane]//TT->Residiul view window->legend window
[NarrowLane]
[Nav Distance from Point (m.)]//TT->Misnamed GPS Occupation Report->column name
[]
[Need Update]//TTools, properties for Surface
[]
[Negative distance]
[]
[NEH]//TT and TL->in advanced import/export options, convertation and open file->Coordiane order(for example SHP files)
[XYZ]
[NEpoch]//TTools->Occupation view->Split GPS Occupations dialog->field name
[]
[Network is weakly linked by ]//TTools;  error message under Adjustment
[]
[NEU]//not used
[]
[New]//TTools; Customize toolbars window; Toolbars Page; button mame
[Yeni]
[New Attribute]//TTools; Codes; Pop-up menu command
[Yeni Öznitelik]
[New Code]//TTools; Codes; text in the column Code when new code is created
[Yeni Kod]
[New Custom Antenna]
[Yeni Özel Anten]
[New Custom Camera]//TTools and TLink->New Custom Camera dialog name
[Yeni Özel Kamera]
[New Custom Datum]//TT and TL->New Custom Datum window name
[Yeni Özel Datum]
[New Custom Projection]//TT and TL->New Custom Projection window name
[Yeni Özel Projeksiyon]
[New Custom TS Instrument]//TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument->Add->window caption
[Yeni Özel TS Cihazı]
[New Datum]//not used
[]
[New Folder]//create new folder
[Yeni Klasör]
[New Group...]//TTools->File->Remote users->add user->button
[Yeni Grup...]
[New Intersect Point]//TTools; CoGo; Intersection
[]
[New Inverse]//TTools->CoGo; Inverse
[]
[New InvPTL]//TTools->CoGo;Inv PTL
[]
[New job]//TT->Startup dialog->button name
[Yeni İş]
[New Layer]//TTools -> Menu Bar -> View -> Layers -> Layers window -> Pop-up menu item Add Layer ->default new layer name
[]
[New Name is Invalid]//TTools->CoGo; PointInDirection, message
[]
[New Point in Direction]//TTools->CoGo; PointInDirection
[]
[New Projection]//not used
[]
[New report]//TT->Report Configuration->button name
[]
[New toolbar]//TTools; Customize toolbars window; Toolbars Page; New Toolbar dialog; caption
[]
[New Traverse Point]//TTools->CoGo->Traverse
[]
[New User...]//TTools->File->Remote users->add group->button
[]
[Next]//TLink->Compute Coordinates->Backsight dialog->button name|button name
[İleri]
[Next >>]//TTools and TLink->Export to Device and Import from Device->button Next
[İleri >>]
[Next>>]
[]
[NGS Antenna]//TTools, TLink; - >  properties dialog; Caption
[NGS Anten]
[NGS Antenna files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[NGS Anten dosyları]
[NGS Antenna Filter]
[]
[NGS Datasheet]//TTools; Import and Export from files; format name; TLink->Convert files->format name
[NGS Veridökümanı]
[NGS Name]//TTools and TLink ->GPS Occupations properties->Antenna Page->Custom Antennas List->Properties for Antenna->Page General->field name
[NGS İsmi]
[Niell]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[NIreland Geoid Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[Nİrlanda Jeoid Dosyaları]
[No]//TLink->Compute Coordinates->Scale factor dialog(for TS measurments)->button name|TTools; TLink; Localization window; Properties; field Use; field content
[Hayır]
[No Adjusted Subnetworks]//TTools; Adjustment; diagnistic message
[]
[No Azimuth Condition]//TTools;  error message under Adjustment
[]
[No Azimuth Condition, No Horizontal Control]//TTools;  error message under Adjustment
[]
[No Azimuth Condition, No Vertical and Horizontal Control]//TTools;  error message under Adjustment
[]
[No Azimuth Condition, No Vetrical Control]//TTools;  error message under Adjustment
[]
[No Backsight on station %s]//diagnostic message during Adjustment and Compute coordinate
[]
[No data for Adjustment. Number Processed observations = %d, points = %d]//TTools;  error message under Adjustment
[]
[No data in file %1]//error message
[]
[No ephemeris]//error message during Quality Control
[]
[No Horizontal Control]//TTools;  error message under Adjustment
[]
[No last Direction]//diagnostic message during Adjustment and Compute coordinate
[]
[No Localization]
[]
[No more Codes allowed]//message box
[]
[No nodes matched query (CountParser)]//for internal use only log message
[]
[No to all]//TLink->Compute Coordinates->Scale factor dialog(for TS measurments)->button name
[Hepsine Hayır]
[No Vertical and Horizontal Control]//TTools;  error message under Adjustment
[]
[No Vertical Control]//TTools;  error message under Adjustment
[]
[None]//Process Properties dialog(TLink spec.), page Compute Coordinates;  List box Adjustment type|combo box name|TTools; Tlink; Text in the Status Bar when current projection is not set|TTools; Tlink; ->Job Configuration->Coordinate Systems -> Projection list box; text or  Convert File; -> Projection list box; text|TTools and TLink ->GPS Occupation properties ->Antenna Tab->Antenna Type list box->possible value|detection type in thumbnail/stereopair view options|TT and TL->in advanced import/export options, convertation and open file->Coordinate System->value|TT and TL->Projection name(while job configurations conflict, for example during job import)
[None]
[Norm.Residual]//TTools; Adjustment; Column name
[]
[Norm.Residual E]//TTools; Adjustment; Column name
[]
[Norm.Residual H]//TTools; Adjustment; Column name
[]
[Norm.Residual N]//TTools; Adjustment; Column name  
[]
[Norm.Residuals]//TTools; Adjustment; Column name
[]
[Normal equations are not resolved: bad Parameter ]//TTools; error message under Adjustment
[]
[Normal equations are not resolved: bad Point ]//TTools;  error message under Adjustment
[]
[Normal equations are not resolved: determinant is 0]//TTools;  error message under Adjustment
[]
[Normal equations are not resolved: not enough conditions for Parameter ]//TTools;  error message under Adjustment
[]
[Normal equations are not resolved: not enough conditions for Point ]//TTools;  error message under Adjustment
[]
[North]//TLink; Resect Export, Header Field name|for internal use only|TT->3D View->left-bottom part of the window->axis name
[Kuzey]
[North Lat]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Kuzey Enl]
[North0]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Kuzey0]
[Northing]//TTools and TLink->Export files and Convert File->Custom format properties->for Grid and Ground systems field in the left panel|TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name|not used|TTools->Map View and Cad View->axis name in Ground and Grid system|TT->Roads tab->Horz. element->right panel->Properties->field name and Horz. element->Graphic View->axis name
[Yukarı]
[Northing Offset]//TTools; TLink ->Job Configuration->Coordinate Systems; Grid to Ground window -> field name; or Convert file dialog -> Grid to Ground
[Yukarı Ofset]
[Northing,Easting,Height]//TLink->Open TS Raw Data Filesand TTools Import->list box Coordinate order->possible value
[Sağa,Yukarı,Yükseklik]
[Norwegian Geoid Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[Norveç Jeoid Dosyaları]
[Not a valid choice]//error message
[Geçerli bir seçim değil]
[Not a valid JFF file %1]//error message
[Geçerli bir JFF dosyası değil %1]
[Not a valid JFF file %1 signature]//error message
[]
[Not a valid JFF file %1 version]//error message
[]
[Not Adjusted]//TTools; DL Obs Properties dialog; Adjustment Page; field Adjustment Status; field text|TTools and TLink->GPS Obs Properties->Adjust Page->field Adjustment Status->possible value|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->Adjustment Status list box->value
[Dengelenemedi]
[Not all tasks have intersections]
[]
[Not Allowed]//TTools; DL Obs Properties dialog; Adjustment Page; list box AutoReject; list box text|TTools and TLink->GPS Obs Properties->Adjust Page->list box AutoReject->possible value|TT->TS Obs tab->Properties for TS Obs->Adjustment tab->AutoReject list box->value
[]
[Not allowed by license]//log error message
[]
[Not an Rinex file]//log message
[]
[Not enough HORZ Controls]//TTools; Adjustment; diagnistic message
[]
[Not processed]//TTools and TLink->GPS Obs Properties ->Method, possible value
[Proses yapılamadı]
[Not sended]//Msg status
[Gönderilemedi]
[Not used]//TT (while job configurations conflict, for example during job import)->Override Job Configuration window->text, if Ground to Grid parameters not used
[]
[Note]//TTools, TLink; Tab View; DL tab; field # |TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools; -> Job Configuration->Coordinate Systems ->field Note|TTools and TLink -> Tabular View ->GPS Occupations Properties->Antenna tab-> Custom Antennas list -> Column name and etc.|TTools and TLink->Images tab->Options->Show tab->check box name|TTools and TLink->Device properties dialog->field name|TTools and TLink->Object comment->Point Properties dialog->Page General and etc.|TT->Tool Bar->Select->Select Points->field name|TL->Custom TS Instrument List->column name;TT and TL->Ts OBS tab->column name and TSObs properties->field name;Tape Dimensions tab->column name;TL->File Properties->Session tab->field name
[Not]
[Note: a point is marked red if it did not pass QC test]//TTools->Map View->Legend window
[]
[ns.]//Ttools and Tlink->GPS Time dialogs->time units
[]
[Number of control codes can not be greater then number of codes]//message box
[]
[Number of Degrees of Freedom is 0]//TTools;  error message under Adjustment
[]
[Number of Points]//properties for Surface; column name in Surface tab and in options
[]
[Number of Triangles]//properties for Surface; column name in Surface tab and in options
[]
[Numeric Attribute]//not used
[]
[O Data File]//not used
[]
[O Export to ]//log message
[]
[O files]//TTools;  Export; Format name;
[]
[O&ptions\\&CAD View...\nOpen CAD View Options Dialog\nCAD View Options]//TL->Tool Bar->View->Options->Cad View|TT->Tool Bar->View->CAD View Options
[S&eçenekler\\CAD Ekranı...\\nCAD Ekranı Seçenekler Menüsünü Aç\nCAD Seçeneklerine Bak]
[O&ptions\\&Images View...\nOpen Images View Options Dialog\nImages View Options]//TT->Tool Bar->View->Images View Options
[]
[O&ptions\\&Map View...\nOpen Map View Options Dialog\nMap View Options]//TT->Tool Bar->View->Options->Map View Options
[]
[O&ptions\\&Occupation View...\nOpen Occupation View Options Dialog\nOccupation View Options]//TT->Tool Bar->View->Occupation View Options
[]
[O&ptions\\&Stereopair View...\nOpen Stereopair View Options Dialog\nStereopair View Options]//TT->Tool Bar->View->Stereopair View Options
[]
[O&ptions\\&Tabular View...\nOpen Tabular View Options Dialog\nTabular View Options]//TL->Tool Bar->View->Options->Tabular View|TT->Tool Bar->View->Tabular View Options
[S&eçenekler\\&Çizelgelere Bak..\Çizelge Seçenek Menüsünü Aç\nÇizelge Seçeneklerine Bak]
[Object Folder]//for internal use only
[]
[Object is in use and cannot be modified]//error message
[]
[Object with this name already exists]//error message
[]
[Objects]//not used
[]
[Objects must be removed]//error message
[]
[Oblique Mercator]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[]
[Observable]
[]
[Observation]//TTools, TLink; DL Obs Properties dialog; Observation Page, Tab name|TTools and TLink ->GPS Obs properties-> page name|TT and TL->Properties for TS Obs->page name
[Gözlemler]
[Observation disagrees by more then 10m with rover coordinates. Rover point is probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Observation disagrees with rover coordinates. Rover point is probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Observation time mode]//not used
[]
[Observation\\Exclude]//TT and TL-> Properties for TSObs->Observation tab->group box name
[]
[Observations GPS PostProcessed Kinematic Failed Obs Filter\nObservations GPS PostProcessed Kinematic Obs Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Kinematic Obs Disabled Filter\nObservations GPS PostProcessed Kinematic Obs Disabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Kinematic Obs Potential Filter\nObservations GPS PostProcessed Kinematic Obs Potential Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Kinematic Obs Pricessed Filter\nObservations GPS PostProcessed Kinematic Obs Pricessed Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Kinematic Occupations Filter\nObservations GPS PostProcessed Kinematic Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Kinematic Points Filter\nObservations GPS PostProcessed Kinematic Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Kinematic Unprocessed Points Filter\nObservations GPS PostProcessed Kinematic Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Static Obs Disabled Filter\nObservations GPS PostProcessed Static Obs Disabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Static Obs Potential Filter\nObservations GPS PostProcessed Static Obs Potential Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Static Obs Processed Filter\nObservations GPS PostProcessed Static Obs Processed Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Static Occupations Filter\nObservations GPS PostProcessed Static Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Static Points Filter\nObservations GPS PostProcessed Static Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Failed Obss Filter\nObservations GPS PostProcessed Go Obs Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Obs Disabled Filter\nObservations GPS PostProcessed Go Obs Disabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Obs Disabled Filter\nObservations GPS PostProcessed Stop Obs Disabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Obs Potential Filter\nObservations GPS PostProcessed Go Obs Potential Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Obs Potential Filter\nObservations GPS PostProcessed Stop Obs Potential Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Obs Processed Filter\nObservations GPS PostProcessed Go Obs Processed Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Obs Processed Filter\nObservations GPS PostProcessed Stop Obs Processed Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Occupations Filter\nObservations GPS PostProcessed Go Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Occupations Filter\nObservations GPS PostProcessed Stop Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Points Filter\nObservations GPS PostProcessed Go Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Points Filter\nObservations GPS PostProcessed Stop Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS PostProcessed Stop and go Unprocessed Points Filter\nObservations GPS PostProcessed Go Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Autotopo Obs Disabled Filter\nObservations GPS RTK Autotopo Obs Disabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Autotopo Obs Enabled Filter\nObservations GPS RTK Autotopo Obs Enabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Autotopo Occupations Filter\nObservations GPS RTK Autotopo Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Autotopo Points Filter\nObservations GPS RTK Autotopo Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Bases Occupations Filter\nObservations GPS RTK Bases Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Bases Points Filter\nObservations GPS RTK Bases Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Topo Obs Disabled Filter\nObservations GPS RTK Topo Obs Disabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Topo Obs Enabled Filter\nObservations GPS RTK Topo Obs Enabled Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Topo Occupations Filter\nObservations GPS RTK Topo Occupations Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations GPS RTK Topo Points Filter\nObservations GPS RTK Topo Points Filter]//TTools; Filters window; tooltip; for internal use only
[]
[Observations with Big Misclosure]//TTools; Adjustment; Table header
[]
[Observations\\DGPS\\]//TTools; Filters window
[]
[Observations\\Digital Level\\Sideshots]//TTools, Filters
[]
[Observations\\Digital Level\\Traverse points]//TTools, Filters
[]
[Observations\\GPS PostProcessed\\]//TTools; Filters window
[]
[Observations\\GPS RTK\\]//TTools; Filters window
[]
[Observations\\Tape Obs]//TT->View->Filters->By Type
[]
[Observations\\Total Station\\Backsights]//TT->View->Filters->By Type
[]
[Observations\\Total Station\\Disabled]//TT->View->Filters->By Type  
[]
[Observations\\Total Station\\Sideshots]//TT->View->Filters->By Type
[]
[Observations\\Total Station\\Stations]//TT->View->Filters->By Type
[]
[Occ]
[]
[Occ&upation View]//TT->Tool Bar->View->Menu item
[]
[Occ.point name]//TLink; Resect Export, Header Field name
[Oturum nokta ismi]
[Occ.Std.deviation]//TLink; Resect Export, Header Field name
[]
[Occupation]//TTools, TLink; DL Occupation Properties dialog; field name|TT->Occupation View Options window->Occupation diagram->comment under cursor
[Oturum]
[Occupation %s, SV G%d]//message
[]
[Occupation %s, SV R%d]//message
[]
[Occupation Filtering...]//log message
[]
[Occupation is more than 10m away from point. It is probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Occupation View]//TT->Window caption
[]
[Occupation View Item]//for internal use only
[]
[Occupation View Item Options]
[]
[Occupation View Options]//TT->Occupation View window caption|TT->View->Options->Occupation view->window caption
[]
[Occupation: ]//log message
[]
[Occupations]//TT->Occupation View window->Legend window
[]
[Occupation's autonomous position is too far away from point. It is probably misnamed]//TT->TabView->Quality Control tab->message
[]
[OFF]//written on diagram's item in legend when it is hidden
[]
[Offline]
[]
[Offset]//TTools and TLink ->GPS Occupations properties-> page name|not used|TT->Point tab->Properties for Point->Offset tab->tab name|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item|TT and TL->Properties for TS Obs->page name
[Ofset]
[Offset Across]//TTools; CoGo; Inverse PTL, Field name|TTools and TLink->Export files and Convert File->TSRaw custom format properties->name of the first group of fields|TT->Point tab->Properties for Point->Offset tab->field name|TT and TL->Properties for TS Obs->Offset tab->field name
[Across Ofset]
[Offset Along]//TTools; CoGo; Inverse PTL, Field name|TTools and TLink->Export files and Convert File->TSRaw custom format properties->name of the first group of fields|TT and TL->Properties for TS Obs->Offset tab->field name
[İleri Ofset]
[Offset dHt]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->name of the first group of fields|TT and TL->Properties for TS Obs->Offset tab->field name
[Ofset dZ]
[Offset Direction]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[]
[Offset Dist]//TT->Point tab->Properties for Point->Offset tab->field name
[Mesf.Ofseti]
[Offset Distance]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Offset H]//TTools; CoGo; Inverse PTL, Field name
[]
[Offset Ht]//TT->Point tab->Properties for Point->Offset tab->field name
[Yksk.Ofseti]
[Offset Type]//TT and TL->Properties for TS Obs->Offset tab->field name
[Ofset Tipi]
[Offset1]//TTools->CoGo; Intersect
[]
[Offset2]//TTools->CoGo; Intersect
[]
[Offsets: ]//TTools->CoGo;Intersection
[]
[OK]//TTools; Adjustment; Button name|TTools->CoGo; Intersect + PointInDirection + ...|button name|TTools->Export->Cut Sheet  user-defined format->button|TTools and TLink->Export files and Convert File->Custom format properties->button    |Ttools->Map View->Options>MrSid Background file activation->Password window->button name|OK Button|OK button|TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Compute Azimuth->button name|TTools->Occupation view->Merge GPS Occupations dialog and Split GPS Occupations dialog->button name|button name|button name|TT->Tool Bar->Select->Select Points, GPS Obs, TS Obs and etc.->button name|TL->button name|TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->Code status->value|TT->Grid to Ground dialog (from Job configuration for example)->button name|Ttools->Map View->Options>MrSid Background file activation->Password window->button name|TTools->File->Remote users->add group->button
[TAMAM]
[One of the modules was disabled (dongle removed)!!\n TopconTools will be closed.]//TT->MessageBox (warning on remove dongle)
[]
[One of the modules was enabled (dongle inserted)!!\n Demo Mode will be ended and TopconTools will be closed.]//TT->MessageBox (warning on insert dongle)
[]
[Online]
[]
[Only TS Points in Ground System will be Adjusted]//TTools; message Adjustment
[]
[Open]//TTools;TLink;log message|Open file dialog name|dialog name|Receive file dlg->Button
[Aç]
[Open a job]//TT->Sturtup dialog->button name
[İş Aç]
[Open EGM Coeff Correction File]//TTools, TLink; for internal use only
[]
[Open file to convert]//not used|not used
[]
[Open Files after Import]//TTools and TLink->Importing Files from Device->Check box
[Yüklemeden sonra Dosyaları Aç]
[Open folder]//Receive file dlg->Button
[]
[Open for Convert]//TLink->Convert File->Open for Convert file dialog caption
[Dönüştürmek için Aç]
[Open Geoid Canadian95 pasport file( h*.slv)]//TTools, TLink; for internal use only
[Kanada95 Geoid pasport dosyası aç( h*.slv)]
[Open Image View on the image\nImage View]//TTools->Menu Bar->View->hint text in the Status Bar
[]
[Open job]//TT->Startup dialog->button name
[]
[Open Orientation View\nOrientation View]//hint for view window/command for stereopairs
[]
[Open Plot\nRawData Plot]
[]
[Open Residual View of vector\nResidual View]//TT->Residiul view window->hint text in the Status Bar
[]
[Open Stereo View\nStereo View]//hint for view window/command for stereopairs
[]
[Open Stereopair View\nStereopair View]//hint for view window/command for stereopairs
[]
[Opening file %s. You can press Esc to break]//not used
[]
[Operation canceled]//error message
[Uygulama iptal edildi]
[Operation in progress, can not close window.]//message box
[Uygulama çalışıyor, pencereyi kapatmayın.]
[Option\tUse\tin current Job\tUse\tin imported Job]//TT (while job configurations conflict, for example during job import)->Override Job Configuration window->dialog elements names
[]
[Options]//TTools->properties for Surface|TTools->CoGo; Options|TTools, TLink; DL Obs Tab; Pop-up menu command|not used|TTools; Linework Tab; Options dialog;|TTools and TLink -> Tabular View ->GPS Occupations tab->Options dialog->capture|orientation points|not used|TTools and TLink->Tab View->Pop-up menu item Options and Options dialog caption|not used|TT->X-Section Templates tab->options dialog|TSObs tab(TT and TL) and Tape Dimensions tab (TT)->Options window name
[Seçenekler]
[Options..]//TT->Loop Closures dialog
[Seçenekler..]
[Options...]
[Seçenekler..]
[Options\\Avoid creating triangles]//TTools->properties for Surface
[]
[Orbit]//TTools and TLink -TabView->GPSObs Tab-> Orbit column name
[Orbit]
[Order]//TT - column and property name in Linework tab|TT->Roads tab->Properties for road vertical elemrnt, road horizontal element, X-section->spin edit name
[Sıra]
[Order and class of survey]//TLink; BlueBook Export Options, Order and class of survey input field name
[]
[Orientation]//TLink; Resect Export, Header Field name
[Yönlendirme]
[Orientation Obs]//orientation points
[Yönlendime Bkş]
[Orientation Obs\nOrientation Obs]//orientation points
[Yönlendime Bkş\nYönlendime Bkş]
[Orientation View]//not used|not used
[]
[Origin Easting]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Sağa Merkez]
[Origin Ell. H]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Elp.H Merkez]
[Origin H]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Orgin H]
[Origin Lat]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Orgin Enl]
[Origin Lon]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Orgin Byl]
[Origin Northing]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[Yukarı Merkez]
[Origin Point]//TTools; TLink ->Job Configuration->Coordinate Systems -> Grid to Ground window ->Ground Origin ->field name
[Nokta Merkez]
[Original Name]//not used|TTools and TLink -> Tabular View ->GPS Occupations Tab  -> column name|for internal use
[Orjinal İsim]
[Original name]//TT->Tool Bar->Select->Select GPS Occup.->field name
[Orjinal isim]
[Orthometric Height]//TLink->Open Coordinate files and TTools Import->Check box name
[Ortametrik Yükseklik]
[OrtoHeight]//TTools->CoGo; GoPointInDirection
[]
[Other]//for internal use only|not used
[Diğeri]
[Other fields]//for internal use only|for internal use only
[Diğer alanlar]
[Outgoing]//Direction
[]
[Outlier]//internal use
[]
[Outlier by Distance]//TTools; Adjustment; diagnostic message for QC
[]
[Outlier by Height]//TTools; Adjustment; diagnostic message for QC
[]
[Outlier by Horizontal Angle]//TTools; Adjustment; diagnostic message for QC
[]
[Outlier by Vertical Angle]//TTools; Adjustment; diagnostic message for QC
[]
[Outliers and Rejected QC filter\nOutliers and Rejected QC filter]//internal use
[]
[Outline]//not used
[]
[Override code plotting styles]//TTools, TLink->line properties
[]
[Override existing]//TTools->Job Configuration->Save->Backup files from devices->possible value
[]
[Override Job Configuration]//TT (while job configurations conflict, for example during job import)->window caption
[]
[Overwite Background Image(s)]
[Arkaplan Resim(leri) Üzerine Yaz]
[P&age Setup...\nChange the printing options\nPage Setup]//TL->Tool Bar->File->Page Setup|TT->Tool Bar->Job->Page Setup
[S&ayfa Ayarları...\nYazıcı ayarlarını değiştir\nSayfa Ayarları]
[P&an mode]
[P&an mod]
[P&rint Setup...]
[Y&azıcı Ayarları...]
[Pa&n Mode\nToggle pan mode on or off\nPan Mode]//TL->Tool Bar->Edit->Pan Mode|TT->Tool Bar->Edit->Pan Mode
[Pa&n Modu\nPan modu açık yada kapalı\nPan Modu]
[Pan mode]
[Pan modu]
[Parabola]//TT->Roads tab->Vertical element->type of the element
[]
[Parabola Long Section]//TT->Roads tab->Vertical element->type of the element
[]
[Parameter]//not used
[]
[Parameters]//TTools; TLink ->Job Configuration->Coordinate Systems; Grid to Ground window -> radio button  name; or Convert file dialog -> Grid to Ground|TTools and TLink->New Custom Antenna->Page name|TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument->Properties for Instrument->tab name|TT->Grid to Ground dialog (from Job configuration for example)->radio button name
[Parametreler]
[Parameters\\Scale Factor]//for internal use only
[Parametreler\\Ölçek Faktörü]
[Parsing file]//not used
[]
[Partial]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Partial]
[Pass Status]//not used
[]
[Passed]//not used
[]
[Password]//Ttools->Map View->Options>MrSid Background file activation->Password Window caption|Ttools->Map View->Options>MrSid Background file activation->Password Window caption|TTools->File->Remote users->add user->prop. name
[]
[Paste]//TL->ToolBar->Edit->Paste|TT->ToolBar->Edit->Paste
[Yapıştır]
[Paste Button Image]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[Paste horizontal element(s)]//Undo action name
[]
[Paste offset(s)]//Undo action name
[]
[Paste vertical element(s)]//Undo action name
[]
[Paste X-Section template(s)]//Undo action name
[]
[Paste X-Section(s)]//Undo action name
[]
[Path]//TTools; TLink -> Job Configuration (Configuration) -> Geoid list -> column name|Ttools->view->Background images->left panel (Available images)->field name
[Yol]
[Pb]//units of files size - send file dialog
[]
[PCV]//TTools and TLink->GPS Occupations ->Antenna Type Properies->Page name
[PCV]
[PCV, GLONASS L1]//TTools and TLink->GPS Occupations ->Antenna Type Properies->Page PSV->group name
[PCV, GLONASS L1]
[PCV, GLONASS L2]//TTools and TLink->GPS Occupations ->Antenna Type Properies->Page PSV->group name
[PCV, GLONASS L2]
[PCV, GPS L1]//TTools and TLink->GPS Occupations ->Antenna Type Properies->Page PSV->group name
[PCV, GPS L1]
[PCV, GPS L2]//TTools and TLink->GPS Occupations ->Antenna Type Properies->Page PSV->group name
[PCV, GPS L2]
[PDOP]//TTools and TLink->GPS Obs Tab->Properties->field name
[PDOP]
[Percent (%)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[Perform a localization\nPerform a localization]//TTools; TLink; ToolBar; Process; Localization; hint text in the Status Bar
[Lokalizasyon Oluştur\nLokalizasyon Oluştur]
[Performs a datum 7 parameters localization\nPerforms a  datum 7 parameters localization]//TTools; TLink; ToolBar; Process; Datum Transformation; hint text in the Status Bar
[Datum 7 parametre değerlerini oluştur\nDatum 7 parametre değerlerini oluştur]
[Phase Diff]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Faz Farkı]
[Photo Note Number:]//TT and TL->Tab View->Point properties->Photo Notes tab->list box name
[Foto Not Numarası:]
[Photo Notes]//TT and TL ->PointProperties->tab name
[Foto Notları]
[Photo notes]//TT ->in advanced import/export options->Phote notes check box name(for example export for Shape files)
[Foto notları]
[Photonotes]
[FotoNotları]
[Picture Height]//TT->Graphic View report(Map View Item,CAD View Item,Occupation View Item,Residual View Item)->Options window->spin edit name
[]
[Picture Width]//TT->Graphic View report(Map View Item,CAD View Item,Occupation View Item,Residual View Item)->Options window->spin edit name
[]
[Plane]//TTools; Adjustment Report, Output use|TT and TL->Properties for TS Obs->General tab->Type list box->value
[]
[Please fill following fields.]//TLink; GPSDataTransfer Export Options, Name of input dialog|TLink; BlueBook Export Options, Name of input dialog
[]
[Please, install DirectX 9.0 to use this feature.\n\nYou can download the latest version at http://www.microsoft.com/windows/Directx/]//www.microsoft.com/windows/Directx/" //TT->3D View->error message
[]
[Plot View]
[]
[Plots]
[]
[Plotting styles]//TTools->Linework->Properties of Line->Page name
[Çizgi Tipleri]
[Point]//TTools->CoGo;Inv PTL|TTools, TLink; Tab View; DL tab; field name|Ttools and TLink->Images tab->Proprties for image->list box nane|for internal use(feature)|TT->Roads tab->for internal use
[Nokta]
[Point [%s:%d]: x=%.3f y=%.3f z=%.3f]//log message
[]
[Point 1]//TT->Identical Points Report->column name
[]
[Point 2]//TT->Identical Points Report->column name
[]
[Point code]//TT->Tool Bar->Select->Select GPS Occup.->field name
[]
[Point Coordinates]//for internal use only
[Nokta Koordinatları]
[Point coordinates cannot be calculated. Please, try to measure the point again.]//message shown if user measured point on images incorrectly
[]
[Point coordinates cannot be calculated: camera positions are too close.]//message shown if camera positions are too close to each other
[]
[Point Coordinates List\nPoint Coordinates List]//for internal use only
[]
[Point does not have grid coordinates]//error message box
[]
[Point From]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink -> Tabular View ->GPS Obs Tab  -> column name|TT and TL->TSObs tab->right panel->column name;TT and TL->TSObs properties->field name
[Nokta dan]
[Point in Chain]//for internal use
[KM Noktası]
[Point in Direction]//TTools->CoGo;Point in Direction
[]
[Point In Direction]//TTools->CoGo; Options
[]
[Point In Direction Task Report]//TTools; CoGo; Point In Direction, report name              
[]
[Point In Direction...]//TTools; Menu Bar; COGO; menu item Point In Direction...
[]
[Point is already in the line]//error message
[]
[Point Name]//not used|TTools and TLink -> Tabular View ->GPS Occupations Tab, column name|TT and TL->Properties for TS Occupation->list box name
[Nokta İsmi]
[Point name]//TT->Tool Bar->Select->Select GPS Occup, TS Occup.->field name
[Nokta ismi]
[Point name can not contain special symbols]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[]
[Point Number]//TTools and TLink->Export files and Convert File->Custom format properties->field in the right panel
[Nokta Numarası]
[Point Precisions]//for internal use only
[Nokta Hassasiyetler]
[Point Report Options]//for internal use only
[Nokta Rapor Opsiyonları]
[Point Standard Deviations]//TT->Job Configuration->Quality Control->Automatic Tests->check box name
[]
[Point Standard Deviations QC filter\nPoint Standard Deviations Quality Control filter]//internal use
[]
[Point Summary Report]//TT->tooltip
[Nokta Özet Raporu]
[Point Symbol]//Ttools->attribute properies->
[Nokta Sembolü]
[Point To]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink -> Tabular View ->GPS Obs Tab  -> column name|TT and TL->TSObs tab->right panel->column name;TT and TL->TSObs properties->list box name;TT->Tape Demensions tab->column name
[Nokta ya]
[Point To Code]//for internal use only
[Kod dan Nokta ya]
[Point type]//TT->Tool Bar->Select->Select Points->list box name
[]
[Point type:]//coordinate order in advanced import/export options
[Nokta tipi:]
[Point(s) %s are absent]
[]
[Point(s) %s have no required coordinates]//TTools; Inverse; error message
[]
[Points]//TTools; Adjustment; diagnistic message|TTools->Menu bar->Edit->Add->Add Line|not used|TT->Occupation view window->axis name|TT->Residiul view window->axis name
[]
[Points Fixing by User]//Process Properties dialog, Tlink spec, Compute Coordinates page, field
[]
[Points in Direction]//TTools->CoGo;Point in Direction: Tab Name
[]
[Points in Direction\nView]//TTools->CoGo;Point in Direction: Hint
[]
[Points in the file:]//Resolve Duplicate Points dialog
[]
[Points in the project]//Resolve Duplicate Points dialog
[]
[Points List\nPoints List]//for internal use
[Nokta Listesi\nNokta Listesi]
[Points renaming]//TT and TL->Points tab->Pop-up menu item Rename Points->Points renaming window name
[Noktalara yeni isim ver]
[Points\\Adjusted points]///TT->Filters window->By Type tab->names of the nodes
[]
[Points\\COGO points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Control points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Design points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Disabled points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Event points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Image measured points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Manual points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Scan points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Stakeout points]//TT->Filters window->By Type tab->names of the nodes
[]
[Points\\Unknown points]//TT->Filters window->By Type tab->names of the nodes
[]
[PointsExport]
[]
[Port]
[Port]
[Position]
[]
[PostProcessed]//Name Of Vector Type   
[]
[PostProcessed Failed]//Name Of Vector Type
[]
[PostProcessing Options]//for internal use only
[]
[PostProcessing Options\\Use SVs]//for internal use only
[]
[Potential]//Name Of Vector Type          
[]
[PP]//TTools and TLink->GPS Obs Properties ->Method, possible value|name of module, in Autorizations dialog and in About
[PP]
[PP Code Diff]//TT->Process properties->GPS+Post Process tab (advanced module)
[PP Kod Farkı]
[PP Go]//TTools and TLink->GPS Obs Properties ->Method, possible value|Solution Name
[PP Git]
[PP Kin]//TTools and TLink->GPS Obs Properties ->Method, possible value
[PP Kin]
[PP Kinematic]//TTools->GPS Vectors Import|Solution Name
[PP Kinematik]
[PP Kinematic Horizontal Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name
[]
[PP Kinematic Precisions]//TT->Job Configuration->Quality Control->Automatic Tests tab->check box name
[]
[PP Kinematic Precisions QC filter\nPP Kinematic Precisions QC filter]//internal use
[]
[PP Kinematic Vertical Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name
[]
[PP L1 Only]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP L1&L2]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP L1&L2c]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP L1+L2]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP L1c]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP L1-L2]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP L2 Only]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP Static]//TTools->GPS Vectors Import|Solution Name
[]
[PP Static Horizontal Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name
[]
[PP Static Precisions]//TT->Job Configuration->Quality Control->Automatic Tests tab->check box name
[]
[PP Static Precisions QC filter\nPP Static Precisions QC filter]//internal use
[]
[PP Static Vertical Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name
[]
[PP Stop]//TTools and TLink->GPS Obs Properties ->Method, possible value|Solution Name
[PP Dur]
[PP VLBL]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PP Wide Lane]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[PPM]//TT->Custom TS Instrument list->column name
[]
[ppm]//Process properties dialog (TLink spec.); Compute Coordinates page; field EDM  measurment unit ppm |TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name, unit name
[ppm]
[Pr&operties...\nView Properties Dialog for the selected object(s)\nView properties]//TL->Tool Bar->Edit->Properties|TT->Tool Bar->Edit->Properties
[Öz&ellikler...\nVSeçilen obje(lerin)özelliklerine bak\nÖzelliklere bak]
[Pr&operties...\tCtrl+Enter]
[Ö&zellikler...\tCtrl+Enter]
[Precise]//TTools and TLink -TabView->GPSObs Tab-> possible value in the Orbit column
[]
[Precision of date is incorrect]//for internal use only log message
[]
[Precisions]//TTools(Job Configuration) and TLink(Configuration)->Display->Precisions tab name
[]
[Prefix can not contain special symbols]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[Önek özel semboller içermemelidir]
[Preliminary]//TTools; Adjustment; context name|not used
[]
[Preparing data for processing]//not used
[]
[Preprocessor not saved file]//not used
[]
[Press Esc to break]//not used??
[]
[Pressure]//TLink; Resect Export, Header Field name|for internal use only
[Basınç]
[Pressure: (mBar)]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Prev]//button name
[Geri]
[Previous]//TLink->Compute Coordinates->Backsight dialog->button name
[Geri Al]
[Principal Point, X]//camera property name
[]
[Principal Point, Y]//camera property name
[]
[Print]//Context menu item on history of messages dlg
[Yazdır]
[Print Pre&view]
[Baskı Ön&izleme]
[Print Pre&view\nDisplay full pages\nPrint Preview]//TL->Tool Bar->File->Print Preview|TT->Tool Bar->Job->Print Preview
[Baskı Ön&izleme\nTüm sayfaları göster\nBaskı Önizleme]
[PrismConstant]//for internal use      
[Prizma Sabitesi]
[Problem with job]//error message
[İş de problem var]
[Process]//log message
[İşleniyor]
[Process failed]//diagnostic message during Adjustment and Compute coordinate
[Proses başarısız]
[Process feature codes]//TTools->Job Configuration
[]
[Process from]//for internal use only
[dan proses]
[Process P&roperties...]
[Proses Ö&zellikleri]
[Process P&roperties...\nOpen Process Properties Dialog\nProcess Properties]//TL->Tool Bar->Process->Process Properties|TT->Tool Bar->Process->Process Properties
[Proses Ö&zellikleri...\nProses Özellikler Tablosunu Aç\nProses Özellikleri]
[Process properties]//TL->Tool Bar->Process->Process Properties|TT->Tool Bar->Process->Process Properties
[Proses özellikleri]
[Process to]//for internal use only
[ya Proses]
[Process/Adjustment\\Adjustment]//Process properties dialog (TTools spec.); Dialog Caption, Page Caption
[Proses/Dengeleme\\Dengeleme]
[Process/Compute Coordinates\\Compute Coordinates]//Process properties dialog (TLink spec.); Dialog Caption, Page Caption  
[Proses/Koordinatları Hesapla\\Koordinatları Hesapla]
[Process/GPS+ PostProcess\\Engine]//TT->Tool Bar->Process->GPS+ PostProcessing (advanced mode)
[]
[Process/GPS+ PostProcess\\General]//TT->Tool Bar->Process->GPS+ PostProcessing
[]
[Process/GPS+ PostProcess\\Troposphere]//TT->Tool Bar->Process->GPS+ PostProcessing (advanced mode)
[]
[Process/Linework\\Linework Processor]//TTools->Job Configuration
[]
[Process/TS Computations\\TS Computations]//Process properties dialog; Dialog Caption, Page Caption
[Proses/TS Hesaplamaları\\TS Hesaplamaları]
[Processed %d vectors from %d]//log message
[]
[Processed DGPS]//TTools->Map View->Legend window->line type
[]
[Processed PP]//TTools->Map View->Legend window->line type
[]
[Processed PP Kinematic]//TTools->Map View->Legend window->line type
[]
[Processing report: ]//TT->Report Configuration->text in the Status Bar while report is executed
[]
[Profile View]
[]
[Profile View\nProfile View]
[]
[Program is not licensed properly: license file is either absent, corrupt or from different program]//error message
[]
[Project Report]//TTools->Report->report Configuration->hint text (for internal use)
[]
[Project Report Options]//TTools->Report->report Configuration->Project Report Options name (for internal use)
[]
[Project Template]//TTools->Report->report Configuration->Project Report Options->template name
[]
[Projection]//TTools; ->Job Configuration->Coordinate Systems ->Projection Properties dialog-> caption|TTools->Job Configuration->Coordinate systems->Projection list box name
[Projeksiyon]
[Projection not selected]//error message
[Projeksiyon seçilmemiş]
[Projection not selected for some objects]//error message
[Bazı objeler için projeksiyon seçilmemiş]
[Projection Type]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box name
[Projeksiyon Tipi]
[Projection:]//TT and TL->in advanced import/export options, convertation and open file->list box name
[Projeksiyon:]
[Properties]//??? not used|TTools; Codes; dialog Properties|dialog Properties caption|TTools and TLink->Custom Antennas List->Properties dialog caption|dialog caption|TTools and TLink->Device properties dialog->caption|TTools and TLink->Menu Bar->Edit->Properies|TL->dialog name|TT->dialog name|TT->Custom TS Instrument list->column name and and Properties for Instrument->window caption|Caption of prop dlg
[]
[Properties of ]//for internal use only
[nın özellikleri]
[PTL]//TT and TL->Properties for TS Obs->Offset tab->Offset type->value
[DADB]
[PTL Offset]//TTools->Map View->Legend window->point type
[]
[QA/QC]//for internal use
[]
[QA/QC Options]//for internal use only
[]
[QAQC]//TTools->Map View options options->tab name|TTools->Occupation View options options->tab name
[]
[QAQC Filter Options]//internal use
[]
[QAQC Quality Filters]//TTools->Filters - dummy property name, may be hidden
[]
[QC fail Observations]//TTools; Adjustment; Table header
[]
[QC fail Points]//TTools; Adjustment; Table header
[]
[Quality]//TTools and TLink->GPS Obs Tab->Properties->Pade nane|for internal use
[]
[Quality Analysis and Quality Control]//for internal use
[Kalite Analzi ve Kalite Kontrol ]
[Quality Control]//TTools,DL Obs Properties dialog; Quality Control, Tab name|TT->TS Obs tab->Properties for TS Obs->tab name
[Kalite Kontrol]
[Quality control]//TTools and TLink->GPS Occupation properies and GPS Obs Properties->Page name|TT->Tab View->Quality control tab->tab name
[Kalite kontrol]
[Quality Control\\Automatic Tests]//TT->Job Configuration->Quality Control->tab name
[]
[Quality Control\\Compare Points]//TTools->Filters
[]
[Quality Control\\DL Obs Precisions]//TT->Job Configuration->Quality Control->tab name
[]
[Quality Control\\Float Solutions]//TTools->Filters
[]
[Quality Control\\GPS Obs Precisions]//TT->Job Configuration->Quality Control->tab name
[]
[Quality Control\\Identical Points]//TTools->Filters
[]
[Quality Control\\Loop Closure Precisions]//TT->Job Configuration->Quality Control->tab name
[]
[Quality Control\\Misnamed Autotopo Rovers]//TTools->Filters
[]
[Quality Control\\Misnamed GPS Occupations]//TTools->Filters
[]
[Quality Control\\Outliers and Rejected by Adjustment]//TTools->Filters
[]
[Quality Control\\Point Precisions]//TT->Job Configuration->Quality Control->tab name
[]
[Quality Control\\Point Standard Deviations]//TTools->Filters
[]
[Quality Control\\PP Kinematic Precisions]//TTools->Filters      
[]
[Quality Control\\PP Static Precisions]//TTools->Filters      
[]
[Quality Control\\RTK Precisions]//TTools->Filters
[]
[Quality Control\\TS Obs Precisions]//TT->Job Configuration->Quality Control->tab name
[]
[R ]
[]
[Radian]//TLink; Resect Export, Angular Unit Name
[Radyan]
[Radians]//TTools->Export(for internal use)|TTools->Job Configuration->Units->Angular Unit list box->possible value; TTools and TLink->Status Bar->list box for angular units
[]
[RadioParser: No radio elements found in pos %xh]//for internal use only log message
[]
[Radius]//TTools and TLink -> Tabular View ->GPS Occupations Properties ->Antenna Tab-> Custom Antennas List -> Properties for Antenna -> Page Parameters-> field name|TT->Roads tab->Horz. element->Properties->group box name
[Yarıçap]
[Raster]//Ttools->view->Background images->left panel (Available images)->Type field->content
[]
[RawData Plot]
[]
[RawData Plot Options]
[]
[Read history]//Conext menu item
[]
[Readed]//Msg status
[Okundu]
[Reading file]//text in the Status Bar during import
[Dosya okunuyor]
[Ready]//message in the Status Bar|TL->text in the Status Bar|TT->text in the Status Bar
[Hazır]
[Real Number]//TTools; Codes; New Attribute; Pop-up menu command|TTools->Codes->New Attribute->possible attribuite type
[]
[Receiver]//TTools and TLink->GPS Obs tab->column name
[Alıcı]
[Receiver Type]//TTools and TLink->GPS Obs tab->column name
[Alıcı Tipi]
[Receivers]//TT->Occupation view window->axis name|TT->Residiul view window->axis name
[Alıcılar]
[Receiving file]//Receive dlg caption
[Dosya alınıyor]
[Recent File]
[]
[Recent File\nOpen this file\nOpen this file]//TL->Tool Bar->File->Text in the Status Bar while opening the recent file
[]
[Recent File\nOpen this job\nOpen this job]//TT->Tool Bar->Job->Text in the Status Bar while opening the recent job
[]
[Recognizing file %s. You can press Esc to break]//not used
[]
[Recommended to fix HORZ for one Point inside ]//TTools; Adjustment; diagnostic message
[]
[Recommended to fix HORZ for Point(s) : %s]//TTools;   diagnostic message during Adjustment
[]
[Rectangle]//for internal use
[]
[Recurse folders]//TTools;Tlink; Drop options dialog; Check box name
[]
[Red]//TTools->attribute properies->color list box->possible value
[Kırmızı]
[Redo]//TTools; TLink; Tool Bat; Edit; menu item
[İleri]
[Redo\tCtrl+Y]//TL->ToolBar->Edit->Redo|TT->ToolBar->Edit->Redo
[İleri\tCtrl+Y]
[Reduce the window to an icon]//Command Minimize for Window; text in the Status Bar
[]
[Reference Line is singular]//TTools; CoGo; Inverse PTL, error message
[]
[Reflector height]//TT->Tool Bar->Select->Select TS Obs->list box name
[Reflektör yüksekliği]
[Reflector Height]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Reflektör Yüksekliği]
[Refraction Coefficient]//Process Properties dialog, TS-Computations page, Caption of the radio-buttons group
[Küresellik Düzeltmesi]
[Refresh]//TTools and TLink->Export to Device and Import from Device->button name
[Yenile]
[Region]//TTools; ->Job Configuration->Coordinate Systems ->Projection Properties dialog-> field name
[Ülke]
[Regional Australian Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Belgium Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Canadian Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid Denmark model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid French98 RAF98 model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid Model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid Model Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Regional Geoid Swedish model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid Swiss 2004 model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid2003 model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Geoid99/Geoid2003 model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional GeoidDutch model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Mexican Geoid97 model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional model geoid]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional NIreland Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional Norwegian Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Regional UK Geoid model]//TTools, TLink; - > Geoid properties dialog; Caption
[]
[Reject]//TTools; Adjustment; Button name
[Çıkart]
[Rejected]//internal use
[Çıkartıldı]
[Rejected Blunder Equations: ]//TTools;  error message under Adjustment
[]
[Rejected by Distance]//TTools; Adjustment; diagnostic message for QC
[]
[Rejected by Height]//TTools; Adjustment; diagnostic message for QC
[]
[Rejected by Horizontal Angle]//TTools; Adjustment; diagnostic message for QC
[]
[Rejected by Horz]//TTools; Adjustment; diagnostic message for QC
[]
[Rejected by Vertical Angle]//TTools; Adjustment; diagnostic message for QC
[]
[Rejected End(sec.)]//not used
[]
[Rejected Observations]//TTools; Adjustment; Table header
[]
[Rejected Start(sec.)]//not used
[]
[Rejected Status]//TTools; Adjustment; Column name
[]
[Rejection Criterion]//Process Properties dialog, Ttools spec., Adjustment page, Caption of the radio-buttons group
[]
[Related obs]//TT->Tool Bar->Select->Select GPS Occup., TS Occup->check box box name
[]
[Related point]//TT->Tool Bar->Select->Select TS Obs->check box name
[]
[Relative]//TT->Point tab->Properties for Point->Offset tab->radio button name
[]
[Remote access]//Job info dlg->Remote access checkbox
[]
[Remote Client Options]//Internal use
[]
[Remote Users Management]//TT->text in caption of dialog
[]
[Remote users...]//Job info dlg->Remote users button
[]
[Remote\\Client]//Internal use
[]
[Remove]//TTools; Codes; Menu Attribute properties; button|TTools and TLink->Custom Antennas List->button name|TTools and TLink->Custom Cameras List->button name|TT and TL->Job Configuration->Coordinate Systems->Geoid List->button name|TT->Report Configuration->Report format->radio button name|TT->TS Obs tab->Properties for TS Occupation->Custom TS Instrument->button name|Remote users dlg->button caption
[Kaldır]
[Remove All]
[]
[Remove Background Image(s)]
[]
[Remove background image(s) from job]//Ttools->view->Background images->Undo operation name
[]
[Remove from group]//TTools->File->Remote users->User prop.->button
[]
[Remove image]//TTools; Background images dialog;
[]
[Remove Photo Note]//TT and TL->Tab View->Point properties->Photo Notes tab->button name
[]
[Remove Point]//TTools; TLink; Localization window; button name
[]
[Remove User]//TTools->File->Remote users->group prop.->button
[]
[Removed modules: ]//Access codes dialog
[]
[Rename]//Resolve Duplicate Points dialog|TT->Job Configuration window->List configurations->Configurations list window->button name
[]
[Rename Points...]//TT and TL->Tab View->Points tab->Pop-up menu for point->command
[]
[Rename Points\nRename Points]//hint text (Pop-up menu for point->Rename Points)
[]
[Rename...]
[]
[Repeated Observations]//TT->Repeated Observations Report Options->Name field->value
[]
[Repeated Observations Report]//TT->tooltip
[]
[Reply]//Context menu item on history of messages dlg
[]
[Report]//menu item
[]
[Report - ]//not used
[]
[Report Configuration]//TT->Report Configuration window name
[]
[Report format]//TT->Report Configuration->Report format group box name
[]
[Report Loops]//TT->Loop Closure Report Options window->group box name
[]
[Report name]//message box
[]
[Report name is too long]//message box
[]
[Report Type]//TT->Repeated Observations Report Options->group box name
[]
[Reports:]//TT->Report Configuration->group box name
[]
[Reprocess GPS Obs]//TT->Residiul view window->pop-up menu
[]
[Required]//for internal use only
[Gerekli]
[Required road templates doesnt exist]//error message
[]
[Res A]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res D]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res e]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res El]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res n]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res u]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res X]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res Y]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Res Z]//TTools->GPS Obs Properties->Adjustment Tab->field name
[]
[Resect Export]//TLink; Resect Export Options,internal use
[]
[Resect Sheet]//TLink; Resect Export Options, Name Of Export Filter
[]
[Resection]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[]
[Resection computation on station %s failed]//TLink->Compute Coordinates->message
[]
[Reset]//TT->Filters window->By Time tab->button name|TTools; Adjustment Report Options, Button Name
[]
[Reset All]//TTools; Customize toolbars window; Toolbars Page; button mame
[]
[Reset Columns]//TTools and TLink->Tabular View->pop-up menu item on the column  headers
[]
[Residiul View]
[]
[Residual]//TT->Residiul View Options window->Residiul diagram->comment under cursor
[]
[Residual / QC]//TTools; Adjustment; Column name
[]
[Residual E]//TTools; Adjustment; Column name
[]
[Residual H]//TTools; Adjustment; Column name
[]
[Residual HA(&quot;)]//TTools; Adjustment; Column name
[]
[Residual N]//TTools; Adjustment; Column name
[]
[Residual SD]//TTools; Adjustment; Column name
[]
[Residual VA(&quot;)]//TTools; Adjustment; Column name
[]
[Residual View]//TT->GPSObs->Menu item
[]
[Residual View Item]//for internal use only
[]
[Residual View Item Options]
[]
[Residual View Options]//TT->Residiul View window caption
[]
[Residuals]//TTools; Adjustment; Column name|TT->Residiul View window->Legend window
[]
[Resolution, X]//camera property name
[]
[Resolution, Y]//camera property name
[]
[Resolve duplicate points]//Resolve Duplicate Points dialog
[]
[Restart]//TTools; Adjustment; Button name
[]
[Restore All]
[]
[Restore pane]//tooltip
[]
[Restore the window to normal size]//Command Restore for Window; text in the Status Bar
[]
[Reverse Line]//debug version only TTools->TabView->Page Code ->Pop-up menu item; tooltip
[]
[Right]
[]
[Right 1]//TTools->CoGo;Intersection
[]
[Right 2]//TTools->CoGo;Intersection
[]
[Rights]//Name of property
[]
[RINEX]//Import,Export,Convert Format Name|TTools and TLink -> Convert File.. ->File format
[]
[RINEX -> TPD not converted]//log message
[]
[RINEX Data File]//for internal use
[]
[RINEX import filter]//log message
[]
[RINEXExport to ]//log message
[]
[RMS]//TTools and TLink->GPS Occupations Properties->Page General->field name
[]
[Road]//TTools->Roads tab->grahic representation of the road|TT->Road properties->Window caption,Roads tab->right panel(graphic wiew of the road)->text under cursor
[]
[Road Cross Sections View]//TT->Roads tab(for internal view)
[]
[Road files]//TTools->Export->Format name
[]
[Road Horizontal Element]//TT->Roads tab->for internal use
[]
[Road Horizontal Elements]//TT->Roads tab->for internal use
[]
[Road Horizontal Elements List View Hint]//TT->Roads tab->for internal use
[]
[Road Horizontal Elements View]//TT->Roads tab(for internal view)
[]
[Road Name]//TTools->CoGo; Convert road to DTM
[]
[Road Vertical Element Object]//TT->Roads tab->for internal use
[]
[Road Vertical Elements]//TT->Roads tab->for internal use
[]
[Road Vertical Elements List View Hint]//TT->Roads tab->for internal use
[]
[Road Vertical Elements View]//TT->Roads tab(for internal view)
[]
[Road View Options]//TT->Roads tab->Options dialog name (for internal use)
[]
[Road\\]//TTools->CoGo; DTM compare
[]
[Roads]//for internal use only|for internal use???
[Yollar]
[Roads View Options]//TT->Roads view options dialog name (for internal use)
[]
[Roads View\nRoads View]//tooltip
[]
[Rollback]//Resolve Duplicate Points dialog
[]
[Rot E]//TTools;  objects description for Adjustment
[]
[Rot N]//TTools; objects description for Adjustment
[]
[Rot U]//TTools; objects description for Adjustment
[]
[Rotation]//TTools;TLink -> ToolBar -> Process -> Localization -> field name
[]
[Rover == Base on TS Obs %s]//diagnostic message during Compute coordinate
[]
[Rover Antenna Height]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Antenna Type]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Code]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Easting]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Elevation]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Ell ht]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Full Codes]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Latitude]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Longitude]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Northing]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Notes]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel
[]
[Rover Stations List\nRover Stations List]//for internal use
[]
[Rovers]//for internal use
[]
[RTK]//TTools and TLink->GPS Obs Properties ->Method, possible value|TTools->Map View->Legend window->line type|not used|name of module, in Autorizations dialog and in About
[]
[RTK (CarrierFixed)]//for internal use only
[]
[RTK (CarrierFloat)]//for internal use only
[]
[RTK (CodeDiff)]//for internal use only
[]
[RTK (CodeDiffSmooth)]//for internal use only
[]
[RTK AutoTopo]//TTools and TLink->GPSObs->Method->possible value|Solution Name
[]
[RTK Base]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[RTK Code Only]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[RTK Fixed]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[RTK Horizontal Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name
[]
[RTK Kinematic]//TTools->GPS Vectors Import
[]
[RTK Kinematic (AutoTopo)]//TTools->Map View->Legend window->point type
[]
[RTK Kinematic(Autotopo)]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[RTK L1 Only]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[RTK L2 Only]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[RTK Precisions]//for internal use only
[]
[RTK Precisions QC filter\nRTK Precisions QC filter]//internal use
[]
[RTK Static]//TTools->GPS Vectors Import
[]
[RTK Static (Topo) & Autonomous]//TTools->Map View->Legend window->point type
[]
[RTK Static Mode:]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[RTK Static(Topo)]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[RTK Stop&Go Mode:]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[RTK Topo]//TTools and TLink->GPSObs->Method->possible value|Solution Name
[]
[RTK Vertical Precision]//TT->Job Configuration->Quality Control->GPS Obs Precisions tab->field name
[]
[Run as Kinematic & Average Coord]//for internal use only
[]
[Run as Static & Average Coord]//for internal use only
[]
[Run as Static & Get Last Coord]//for internal use only
[]
[Run as Stop&Go & Average Coord]//for internal use only
[]
[Run as Stop&Go & Get Last Coord]//for internal use only
[]
[Run Background images dialog\nBackground images]//hint text in the Status Bar for the command  View->Background images
[]
[Run Filters dialog\nFilters]//for internal use only
[]
[Run Kinematic processing...]//log message
[]
[Run RTK processing (%d) (%s)...]//log message
[]
[Run Static processing...]//log message
[]
[Run Stop&Go processing...]//log message
[]
[RX]//TTools; TLink; Datum Transformation dialog; Datum parameter name  |TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name
[]
[RY]//TTools; TLink; Datum Transformation dialog; Datum parameter name|TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name
[]
[RZ]//TTools; TLink; Datum Transformation dialog; Datum parameter name  |TTools; ->Job Configuration->Coordinate Systems ->Custom datums list or Datum Properties dialog-> field name
[]
[s]//TT->Tool Bar->Select->Select GPS Occup and GPS Obs->Duration->spin edit name
[]
[S]//TTools; CoGo; Intersection|TLink; Resect Export, VA Measurement|TTools and TLink->Tabular View, Latituide, part of BLH coordinate value (insted of -)|TTools and TLink->Tabular View, Longituide, part of coordinate value (insted of +)|TTools; part of coordinate value on axis|TTools; part of coordinate value on axis|TTools and TLink->Tabular View, Longituide, part of coordinate value (insted of +)|not used
[]
[Sa&ve Job As...\nSave the job copy with a new name or in a different location\nSave Job As]//TT->Tool Bar->Job->Save Job as
[]
[Satellite]
[Uydu]
[Save]//TTools;TLink;log message|TTools; TLink; Datum Transformation window; button name|Save file dialog name|TTools (Job Configuration) and TLink (Configuration)->Save node name
[Kaydet]
[Save &As...]
[Farklı &Kaydet...]
[Save &As...\nSave the active file with a new name\nSave As]//TL->Saving a file to a different location(Tool Bar->File->Save As)
[Farklı &Kaydet...\nAktif dosyayı yeni isimle kaydet\nFarklı Kaydet]
[Save &As...\tF4]
[Farklı &Kaydet...\tF4]
[Save As]//Save as file dialog name
[Farklı Kaydet]
[Save as]//dialog name
[Farklı kaydet]
[Save as Surface]//TTools->CoGo->Compare Surfaces
[]
[Save changes to %s ?]//TTools;TLink; message box when closing a file
[]
[Save configuration]//TT->Job Configuration window->button name
[]
[Save datum as]
[]
[Save in:]//for internal use only|???
[]
[Save is not supported for this format. Do you want to save the file into a different format?]//message
[]
[Save Preliminary Coordinates]//TTools; Adjustment; Button name
[]
[Save Residuals]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Save View to File...]
[]
[Save...]//Context menu item on history of messages dlg
[Kaydet...]
[Saving]//TTools;TLink; message when closing a file
[Kaydediliyor]
[Saving build information...]//TL->log message|TT->log message
[]
[Saving file %s]//TTools;TLink;log message
[Dosya kaydediliyor %s]
[Saving file %s. You can press Esc to break]//not used
[]
[Saving job file %s...]//TT->Save job->text in the Status Bar
[]
[Saving project: ]//TT->text in the Status Bar
[]
[Scale]//TTools;  objects description for Adjustment|TLink; Resect Export, Header Field name|TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[Ölçek]
[Scale Factor]//TLink->Compute Coordinates->Scale factor dialog(for TS measurments)->caption|TTools; TLink ->Job Configuration->Coordinate Systems; Grid -> Ground window; Scale factor list box; name or Convert file dialog -> Grid -> Ground
[Ölçek Faktörü]
[Scale factor computed from MultiBS on station %s is %.7lf. Apply it ?]//TLink->Compute Coordinates->message
[]
[Scale factor computed from resection on station %s is %.7lf. Apply it ?]//TLink->Compute Coordinates->message
[]
[Scale ppm]//TTools; TLink; Datum Transformation dialog; Datum parameter name
[Ölçek ppm]
[Scan]//TTools and TLink->Images tab->Options->Show tab->check box name|TT->Tool Bar->Select->Select Points->Point type list box->value
[Tarama]
[Scan points filter\nScan points filter]//for internal use only
[]
[Scan Session]//Ttools->Scan Sessions tab->Properies window caption
[]
[Scan Session View Options]//TTools->Scan Sessions tab->Scan Session View options dialog->window caption
[]
[Scan Sessions]//TTools->Tabular View->tab name
[]
[Scan Sessions View\nScan Sessions View]//tooltip
[]
[Scanned]//not used
[]
[SD]//TLink; Resect Export, Header Field name|TL->Convert File->Advanced options->right panel->radio button name
[]
[SD misclosure]//TTools; Adjustment; Column name
[]
[SDist Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[EM Kaba Hatası]
[SDW files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[Second surface does not have unique HORZ projection]//TTools; CoGo; Compare surfaces, error message
[]
[Segment type]
[]
[Segments order change]
[]
[Select]//TLink->Convert File->Select a file file dialog->button name|Selection Header|TT->Point summary Report Options->group box name
[]
[Select &All]//TT->Tool Bar->Select->command name
[]
[Select &GPS Occupations...]//TT->Tool Bar->Select->command name
[]
[Select &None]//TT->Tool Bar->Select->command name
[]
[Select &Points...]//TT->Tool Bar->Select->command name
[]
[Select &TS Occupations...]//TT->Tool Bar->Select->command name
[]
[Select a file]//TLink->Convert File->selecting destination->Select a file file dialog caption
[]
[Select a folder for job]//TT->Creare a new job->message
[]
[Select all]//Context menu item on history of messages dlg
[]
[Select All]
[]
[Select all objects\nSelect all objects]//TT->Tool Bar->Select->Select All->hint text in the Status Bar
[]
[Select changed objects]
[]
[Select changed objects\nSelect changed objects]
[]
[Select folder]//for internal use only
[]
[Select GPS &Obs...]//TT->Tool Bar->Select->command name
[]
[Select GPS Obs]//TT->Tool Bar->Select->Select GPS Obs->Select GPS Obs dialog caption
[]
[Select GPS Obs...]//TT->Tool Bar->Select->command name
[]
[Select GPS Obs\nSelect GPS Obs]//TT->Tool Bar->Select GPS Obs->hint text in the Status Bar
[]
[Select GPS Occupations]//TT->Tool Bar->Select->Select GPS Occup->Select GPS Occup dialog caption
[]
[Select GPS Occupations...]//TT->Tool Bar->Select->command name
[]
[Select GPS Occupations\nSelect GPS Occupations]//TT->Tool Bar->Selec GPS Occupations->hint text in the Status Bar
[]
[Select None]//TT->Tool Bar->Select->command name
[]
[Select path for export]//TTools and TLink; browse for folder|not used
[]
[Select Plot: Functions]
[]
[Select Plot: Parameters]
[]
[Select Points]//TT->Tool Bar->Select->Select Points->Select Points dialog caption
[]
[Select points and/or lines in any view to add them to Surface]//TTools, helper text in status bar
[]
[Select points to add them to line]//TTools, helper text in status bar
[]
[Select points to insert them to line]//TTools, helper text in status bar
[]
[Select Points...]//TT->Tool Bar->Select->command name
[]
[Select Points\nSelect Points]//TT->Tool Bar->Selec Points->hint text in the Status Bar
[]
[Select static GPS observations that form a loop. Press Finish when you are done, and loop closure report will be displayed]//TT->Tool Bar->Process-> Loop Clousures->Loop Clousures window->comment
[]
[Select this Image as Surface Texture\nSet as Surface Texture]//TTools, HINT
[]
[Select this point as Inverse From\nInverse From]//TTools; for internal use only
[]
[Select this point as Inverse To\nInverse To]//TTools; for internal use only
[]
[Select TS O&bs...]//TT->Tool Bar->Select->command name
[]
[Select TS Obs]//TT->Tool Bar->Select->Select TS Obs->Select TS Obs dialog caption
[]
[Select TS Obs...]//TT->Tool Bar->Select->command name
[]
[Select TS Obs\nSelect TS Obs]//TT->Tool Bar->Selec TS Obs->hint text in the Status Bar
[]
[Select TS Occupations]//TT->Tool Bar->Select->Select TS Occup->Select TS Occup dialog caption
[]
[Select TS Occupations...]//TT->Tool Bar->Select->command name
[]
[Select TS Occupations\nSelect TS Occupations]//TT->Tool Bar->Selec TS Occupations->hint text in the Status Bar
[]
[Selected area size is %s %s x %s %s]//text in the Status Bar during selecting the area
[]
[Selected columns]//TTools and TLink->Tabular View->Options->group box name|TT->Compare Point Report Options window->grop box name|TT->Report->Report Configuration->TS Obs report options->group box name|TT->Report->Report Configuration->Cut Sheet Report->Optionsgroup box name|TT->Point summary Report Options->group box name|TTools->DL Obs Report -> Options dialog|TT->Localization summary Report Options->group box name
[Seçilmiş sütunlar]
[Selected occupations < %s. Plot CANNOT be drawn]
[]
[Selection]//TTools->Map View options and Cad View options->tab name
[Seçim]
[Semicolon]//TTools and TLink->Export files and Convert File->Custom format properties->Delimeters list box->possible value
[]
[Semicolon (;)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[Send]//Send files dlg button
[]
[Send file(s)]//Conext menu item
[]
[Send To]
[]
[Send To ...]
[]
[Send To\nSend To Dyna User]
[]
[Sended]//Msg status
[]
[Sending file(s)...]//Sending files dlg caption
[]
[Sending mail is not supported]//TopconLink error message box from menu Help/Feedback/SendBug|SendQuestion|TopconTools error message box from menu Help/Feedback/SendBug|SendQuestion
[]
[Server]//TT->for future release|Internal use
[]
[Session]//TL->File properties->page name
[]
[Sessions]//for internal use
[]
[Sessions List\nSessions List]//for internal use
[]
[Set as Surface Texture]//TTools, properties for Surface
[]
[Set default]//TT->Tool Bar->Select->Select GPS OBS,GPS Occup, Points, TS Obs, TS Occup->button name
[]
[Set Default Image]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[Set GLN Relative]//TT->Residiul view window->pop-up menu
[]
[Set GPS Relative]//TT->Residiul view window->pop-up menu
[]
[Set Image Measured Coordinates]//for internal use only
[]
[Shape]//TTools  -> Import; Export-> Format name
[]
[Shift]//Shortcut Description
[]
[Short ID]//for internal use only
[]
[Show]//for internal use only|TTools->Images tab->Options->Page name|TT->Occupation View Options window->tab name|TT->Residiul View Options window->tab name
[]
[Show all]//TT->Residiul view window->pop-up menu
[]
[Show Antennas List\nAntennas List]//for internal use
[]
[Show area size]//TTools->Map View options and Cad View options->Show page->check box name
[Alan değerini göster]
[Show azimuth]//TTools->Map View options and Cad View options->Show page->check box name
[Azimutu göster]
[Show Background Map]//Ttools->Map View and CAD View->Option in Options dialog
[Arkaplan Haritasını Göster]
[Show Bitmap]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[Bitmap Göster]
[Show Bitmap And Text]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[]
[Show Columns]//in options|TTools and TLink->GPS Occupations and GPS Obs Options-> frame name|orientation points|TT->Tabular View Optioms window|TT->Roads tab->Options dialog->group box name|TTools and TLink->GPS Occupations and GPS Obs Options-> frame name
[Sütunları Göster]
[Show columns]//TTools->CoGo; Options
[Sütunları göster]
[Show columns in left pane]//TTools, TLink; DL Obs Tab; Options dialog; text|TT->Tabular View Optioms window->Linework tab->group box name|TT and TL->TS Obs and Tape Dimensions tab->options->group box name
[Sol pencerede sütunları göster]
[Show columns in right pane]//TTools, TLink; DL Obs Tab; Options dialog; text|TT->Tabular View Optioms window->Linework tab->group box name|TT and TL->TS Obs and Tape Dimensions tab->options->group box name
[Sağ pencerede sütunları göster]
[Show columns left]//TTools; Linework Tab; Options dialog;|TT->X-Section Templates tab->options dialog->bottom group box name
[Sol sütunları göster]
[Show columns right]//TTools; Linework Tab; Options dialog;|/TT->X-Section Templates tab->options dialog->upper group box name
[Sağ sütunları göster]
[Show dimensions]//TTools->Map View options and Cad View options->Show page->check box name
[Boyutları göster]
[Show distance]//TTools->Map View options and Cad View options->Show page->check box name
[Mesafe göster]
[Show Ellipses]//TTools->Map View options->Show page->check box name
[]
[Show Grid]//TT->Roads tab and X-Section Templates tab->right panel->Options->Graphic Views->Check box name
[Gridleri göster]
[Show grid]//TTools->Map View options and Cad View options->Show page->check box name|TT->Occupation View Options window->Show tab->check box name|TT->Residiul View Options window->Show tab->check box name
[Gridleri göster]
[Show images]//TTools and TLink->Images tab->Options->Show tab->group box name
[Resimleri Göster]
[Show Legend]
[Lejandı Göster]
[Show legend]//TTools->Map View options->Show page->check box name|TT->Occupation View Options window->Show tab->check box name|TT->Residiul View Options window->Show tab->check box name
[Lejandı Göster]
[Show Lines in a table\nLines tab]//TTools->hint text->for internal use only
[]
[Show occupations by points]//TT->Occupation View Options window->Occupation View tab->radio button name
[]
[Show occupations by receivers]//TT->Occupation View Options window->Occupation View tab->
[]
[Show offline]//Conext menu item
[]
[Show offsets]//for internal use
[Ofsetleri göster]
[Show Offsets]//for internal use only
[Ofsetleri Göster]
[Show only ]//TT->Residiul view window->pop-up menu
[Sadece göster]
[Show or hide 3D View of the current job\n3D View]//TTools,tooltip
[]
[Show or hide CAD View of the current job\nCAD View]//TTools->Menu Bar->View->hint text in the Status Bar
[]
[Show or hide Codes List of the current job\nView Codes List]//TTools; Control Bar; Codes; Hint text in the Status Bar
[]
[Show or hide Layers List of the current job\nView Layers List]//TTools -> Menu Bar -> View -> Layers-> tooltip in the Status Bar
[]
[Show or hide Map View of the current job\nMap View]//TTools->Menu Bar->View->hint text in the Status Bar
[]
[Show or hide Occupation View of the current job\nOccupation View]//TT->Occupation view window->hint text in the Status Bar
[]
[Show or hide\nShow or hide this diagram]//not used
[]
[Show QAQC information in tooltip]//TTools->Map View options->QAQC page->check box name|TTools->Occupation View options->QAQC page->check box name
[]
[Show related DL Observations]//TT->command hint
[]
[Show related GPS Observations]//TT->command hint
[]
[Show related GPS Occupations]//TT->command hint
[]
[Show related Image]//TT->command hint
[]
[Show related Image Measured Points]//TT->command hint
[]
[Show related Images]//TT->command hint
[]
[Show related Lines]//TT->command hint
[]
[Show related objects]//TT->hint text in the Status Bar of command
[]
[Show related objects\\DL Observations]//TT->command name
[]
[Show related objects\\GPS Observations]//TT->command name
[]
[Show related objects\\GPS Occupations]//TT->command name
[]
[Show related objects\\Image]//TT->command name
[]
[Show related objects\\Image Measured Points]//TT->command name
[]
[Show related objects\\Images]//TT->command name
[]
[Show related objects\\Lines]//TT->command name
[]
[Show related objects\\Point]//TT->command name
[]
[Show related objects\\Points]//TT->command name
[]
[Show related objects\\Road IPs]//TT->command name
[]
[Show related objects\\Roads]//TT->command name
[]
[Show related objects\\Scan Sessions]//TT->command name
[]
[Show related objects\\Stereopairs]//TT->command name
[]
[Show related objects\\Surfaces]//TT->command name
[]
[Show related objects\\Tape Observations]//TT->command name
[]
[Show related objects\\TS Observations]//TT->command name
[]
[Show related objects\\TS Occupations]//TT->command name
[]
[Show related Point]//TT->command hint
[]
[Show related Points]//TT->command hint
[]
[Show related Road IPs]//TT->command hint
[]
[Show related Roads]//TT->command hint
[]
[Show related Scan Sessions]//TT->command hint
[]
[Show related Stereopairs]//TT->command hint
[]
[Show related Surfaces]//TT->command hint
[]
[Show related Tape Observations]//TT->command hint
[]
[Show related TS Observations]//TT->command hint
[]
[Show related TS Occupations]//TT->command hint
[]
[Show station name on cursor]//TT->Roads tab and X-Section Templates tab->right panel->Options->Graphic Views->Check box name
[Kursor da istasyon ismini göster]
[Show station name on station]//TT->Roads tab and X-Section Templates tab->right panel->Options->Graphic Views->Check box name
[İstasyon da istasyon ismini göster]
[Show station name on status bar]//TT->Roads tab and X-Section Templates tab->right panel->Options->Graphic Views->Check box name
[Durum çubuğunda istasyon ismini göster]
[Show SVs]//TT->Occupation View window->Pop-up menu item on occupation
[SVs leri Göster]
[Show Text]//TTools; Customize toolbars window; Commands Page; Pop-up menu item on the image in the Toolbar
[Text Göster]
[SHP]//TTools  -> Import; Export-> Format name
[]
[Side]//TT->Roads tab->X-sections->right panel->properties->list box name and column name|TT and TL->Properties for TS Obs->General tab->Type list box->value
[Kenar]
[Sight]//sight diagram name (Comment) (Croix in the centre ) ( CAD View openåd on TSMeasurement or TSImage )
[]
[Sigma]//not used
[]
[SigmaX]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel|for internal use only
[]
[SigmaY]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel|for internal use only
[]
[SigmaZ]//TTools and TLink->Export files and Convert File->Custom vector format properties->field in the left panel|for internal use only
[]
[SignalLevel]//for internal use
[]
[SIMA Coordinates]//TTools and TLink->Import, Export, Convert->Format name;
[]
[Size]//TTools and TLink; Import from device
[Boyut]
[Skip disabled SVs/epochs]//TTools and TLink->Export and Convert->Advanced options for GPS Raw Data files
[]
[Skip this object]//message  box
[]
[Skipped %d components with conditional %s coordinates]//TTools; diagnostic message during Adjustment
[]
[Slant]//TTools and TLink -> Tabular View ->GPS Occupations Propertie, Antenna tab ->Antenna Height Method list box -> text
[]
[Slant height should be positive]//TTools and TLink->error message for antenna height
[]
[Slope]//TT ->in advanced import/export options->Distance mode list box->value(for example export TS Obs->FC5 Raw)
[Eğik]
[Slope dist]//TT->Tool Bar->Select->Select TS Obs->list box name
[Eğik mesafe]
[Slope Distance]//TTools; Inverse window; bottom pane and Properties window|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Eğik Mesafe]
[Small Icons]//not used
[]
[Solid]//TTools->attribute properies->Outline tab->Style list box->possible value|TT->3D View->click on the 3D View window->Pop-up menu item Fill mode->Solid
[]
[Solution Type]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink ->GPS Obs tab and Properties for Observation-> column name
[Çözüm Tipi]
[Solution type]//TT->Tool Bar->Select->Select GPS Obs.->list box name
[Çözüm tipi]
[Some autotopo observations disagree with point coordinates by more then 10m. Point is probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Some autotopo observations disagree with point coordinates. Point is probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Some Control Points have Global Coordinates and some Local ones]//error message under Adjustment and Compute  Coordinates
[]
[Some Coordinates are unknown]//TTools; Inverse window; error message
[]
[Some Diagrams are EMPTY]
[]
[Some engine(s) is running. Stop it and close job?]//TT->Close job->message
[]
[Some fields cannot be saved to this format. Do you wish to save to another format?]//TTools;TLink; message box durin saving the file
[]
[Some file(s) failed to open, becouse source is not valid]
[]
[Some GPS occupations are more than 10m away from point. They are probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Some GPS occupations' autonomous positions are too far away from point. They are probably misnamed]//TT->TabView->Quality Control tab->message
[]
[Some objects have incorrect format]//error message
[]
[Some objects not processed because of db errors]//error message
[]
[Some objects not processed because of incorrect file name]//error message
[]
[Some of the points in Surface %s do not have coordinates in current grid or ground coordinate system. Those points will be missing from the triangulation]//TTools, message box
[]
[Some of the values are too long to be saved in this file format]//error message
[]
[Some Points have Global Coordinates and some Local ones]//error message under Adjustment and Compute  Coordinates
[]
[Some points haven't height]//message box
[]
[Some special symbols cannot be used in names]//TT->error message
[]
[Some users will be removed]//Remote users dlg->warning dlg->text
[]
[Sort]//TTools and TLink->Tabular View->pop-up menu item on the column  headers
[]
[Sort by selection]//Popup menu item on the column headers|Popup menu item on the column headers
[Seçilene göre sırala]
[Source]//???? for internal use only|TTools ->Tabular View ->GPS Occupations Properties->field name|TLink->Convert File->Left Panel->list box name|TTools and TLink->Properties for GPS Occupation->field name|TT->Tool Bar->Select->Select Points->field name|TT and TL->TSObs properties->General tab->field name
[Kaynak]
[Source type:]//not used
[]
[Source:]//TLink->Convert File dialog->list box name
[Kaynak:]
[South]//for internal use only
[]
[South Lat]//TTools; TLink -> Job Configuration or Convert file -> Custom Projections List -> Properties->Name column
[]
[Southing]//TTools->Map View and Cad View->axis name in Ground and Grid system
[]
[SP3 Precise Ephemeris Data File]
[]
[SP3&SP3C]
[]
[Space]//TTools and TLink->Export files and Convert File->Custom format properties->Delimeters list box->possible value|Shortcut Description
[Boşluk]
[Space ( )]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[Boşluk ( )]
[Spatial Object]//not used
[]
[Spiral]//TT->Roads tab->type of the added element
[Klotoid]
[Spiral 1 Len]//TT->Roads tab->Horz. element->Intersection->Properties->field name
[Klotoid Uzn 1]
[Spiral 2 Len]//TT->Roads tab->Horz. element->Intersection->Properties->field name
[Klotoid Uzn 2]
[Spiral Const]//TT->Roads tab->Horz. element->Properties for Spiral->field name
[Klotoid Parametresi]
[Spiral Const 1]//TT->Roads tab->Horz. element->Properties for Intersection->field name
[Klotoid A1]
[Spiral Const 2]//TT->Roads tab->Horz. element->Properties for Intersection->field name
[Klotoid A2]
[Spiral Dir]//TT->Roads tab->Horz. element->Spiral->Properties->list box name
[Klotoid Yönü]
[Split by:]//TTools->Occupation view->Split GPS Occupations dialog->list box name
[]
[Split Epoch]//not used
[]
[Split GPS Occupation:]//TTools->Occupation view->Split GPS Occupations dialog caption
[]
[Split Line]
[]
[Split selected line\nSplit selected line]
[]
[Split Time]//TTools->Occupation view->Split GPS Occupations dialog->list box name
[]
[Split...]//TTools->GPS Obs popup menu
[]
[Split\nSplit Occupation]//TTools->GPS Obs popup menu
[]
[Sq.%s]//template for making abbreviated square unit name out of regular linear unit name
[]
[Square %s]//template for making square unit name out of regular linear unit name
[]
[SS]//TTools, TLink; DL Obs Properties dialog; General Page, Type, field content|TT and TL->Properties for TS Obs->General tab->Type list box->value
[]
[Sta/Chainage]//TT->Roads tab->Properties for X-Section, Grade->field name
[İstasyon/KM]
[Sta/Chainage: ]//TTools->Roads tab->grahic representation of the road->text in the Status Bar|TT->Roads tab->Horz. and Vertical element->Graphic View->text in the Status Bar
[İstasyon/KM:]
[Staked]//TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[]
[Staked Point]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|???for internal use only|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[]
[Stakeout]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Stakeout points filter\nStakeout points filter]//for internal use only
[]
[Standalone]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value|TT->for future release
[]
[Standard]//not used
[]
[Standarddev.: ]//TLink; Resect Export, Subfield name
[]
[Start]//not used
[]
[Start adding points and lines to this Surface by clicking on them\nAdd Points and Lines to Surface]//TTools, tooltip
[]
[Start Deg Chord]//TT->Roads tab->Horz. element->Properties for Curve, Spiral, Intersection->field name
[]
[Start Deg Curve]//TT->Roads tab->Horz. element->Properties for Curve, Spiral, Intersection->field name
[]
[Start Grade]//TT->Roads tab->Vert. element->right panel->column name
[Eğim Başı]
[Start Name]//TTools->Convert road to points
[]
[Start Point]//for internal use only|TT->Roads tab->left panel->Road properties->list box name
[Başlangıç Noktası]
[Start Radius]//TT->Roads tab->Horz. element->right panel->column name
[]
[Start Sta/Chainage]//TT->Roads tab->left panel->Road properties->field name
[]
[Start Time]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools->Occupation view->Split GPS Occupations dialog->field name
[]
[Start time]//TT->Tool Bar->Select->Select GPS Obs.->list box name
[]
[Start Time Nanoseconds]//not used
[]
[Start Time Seconds]//not used
[]
[Starting autosave]//TTools; write message in log during the job autosaving
[]
[Startup]//TT->Startup dialog->caption
[]
[State or country code]//TLink; BlueBook Export Options, Processing  State or country code input field name
[]
[State/country code]//TLink; GPSDataTransfer Export Options, Name of input dialog
[]
[Static]//TTools and TLink ->Properties for Occupation->field Method->possible field content
[]
[Static Horizontal Precision]//TT->Job Configuration->Quality Control->Point Precisions tab->field name
[]
[Static occupations]//TT->Occupation View window->Legend window
[]
[Static Vertical Precision]//TT->Job Configuration->Quality Control->Point Precisions tab->field name
[]
[Static:]//for internal use only
[]
[Static\\Obs\\Disabled]//TTools; Filters window
[]
[Static\\Obs\\Potential]//TTools; Filters window
[]
[Static\\Obs\\Processed]//TTools; Filters window
[]
[Static\\Occupations]//TTools; Filters window
[]
[Static\\Points]//TTools; Filters window
[]
[Station]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TT->Job Configuration->Display->Roads tab ->Display CL Pos as list box->possible value
[İstasyon]
[Station East]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Station Elevation]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Station Interval]//TTools->Convert road to Lines
[]
[Station North]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item
[]
[Stationing Stakeout Interval]//TT->Roads tab->left panel->Road properties->field name
[]
[Stations]//not used|TTools and TLink->Export files and Convert File->TSRaw custom format properties->name of the first group of fields|not used
[]
[Statistical]
[]
[Status]//Name of Field
[]
[Status:]//Send files dlg static
[]
[Std Dev]//TTools, TLink; Tab View; DL tab; field name 
[Karesel Ort.Hata]
[Std Dev e]//TTools->Point Properties->General tab->Adjustment tab->field name
[]
[Std Dev Horizontal]//TT->Tool Bar->Select->Select Points->list box name
[]
[Std Dev Hz]//TTools->Point Properties->General tab->Adjustment tab->field name
[]
[Std Dev n]//TTools->Point Properties->General tab->Adjustment tab->field name
[]
[Std Dev u]//TTools->Point Properties->General tab->Adjustment tab->field name
[]
[Std Dev Vertical]//TT->Tool Bar->Select->Select Points->list box name
[]
[StdDev E]//TTools; Adjustment; Column name
[]
[StdDev H]//TTools; Adjustment; Column name
[]
[StdDev N]//TTools; Adjustment; Column name
[]
[Stereo Pair]//internal use
[]
[Stereo Pairs View\nStereo Pairs View]//stereo pair view command hint
[]
[Stereo View]//not used|not used
[]
[Stereo View Options]//TTools->Stereopair View options
[]
[Stereographic]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[]
[Stereopair View]//name of view window/command for stereopairs
[]
[Stereopair View Options]//header of "Stereopair View Options" dialog (View->Stereopair View Options)
[]
[Stereopairs]//stereo pair view window title
[]
[Stop]//TTools and TLink->GPS Occupations->Method->possible value
[Bitiş]
[Stop Time]//TTools and TLink -> Tabular View ->GPS Occupations Tab, column name
[Bitiş Zamanı]
[Stop&Go:]//for internal use only
[]
[Stop\\Obs\\Disabled]//TTools; Filters window
[]
[Stop\\Obs\\Potential]//TTools; Filters window
[]
[Stop\\Obs\\Processed]//TTools; Filters window
[]
[Stop\\Occupations]//TTools; Filters window
[]
[Stop\\Points]//TTools; Filters window
[]
[String]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools->Linework->Properties of Line|TT->Properties for point->String tab->field name|TT and TL->Properties for TS Obs->String tab->tab and field name
[Hat]
[String and Control Codes]//for internal use only
[]
[Strings]//TTools->Menu bar->Edit->Add->Add Line|TT(Job Configuration) and TL(Configuration)->Display ->Strings tab name
[]
[Subnetwork ]//TTools; Adjustment; diagnistic message
[]
[Subnetwork %s]//TTools; message during Adjustment
[]
[Subnetworks Count: ]//TTools; Adjustment; diagnistic message
[]
[Substitute with id='%s' already exists]//for internal use only log message
[]
[Substitute with id='%s' not found]//for internal use only log message
[]
[SubstituteParser: NULL]//for internal use only log message
[]
[Suffix can not contain special symbols]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[]
[Surface]//caption in Surface properties|TTools->CoGo->Compare Surfaces; Second Surface type|part of the window caption name  ( CAD View openåd on DTM )
[]
[Surface %s is not built]//TTools, TDTM::Update returns E_FAIL
[]
[Surface already exists. Overwrite?]//TTools->CoGo; Road2DTM
[]
[Surface from Road is not created]//TTools->CoGo; Convert road to DTM
[]
[Surface Name]//TTools->CoGo; Convert road to DTM
[]
[Surface Table View Options]//caption of Options dialog
[]
[Surface\\]//TTools->CoGo; DTM compare
[]
[Surfaces]//caption of Surface tab
[]
[Surfaces List\Surfaces List]//currently not used
[]
[Surveyor]//TLink; Resect Export, Header Field name|TL->File properties->Session tab->field name
[]
[Surveys]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->name of the first group of fields
[]
[Suspected Repeated GPS Observations]//TTools; Adjustment; Table header
[]
[Suspected Repeated Observations]//TTools; Adjustment; Table header
[]
[Swap Images]//TTools->Stereopairs tab->pop-up menu item for the left pane
[]
[Swap Images\nSwap Images]//TTools->Stereopairs tab->pop-up menu item for the left pane->tooltip
[]
[Swing]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[]
[Switch to the next document window]//Command Next for Window; text in the Status Bar
[]
[Switch to the previous document window]//not used
[]
[System]//TT->Process properties->GPS+Post Process tab->list box name
[]
[Systems and Units]//for internal use only|for internal use only|TTools->GPS Vectors Import|for internal use
[]
[Tab]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box|TTools and TLink->Export files and Convert File->Custom format properties->Delimeters list box->possible value
[Tab]
[Table]//TT->Roads tab->left panel->node name
[]
[Tabular View Options]//TL->Tool Bar->View->options->Tabular View|TT->View->Optioms->Tabular View->window caption
[Tablo Görünüm Seçenekleri]
[Tangent]//TT->Roads tab->Horz. element->Properties for Curve->field name
[]
[Tangential to prev element]//TT->Roads tab->Horz. element->right panel->Properties ->check box name
[]
[Tape]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Tape Dimensions]//TTools->Map View->Legend window->line type|TT->Tabular View Options->page name
[]
[Tape Obs]//TT->Tabular View->tab name
[]
[Tape Obs filter\nTape Obs filter]//TT->View->Filters->By Type
[]
[Tape Obs Ref.Line]//for internal use
[]
[Tape Obs View\nTape Obs View]//TT->Tabular View->hint for Tape Dimensions tab
[]
[Tau / Tau Crit.]//TTools; Adjustment; Column name 
[]
[Tau Criterion]//Process Properties dialog, Ttools spec., Adjustment page,  radio-button
[]
[Tb]//units of files size - send file dialog
[]
[TDD Code Library]//TTools; Codes; Export to file; file format
[TDD Kod Kütüphanesi]
[TDS export filter]//log message
[]
[TDS import filter]//log message
[]
[TDS Raw Data File]//for internal use
[]
[TDS RD5]//TTools->Export->Format name
[]
[TDS RW5 GPS Obs]//Import,Convert: Format Name
[]
[TDS RW5 TS Obs]//Import,Convert: Format Name
[]
[TDS TP5]//TTools->Export->Format name
[]
[TDSExport to ]//not used
[]
[Tekla XRoad File]//"Tekla XRoad File"  //TTools->Export->Format name
[]
[Telescopic]//TTools and TLink->Images tab->Options->Show tab->check box name
[Teleskopik]
[Tell your version number \r\n%s\r\n to Topcon Sales&Support representative and get your Access Code]//not used
[]
[Temperature]//TLink; Resect Export, Header Field name|for internal use only
[Sıcaklık]
[Template]//TT->Roads tab->X-sections->right panel->properties->list box name and column name
[Şablon]
[TerminatedParser: Not all data parsed]//for internal use only log message
[]
[TerminatedParser: Number of parsers != 2]//for internal use only log message
[]
[TerminatedParser: Reach end]//for internal use only log message
[]
[Text]//TTools; Codes; New Attribute; Pop-up menu command|TTools->Codes->New Attribute->possible attribuite type|Message prop. name
[]
[Text Attribute]//not used
[]
[Text cannot be empty]//error message
[]
[Text Documents (*.txt)]//Msg history dlg -> Save -> Filter name
[]
[TFW files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[tH]//TLink; Resect Export, Header Field name
[]
[The ephemeris file is empty.\nPlease be sure you have correct ephemeris\nand repeat import again.]//not used
[]
[The imported TopSURV or Topcon Tools job configuration is different from the current Topcon Tools job configuration as shown below. Check the box next to the configuration item(s) you want to use]//TT (while job configurations conflict, for example during job import)->Override Job Configuration window->text
[]
[The job %s already exists, overwrite?]//TT->Create a new job->message
[]
[The maximum number of custom reports (99) is reached. If you want to add more reports, delete some unnecessary reports.]//message box
[]
[The maximum number of invalid codes exceeded]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog->message
[]
[The point with name '%s' already exists]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[]
[The program has been closed.]//message
[]
[The starting number is empty. Enter a staring number, for example '0001' or 'Pt0001'.]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[]
[The starting number should contain digits. Enter a valid staring number, for example '0001' or 'Pt0001'.]//TT and TL->Points tab->Pop-up menu item Renumber Points->Points renumbering/renaming window->message
[]
[The toolbar name you have specified cannot be used because there is already a toolbar with that name]//TTools; Customize toolbars window; Toolbars Page; New Toolbar dialog; error message during creation new toolbar
[]
[The TopSURV job you are trying to open was created in a newer version than the version of Link/Tools  you are using. Please upgrade to the latest version of Link/Tools available. ]
[]
[The TopSURV job you are trying to open was created in a newer version than the version of Link/Tools  you are using. Trying to open this job can result in loosing some data. Do you still want to continue?]
[]
[There are multiple Surfaces selected for export; only one will be exported]//TT->export->log message
[]
[There are no objects to show]//Message box (cmd show related objects)
[]
[There are no vectors for export]//log message
[]
[There are no vectors for processing]//log message
[]
[There are not data for exporting]//for internal use only log message
[]
[There are not occupations for export]//log message
[]
[There are two ways to enter the azimuth:\r\n  1. Directly...For example: 322\xB012'10.1"\r\n  2. As PtStart-PtEnd+Angle or PtStart-PtEnd-Angle]//TTools; CoGo; Intersection
[]
[There are two ways to enter the distance:\r\n  1. Directly...For example: 101.20\r\n  2. As PtStart-PtEnd+Distance or PtStart-PtEnd-Distance]//TTools; CoGo; Intersection
[]
[There is no antenna information for some of the RTK Bases\r\nPhase center coordinates will be used to compute rover positions]//TTools; Adjustment;  message
[]
[There is no BS on station %s. Do you want to use the measurement #%d to point %s as BS ?]
[]
[There is no intersection]//TTools; CoGo; Intersection
[]
[There is no registered viewer for this file]//error message
[]
[They are probably identical]//TT->TabView->Quality Control tab->message
[]
[This control point does not link with the network. To view or edit properties for this point right-click a selected point and click Properties on the pop-up menu. Test determines that this point is not linked with network. The test is performed in the background mode during adjustment.  It is only warning for user. It is necessary to analyze situation: 1) The control point was not assign correctly; 2) In some cases it doesn’t lead to any errors.  For example, the control points were in large excess.  To turn off the feature that marks a point red when it fails some quality control tests, select the Ignore QC check box.]
[]
[This DL observation is marked in red on the Views  and in the Reports because of not satisfying the precision values for the DL Obs ((Job->Job configuration->Quality Control->DL ObsPrecision tab). . To view or edit properties for this occupation right-click a selected point and click Properties on the pop-up menu. The Quality Control tab contains informational text on the selected observation (marked in red on the Views and in the Reports).  After the net has been adjusted, a level measure with bad elevation is found. In this case, the level measure has precision worse than the value in the settings for the job (Job->Job configuration->Quality Control-> DL Obs Precision tab). After testing, the pair of the points (BS and FS) of DL observation found will not be used in the adjustment of this net.  To turn off the feature that marks an observation red select the Ignore QC check box. The precisions values can be change, if it is necessary. Click Job->Job Configuration or press Ctrl+F2, then click Quality Control on the menu tree in the left panel. In the tab DL Obs Precisions change the values of precisions.]
[]
[This format doesn't support compound spirals.]//error message
[]
[This format doesn't support linework with arcs.]//error message
[]
[This GPS observation is marked in red on the Views  and in the Reports because of not satisfying the precision values for the GPS Obs ((Job->Job Configuration ->Quality Control->GPS ObsPrecision tab). To view or edit properties for this observation right-click a selected observation and click Properties on the pop-up menu. The Quality Control tab contains informational text on the selected observation (marked in red on the Views and in the Reports). The test is performed after adjustment. In this case Horizontal Precision/Vertical Precision for RTK and GPS post-processing vector are worse than the value in the settings for the job (Job->Job Configuration ->Quality Control-> GPS Obs Precision tab).  To turn off the feature that marks an observation red select the Ignore QC check box. The precisions values can be change, if it is necessary. Click Job->Job Configuration or press Ctrl+F2, then click Quality Control on the menu tree in the left panel. In the tab GPS Obs Precisions change the values of precisions.]
[]
[This GPS observation is marked in red on the Views and in the Reports because it is failed to process. To view or edit properties for this observation, right-click a selected observation and click Properties on the pop-up menu.  The Quality Control tab contains informational text on the selected observation (marked in red on the Views and in the Reports). The GPS post-processing vector could not be processed because of incomplete set of data,  for example,  due to the absence of navigation data for corresponding  observation data. The user has to download the navigation data. To turn off the feature that marks an observation red select the Ignore QC check box.]
[]
[This GPS observation is marked in red on the Views and in the Reports because it is processed with ambiguities. To view or edit properties for this observation right-click a selected observation and click Properties on the pop-up menu.  The Quality Control tab contains informational text on the selected observation (marked in red on the Views and in the Reports). If the results are not suitable for you then analyze data or obtain new data.  To turn off the feature that marks an observation red select the Ignore QC check box.]
[]
[This GPS observation is marked in red on the Views and in the Reports because of not satisfying the precision values for the GPS Obs ((Job->Job configuration ->Quality Control->GPS Obs Precision tab). To view or edit properties for this observation right-click a selected point and click Properties on the pop-up menu. The Quality Control tab contains informational text on the selected observation (marked in red on the Views and in the Reports).   After the net has been adjusted, a bad component is found (Plane or Height). In this case, the bad component is a component of GPS observation (vector) which has precision worse than the value in the settings for the job (Job->Job configuration->Quality Control-> GPS Obs Precision tab). After testing, the outlier (bad) component of vector found will not be used in the adjustment of this net. To turn off the feature that marks an observation red select the Ignore QC check box.  The precisions values can be change, if it is necessary (  Job->Job Configuration -> Quality Control-> GPS Obs Precisions ).]
[]
[This is a reserved keyword and cannot be used as code or layer name]//TT->error message
[]
[This is incorrect code!!!]//TT->Tool Bar->Help->Access Codes->Enter Access Code dialog (warning message)
[]
[this is not a Traverse]//diagnostic message during Adjustment and Compute coordinate
[]
[This point (see GPS Occupation tab) is marked in red on the Views and in the Reports because of not passing the Misnamed Autotopo Rovers test. For kinematic measurements only. This test determines that this occupation probably does not belong to the specified point, because these coordinates are by more than 30 meters different from the coordinates of the other occupations corresponding to the point. It is a warning for user. In this case the user has to change the site name for the suspect occupation or to verify errors of the parameters for the corresponding occupation.  The presence of such occupations is a warning for user. It is necessary to analyze such occupation carefully. If there are some misnamed occupations indeed, it can lead to the distortion of the network connectivity during adjustment. For finding the source of errors can be useful to view Misnamed GPS Occupations Report. The test is performed in the background mode after any changing of the occupation’s parameters. To turn off the feature that marks a point red when it fails some quality control tests, select the Ignore QC check box. It is possible to cancel executing of this test at all for all points. To do this click   Job->Job configuration->Quality Control->Automatic Tests tab and turn off the corresponding check box]
[]
[This point (see GPS Occupation tab) is marked in red on the Views and in the Reports because of not passing the Misnamed GPS Occupations test.For static measurements only. This test determines that this occupation probably does not belong to the specified point, because these coordinates are by more than 30 meters different from the coordinates of the other occupations corresponding to the point. It is a warning for user. In this case the user has to change the site name for the suspect occupation or to verify errors of the parameters for the corresponding occupation.  The presence of such occupations is a warning for user. It is necessary to analyze such occupation carefully. If there are some misnamed occupations indeed, it can lead to the distortion of the network connectivity during adjustment. For finding the source of errors can be useful to view Misnamed GPS Occupations Report. The test is performed in the background mode after any changing of the occupation’s parameters. To turn off the feature that marks a point red when it fails some quality control tests, select the Ignore QC check box. It is possible to cancel executing of this test at all for all points. To do this click   Job->Job configuration->Quality Control->Automatic Tests tab and turn off the corresponding check box.]
[]
[This point is marked in red on the Views and in the Reports because of not passing the Identical Points test (see the Quality Control tab of the Properties for point) . This test determines the points with a small distance between them (less then Horizontal Precision /Vertical Precision).  The test is performed in the background mode after opening the job, after any changing of the points coordinates, and after creating or importing the new points.  The presence of such points is a warning for user. It is necessary to analyze such point carefully.  To turn off the feature that marks a point red when it fails some quality control tests, select the Ignore QC check box.  The precisions values can be change, if it is necessary. Click Job->Job configuration or press Ctrl+F2, then click Quality Control on the menu tree in the left panel. In the tab Point Precisions  change the values of precisions depending of the point type. It is possible to cancel executing of this test at all for all points. To do this click   Job->Job configuration -> Quality  Control ->Automatic Tests tab and turn off the corresponding check box.]
[]
[This point is marked in red on the Views and in the Reports because of not passing the Misnamed GPS Occupations test. test (see the Quality Control tab of the Properties for point). Test determines that there are several occupations for this point and the difference between the coordinates of the occupations is more than 30 meters.  The presence of such points is a warning for user. It is necessary to analyze such point carefully. The presence of such points can lead to the errors in Adjustment. If there are some misnamed occupations indeed, it can lead to the distortion of the network connectivity during adjustment.   The possible reasons are: 1. These occupations probably are misnamed.  In this case the user has to change the site name for the suspect occupation; 2. There were   errors in point’s coordinates or parameters of the corresponding occupation during entering the data.  The test is performed in the background mode after any changing of the points coordinates.  To turn off the feature that marks a point red when it fails some quality control tests, select the Ignore QC check box.  It is possible to cancel executing of this test at all for all points. To do this click   Job->Job configuration-> Quality Control->Automatic Tests tab and turn off the corresponding check box.]
[]
[This point is marked in red on the Views and in the Reports because of not passing the Point Standard Deviation test (see the Quality Control tab of the Properties for point).In this case Horizontal Precision /Vertical Precision for this point are worse than the value in the settings for the job (Job->Job configuration ->Quality Control ->Point Precision tab).   The precision values   depend on the selected Job Configuration. The test is performed during Adjustment, after any changing of the point’s standard deviations and after importing the TopSurv Jobs. The presence of large quantity of such points indicates that the network has a bad precision and it is necessary to take it into account and to analyze the situation.  Points with precision’s values dozens of times more then Point Precession tab settings indicate that : 1. There are blunders in the network; 2. The presence of the points with the same name corresponded to the different measurements; 3. Assignment  of  the  same name for the TS and GPS measurements mistakenly; 4. Incorrect fixing of the control points; 5.The presence of blunders during the  measurements; 6. Incorrect settings of  the antenna’s height and type for the reflector.To turn off the feature that marks a point red when it fails some quality control tests, select the Ignore QC check box.   The precisions values can be change, if it is necessary. Click Job->Job configuration or press Ctrl+F2, then click Quality Control on the menu tree in the left panel. In the tab Point Precisions  change the values of precisions depending of the point type. It is possible to cancel executing of this test at all for all points. To do this click   Job -> Job configuration ->  Quality Control -> Automatic Tests tab and turn off the corresponding check box.]
[]
[This point is very close to point %s. They are probably identical]//TT->TabView->Quality Control tab->message
[]
[This program requires a hardware lock (dongle)]//error message
[]
[This TS observation is marked in red on the Views and in the Reports because of presence a suspect component (Horizontal/ Vertical Angle or Distance). The suspect component is a component of TS observations, which is different from corresponding repeated  vectors components by more than the value in the  settings for the job (Job->Job configuration->Quality Control->TS Obs Precision tab).  To view or edit properties for this occupation right-click a selected point and click Properties on the pop-up menu. The Quality Control tab contains informational text on the selected observation (marked in red on the Views and in the Reports).  In the family of repeated (more than 2) TS observations a suspect component (Horizontal/ Vertical Angle or Distance) is found. The suspect component is a component of TS observations, which is different from corresponding repeated  vectors components by more than the value in the settings for the job (Job->Job configuration->Quality Control->TS Obs Precision tab). This test is executed during the net adjustment, and the outlier (suspect) component of TS observation found will not be used in the adjustment of this net. To turn off the feature that marks an observation red select the Ignore QC check box. The precisions values can be change (  Job->Job Configuration -> Quality Control-> TS Obs Precisions )]
[]
[Tilde (~)]//TTools->Export->Cut Sheet  user-defined format->Delimeters list box
[]
[Tile &Horizontally]
[Yatay &Döşe]
[Tile &Horizontally\nArrange windows as non-overlapping tiles\nTile Windows Horizontally]//TL->Tool Bar->Window|TT->Tool Bar->Window
[Yatay &Döşe\nArrange windows as non-overlapping tiles\nPencereleri Yatay Döşe]
[Tile &Vertically]
[Düşey &Düşe]
[Tile &Vertically\nArrange windows as non-overlapping tiles\nTile Windows Vertically]//TL->Tool Bar->Window|TT->Tool Bar->Window
[Düşey &Döşe\nArrange windows as non-overlapping tiles\nPencereleri Düşey Döşe]
[Time]//TTools->Occupation view->Split GPS Occupations dialog->Split by list box->value|Message prop. name
[Zaman]
[Time Filter]//for internal use only
[Zaman Filitre]
[Time Filter Options]//for internal use only
[Zaman Filitre Seçenekleri]
[Time span of GPS Occupations are intersected]//TTools->Occupation view->Merge->message
[]
[Time Stamp]//TTools->Export->Cut Sheet  user-defined format properties dialog->possible item|TT and TL - tab name in Properties for staked points|TT->Report->Report Configuration->Cut Sheet Report->Options->available report item
[]
[TN3 Surface]//TT->Export,Import->format name
[TN3 Yüzey]
[TN3 Surface File]//not used
[]
[To]//TTools->CoGo;Inv PTL|TTools, TLink; Tab View; DL tab; field name|TTools->Job Configuration->Coordinate Systems->Grid to Ground->Ground Origin->Compute Azimuth->list box name name|TLink->Convert File dialog->left group box caption|TT->Tab View->Linework tab->Column name|Message prop. name
[ya]
[To 1]//TTools; CoGo; Intersection
[]
[To 2]//TTools; CoGo; Intersection
[]
[To add a command to a toolbar, drag the command item from commands list onto a toolbar.]//TTools; Tool Bar; View; Customize; Customize toolbars; Commands tab; hint text
[]
[To Civil 3D job]
[Civil 3D İşine ]
[To point]//TT->Tool Bar->Select->Select TS Obs->field name
[]
[To Point]//TTools->CoGo->Traverse|TT->Point tab->Properties for Point->Offset tab->list box name
[]
[To:]//TTools; Inverse window; right-upper pane name|Send files dlg group caption
[]
[Too big misclosure for: ]//TTools;  error message under Adjustment
[]
[Too few conditions for ]//TTools;  error message under Adjustment
[]
[Too FEW points in Subnetwork]//TTools; Adjustment; diagnistic message
[]
[Toolbar name]//TTools; Customize toolbars window; Toolbars Page; New Toolbar dialog; field name
[]
[Toolbars]//TTools; Tool Bar; View; Customize; Customize toolbars window; Page name
[]
[Top left corner - X]//Ttools->view->Background images->left panel (Available images)->field name
[]
[Top left corner - Y]//Ttools->view->Background images->left panel (Available images)->field name
[]
[Topcon DL Obs]//TTools; Import, Export; Format name; extensions
[]
[Topcon Geoid files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[]
[Topcon Japan Coordinates]//TTools and TLink->Import, Export, Convert->Format name;
[]
[Topcon Japan Raw]//TTools and TLink->Import, Export, Convert->Format name;
[]
[Topcon Link]//TL->main window name
[Topcon Link & PAKSOY TEKNİK HİZ.]
[Topcon Link Ver. 6.11]//TL->Tool Bar->Help->About Topcon Link window->text
[]
[Topcon Logo Item]//for internal use only
[]
[Topcon Logo Item Options]//for internal use only
[]
[Topcon MC]//TTools->Export->Format name
[]
[Topcon Positioning Systems, Inc]//TL->Tool Bar->Help->About Topcon Link window->text|TT->Tool Bar->Help->About Topcon Tools window->text
[]
[Topcon SSS]//TTools->Export->Format name
[]
[Topcon Tools]//TT->part of the main window name(job name - Topcon Tools) and text in the message box when jod is deleted
[]
[Topcon Tools Job]//TT->Export,Import->Format name; TT->Job Info->window caption
[]
[Topcon Tools Job(*.ttp)|*.ttp]//TT->Export,Import->Format name;
[]
[Topcon Tools Jobs (*.ttp)|*.ttp||]//TT->Open a job->Open-Files of type list box->content
[]
[Topcon Tools Ver. 6.11]//TT->Tool Bar->Help->About Topcon Tools window->text
[]
[Topcon XML]
[Topcon XML]
[Topcon xml Antenna files]//TTools, TLink; -> Antenna List;, Add button; ->Open dialog;  -> Job Configuration->Equipment->ImportCalibrationSetFormat name
[Topcon xml Anten dosyaları]
[Topcon XML DL Obs]//Import,Export,Convert: Format Name
[Topcon XML DL Gözl.]
[Topcon XML GPS Obs]//Import,Export,Convert: Format Name
[Topcon XML GPS Gözl.]
[Topcon XML Points]//Import,Export,Convert: Format Name
[Topcon XML Noktaları]
[Topcon XML Roads]//Import,Export,Convert: Format Name
[Topcon XML Yolları]
[Topcon XML TS Obs]//Import,Export,Convert: Format Name  
[Topcon XML TS Gözl.]
[Topcon XML X-Section Templates]//Import,Export,Convert: Format Name
[Topcon XML Enkesit Şablonları]
[Topo]//TTools and TLink ->Properties for Occupation->field Method->possible field content
[]
[Topo occupations]//TT->Occupation View window->Legend window
[]
[Topo&Autonomous\\Points]//TTools; Filters window
[]
[Topo\\Obs\\Disabled]//TTools; Filters window
[]
[Topo\\Obs\\Enabled]//TTools; Filters window
[]
[Topo\\Occupations]//TTools; Filters window
[]
[TopSURV]//TTools->Export->Format name
[TopSURV]
[TopSURV 6.11 Job]
[TopSURV 6.11 İşi]
[TopSURV CE Job]
[TopSURV CE İşi]
[TopSurv Coordinates]//TTools, Import and Export from files; format name
[TopSurv Koordinatları]
[TopSURV Filter]
[TopSURV Filitre]
[TopSurv installation is not complete on the controller]//TT and TL->Export to Device,Import from Device ->error message
[Kontrol Ünitesine TopSurv ün yüklenmesi tamamlanmadı]
[TopSURV Job]
[TopSURV İşi]
[TopSURV PC Job]
[TopSURV PC İşi]
[Total RMS]//TTools; TLink; Localization; Properties; field name
[Toplam RMS]
[Total size:]//Send files dlg static
[]
[Total Station Image]//for internal use only
[]
[Total station observations]//for internal use
[]
[Towards %s]//not used
[]
[TPD]//Import, Export, Convert: Fromat Name
[]
[TPD -> RINEX not converted]//log message
[]
[TPD filter not found]//log message
[]
[TPD Import Filter]//log message
[]
[TPDExport to ]//log message
[]
[TPS]//TTools and TLink -> Import; Export; Convert File-> Format name
[]
[TPS controller]
[]
[TPS import filter]//log message
[]
[Track]//for internal use
[]
[Tracks]//for internal use
[]
[Tracks List\nTracks List]//for internal use
[]
[Tracks View Options]//for internal use
[]
[Transaction Path]
[]
[Transfer operation is in progress. If you interrupt it, the transferred files can be corrupted. Are you sure you want to interrupt?]//message box
[]
[Transferred:]//Send files dlg
[]
[Transit]//Process Properties dialog(TLink spec.), page Compute Coordinates;  List box Adjustment type|Direction
[]
[Transverse-Mercator]//TTools; TLink;->Job Configuration (TTools); Convert File -> Projection -> Custom Projections List -> Properties -> Projection Type list box -> text
[]
[Traverse]//TTools, Traverse, Caption
[]
[Traverse has bad configuration]//diagnostic message during Adjustment and Compute coordinate
[]
[Traverse Task Report]//TTools; CoGo; Traverse, report name
[]
[Traverse...]//TTools; Menu Bar; COGO; menu item Traverse...
[]
[Treated %d Kinematic GPS Obs]//TTools; Adjustment; diagnistic message       
[]
[Treated %d Offset Points]//TTools; Adjustment; diagnistic message   
[]
[Treated %d Tape Measurements]//TTools; Adjustment; diagnistic message
[]
[Treated %d Track(s)]//diagnostic message during Compute coordinate
[]
[Treated %d Vector(s)]//diagnostic message during Compute coordinate
[]
[Triangulation ]//Ttools, message
[]
[Troposhepre model:]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Troposphere parameters are applied in all non-RTK modes]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[TS]//TTools->Map View->Legend window->line type|name of module, in Autorizations dialog and in About
[]
[TS ]//TTools; Adjustment;
[]
[TS Backsight]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[TS Backsights filter\nTS Backsights filter]//TT->View->Filters->By Type
[]
[TS Distance Precision]//TT->Job Configuration->Quality Control->TS Obs Precisions tab->field name
[]
[TS from point %s%s to point %s%s ]
[]
[TS HA Precision (sec.)]//TT->Job Configuration->Quality Control->TS Obs Precisions tab->field name
[]
[TS Instrume&nts]//for internal use
[TS Cihazlar&ı]
[TS Instruments]//for internal use
[TS Cihazlar]
[TS Instruments List\nTS Instruments List]//for internal use
[TS Cihaz Listesi\TS Cihaz Listesi]
[TS Obs]//TL->File properties->part of the window name; TL->Convert file->file format
[TS Gözl.]
[TS Obs Report]//TT->Report->Report Configuration->TS Obs report options->hint (for internal use)
[]
[TS Obs Report Options]//TT->Report->Report Configuration->TS Obs report options window name
[TS Gözl.Rapor Seçenekleri]
[TS Observations List\nTS Observations List]//TT and TL->TSObs->hint text(for internal use)
[TS Gözlemleri Listesi\nTS Gözlemleri Listesi]
[TS Occupation]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value|TT and TL->TS Occupation properties->window caption
[]
[TS Occupations]//for internal use
[TS Oturumları]
[TS Occupations List\nTS Occupations List]//not used
[]
[TS Points do not have WGS84 coordinates and will NOT be adjusted]//ATTools; message during Adjustment
[]
[TS Precisions]//for internal use only
[]
[TS Raw Data Measurements]//for internal use only
[TS Ham Data Ölçümleri]
[TS Sideshot]//TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[TS Sideshots filter\nTS Sideshots filter]//TT->View->Filters->By Type
[]
[TS Stations filter\nTS Stations filter]//TT->View->Filters->By Type
[]
[TS to SC]//TT->Roads tab->Add Horz. Element: Spiral window->Spiral Dir list box->value
[TS dan SC  ]
[TS VA Precision (sec.)]//TT->Job Configuration->Quality Control->TS Obs Precisions tab->field name
[]
[TS vectors only]//TT->Repeated Observations Report Options->radio button name
[]
[TS-Computations]//Process Properties dialog, TS-Computations page, Caption
[]
[TS-Export]
[TS-Aktar]
[TSRaw custom format properties]//TTools and TLink->Export files and Convert File->Custom format properties dialog name
[TSHam özel format özellikleri]
[Turn]//TT->Roads tab->Horz. element->Spiral and Curve->Properties->list box name
[Dönüş]
[Turning Pt.]//TTools, TLink; DL Obs Properties dialog; General Page, Type, field content
[]
[Twice defined function %s]
[]
[Type]//TTools; Adjustment; Column name|TTools, TLink; DL Occupation Properties dialog; field name|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools->Linework->Properties of Line|for internal use only|Ttools->view->Background images->left panel (Available images)->field name|for internal use only|TTools and TLink->Codes->Attribuite type|TT->Repeated Observations Report list->column name|TT->Roads tab->Horz and Vertical element->right panel->column name|TT->Tool Bar->Select->Select GPS Obs->list box name|TT and TL->TS Obs tab->column name and Properties for TS Obs->General tab->list box name
[Tip]
[U Residual]//TTools; TLink; Datum Transformation; Properties; field name
[]
[UK Geoid Files]//TTools, TLink; -> Geoid List, Add button; ->Open dialog; Format name
[UK Geoid Dosys]
[Unable to autosave: ]//message when autosave fails
[]
[Unable to create a new folder: %s]//message box in Convert dialog|message box|TT->New Job->message
[]
[Unable to overwrite file %s: %s]//message box|message box|message box
[]
[Unable to save file %s. %s]//TTools;TLink; message box durin saving the file
[]
[Unable to save file %s: %s]//messaage box
[]
[UNBabc]//TT->Process properties->GPS+Post Process tab (advanced module)
[]
[Unconnected]//TT->Tool Bar->Select->Select Points->Point type list box->value
[]
[Undefined error]//not used
[]
[Undo]//TTools; TLink; Tool Bat; Edit; menu item
[Geri Al]
[Undo\tCtrl+Z]//TL->ToolBar->Edit->Undo|TT->ToolBar->Edit->Undo
[Geri Al\tCtrl+Z]
[Unexpacted token %3c (required %3c) in line %d]
[]
[Unexpacted token %c (required %c) in line %d]
[]
[Unexpected end of line %d]
[]
[Unfix]//TTools; Adjustment; Column name
[]
[Units]//TTools->Job Configuration->left panel->node name
[]
[Unknow Time System Indicator (pos:10 line:13)]
[]
[Unknow type of satellite for version b (required G, R, M ) (line:13)]
[]
[Unknown]//TTools; Tlink;-> Convert File; -> Linear Unit list box; text|TTools and TLink -TabView->GPSObs Tab-> possible value in the Orbit column|TTools->Map View->Legend window->point type|TT->Tool Bar->Select->Select Points->Point type list box->value
[Bilinmeyen]
[unknown]//log message|message
[bilinmeyen]
[-Unknown-]//for internal use only|for internal use only|for internal use only
[-Bilinmeyen-]
[Unknown error]//not used
[]
[Unknown file type]//not used
[]
[Unknown format version]//error message
[]
[Unknown header label: ]//log message
[]
[Unknown points filter\nUnknown points filter]//for internal use only
[]
[UnPack filter not found]//not used
[]
[Unprocessed DGPS]//TTools->Map View->Legend window->line type
[]
[Unprocessed PP]//TTools->Map View->Legend window->line type
[]
[Unprocessed PP Kinematic]//TTools->Map View->Legend window->line type
[]
[Unprocessed Vectors]//TTools; Adjustment; Table header
[]
[Unreject]//TTools; Adjustment; Button name
[]
[Unselect all objects\nUnselect all objects]//TT->Tool Bar->Select->Select None->hint text in the Status Bar
[]
[Update]//TTools->CoGo; Command Name|TT->for future release
[Güncele]
[Update Project\nUpdate]//TT->for future release
[]
[Update Surface ]//TTools, string from Undo
[]
[Update Surface(s)]//TTool, command name                
[]
[Update Surface(s)\nUpdate Surface(s)]//TTools, command HINT
[]
[Upload TopSURV job to device]//TT and TL->Export to Device->Progress bar text
[Cihaz a TopSURV İşi Yükle]
[Upper digits were truncated]//message box
[]
[Use]//TTools; TLink; Localization; Properties; field name|TT->Process properties->GPS+Post Process tab (advanced module)
[Kullan]
[USE]//TLink; Resect Export, Header Field name
[KULLAN]
[Use GLONASS]//for internal use only
[GLONASS Kullan]
[Use GPS]//for internal use only
[GPS Kullan]
[Use Meteo Model]//TT->Process properties->GPS+Post Process tab (advanced module)
[Meteo Model Kullan]
[Use Original Size]//TT->Graphic View report(Map View Item,CAD View Item,Occupation View Item,Residual View Item)->Options window->check box name
[Orjinal Boyutu Kullan]
[Use prefix]//TT and TL->Points tab->Pop-up menu item Rename Points->Points renaming window->radio button name
[Önek kullan]
[Use starting number]//TT and TL->Points tab->Pop-up menu item Rename Points->Points renaming window->radio button name
[Başlangıç numarası kullan]
[Use Texture]//TTools, properties for Surface
[Texture Kullan]
[Use the Point]
[Noktayı kullan]
[Used fields]//for internal use only|for internal use only
[Kullanılmış alanlar]
[Used Iterations count: %d]//TTools;  error message under Adjustment
[]
[User]//not used|TTools and TLink, default name for new point created by Add Point|TTools->File->Remote users->add user->dlg caption|Internal use
[Kullanıcı]
[User actions]//log message|log message
[]
[User Break]//message
[]
[User has changed tab to <]//log message
[]
[User name]//TTools->File->Remote users->add user->prop. name
[Kullanıcı adı]
[User report]//TT->Report Configuration->Reports panel->
[Kullanıcı raporu]
[User will be removed]//Remote users dlg->warning dlg->text
[Kullanıcı kaldrıldı]
[User/Group]//Name of property
[Kullanıcı/Grup]
[User:]//Send files dlg static
[Kullanıcı:]
[Users]//TTools->File->Remote users->add group->add user->dlg caption
[Kullanıcılar]
[UWE]//TTools; Adjustment; Column name
[]
[UWE = %5.2f; bounds = (%5.2f, %5.2f)]//TTools; error message under Adjustment
[]
[V]//TLink; Resect Export, VA Measurement
[V]
[V angle]//TT->Tool Bar->Select->Select TS Obs->list box name
[Dşy açı]
[V Control]//TTools->Map View->Legend window->point type
[Dşy Kontrol]
[V dist]//TT->Tool Bar->Select->Select TS Obs->list box name
[]
[V precision]//TT->Tool Bar->Select->Select GPS Obs.->list box name
[Dşy hassasiyet]
[V residual]//TT->Tool Bar->Select->Select TS Obs->list box name
[]
[V. Dist]//TT->X-Section Templates tab->right panel->X-Section segment properties->field name
[Dşy.Mesafe]
[V. Offset from CL]//TT->X-Section Templates tab->right panel->X-Section segment properties->field name
[Aks dan Dşy.Ofset]
[VA misclosure(&quot;)]//TTools; Adjustment; Column name
[]
[VA Sigma, (sec)]//Process properties dialog (TLink spec.); Compute Coordinates page; field VA Sigma 
[Sigma DA,(sn)]
[Value]//not used|column name|not used|for internal use only|TTools->Point Properties->CAD tab->right panel->column name
[Değer]
[Value cannot be empty]//error message
[Değer boş olamaz]
[Value cannot be negative]//error message
[Değer negatif olamaz]
[Value is out of range]//message box|error message
[Değer aralık dışında]
[Value must be positive]//error message
[Değer pozitif olmalıdır]
[Value not chosen]//not used
[]
[VAngle Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[DA Kaba Hatası]
[VDist Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[KF Kaba Hatası]
[VDOP]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TTools and TLink->GPS Obs Tab->Properties->field name
[VDOP]
[Vector]//Ttools->view->Background images->left panel (Available images)->Type field->content
[Vektör]
[Vector Type]//TTools->GPS Vectors Import
[]
[Vector[%s:%d]: dx=%.3f dy=%.3f dz=%.3f %s]//log message
[Vektör[%s:%d]: dx=%.3f dy=%.3f dz=%.3f %s]
[Vectors]//for internal use only
[Vektörler]
[Vectors from Base]//not used
[]
[Vectors from Rover]//not used
[]
[VectorsExport]
[]
[Version of SP3 file is invalid (line:%d)]
[]
[Vert]//TTools; Adjustment; diagnistic message
[]
[Vert Control Points: ]//TTools; Adjustment; diagnistic message
[]
[Vert Element]
[]
[Vert only]//TTools; Adjustment; diagnistic message
[]
[Vert Tolerance]//TT->Loop Closure Report->Column name
[]
[Vert Tolerance abs.]//TT->Loop Closures Report->column name
[]
[Vert Tolerance rel.(ppm)]//TT->Loop Closures Report->column name
[]
[Vert. Accuracy]//TT->Custom TS Instrument list->column name
[]
[Vert. Precision]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel
[]
[Vert.Angle]//not used
[]
[Vert.Dist]//not used
[]
[Vert.Offset]//TTools, TLink; DL Occupation Properties dialog; field name
[Düşy.Ofset]
[Vertex]//not used
[]
[Vertical]//TTools; Adjustment; Column name|TTools; TLink; Localization window; Properties; field Use; field content|TTools and TLink -> Tabular View ->GPS Occupations Propertie, Antenna tab ->Antenna Height Method list box -> text|TTools and TLink->Point Properties->General tab->list box Control->possible value|TT and TL->Properties for TS Obs->General tab->Type list box->value
[Düşey]
[Vertical Adjustment will NOT be done ]//TTools; Adjustment; diagnistic message 
[]
[Vertical alignment]//TT->Roads tab->left panel->node name
[]
[Vertical Alignment]
[]
[Vertical Angle]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel  |TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Düşey Açı]
[Vertical Angle mode]//TL->Convert File->Advanced options->group box name
[Düşey Açı modu]
[Vertical angle mode:]//angle mode in advanced import/export options
[Düşey açı modu]
[Vertical Control]//TT->Tool Bar->Select->Select Points->Point type list box->value
[Düşey Kontrol]
[Vertical Distance]//TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel  |TT and TL->TSObs tab->right panel->column name and Properties for TSObs->Observation tab->field name
[Kot Farkı]
[Vertical Precision]//TTools and TLink ->GPS Obs properties-> page Observation ->field name
[Düşey Hassasiyet]
[Vertical Resection]//TT and TL->Properties for TS Obs->General tab->Type list box->value
[Düşey Kestirme]
[View]//not used
[]
[View GPS occupation properties\nView GPS occupation properties]//not used
[]
[View history]//Command name
[Geçmişe bak]
[View Job Properties\nView Job Properties]//for internal use
[]
[View properties of backsight\nView properties of backsight]//not used
[]
[View properties of DL observation\nView properties of DL observation]//??? not used
[]
[View properties of DL Run\nView properties of DL Run]//??? not used
[]
[View properties of session\nView properties of session]//not used
[]
[View properties of TS observation\nView properties of TS observation]//not used
[]
[View properties of TS Occupation\nView properties of TS Occupation]//not used
[]
[View properties\nView properties]//TTools and TLink->Menu Bar->Edit->Properies->hint text in the Status Bar
[]
[View Type]//not used
[]
[View X-Section Templates\nView X-Section Templates]//TT->X-Section Templates tab->tooltip
[EnKesit Şablonlarına Bak\nEnKesit Şablonlarına Bak]
[Visible]//TT->Tool Bar->View->Layers->Column name
[Göster]
[Void]//not used
[]
[Volumes]//TTools->Job Configuration->Display->Precisions
[Hacim]
[W]//TTools; CoGo; Intersection|TTools and TLink->Tabular View, Longituide, part of BLH coordinate value (insted of -)|TTools and TLink->Tabular View, Latituide, part of coordinate value (insted of +)|TTools; part of coordinate value on axis|TTools; part of coordinate value on axis|TTools and TLink->Tabular View, Longituide, part of  coordinate value (insted of -)|not used
[B]
[Wait]
[Bekleyin]
[Warn Float solutions]//TT->Job Configuration->Quality Control->Automatic Tests tab->check box name
[]
[Warn Float Solutions QC filter\nWarn Float Solutions Quality Control filter]//internal use
[]
[Warning]//Remote users dlg->warning dlg->caption
[]
[Warning: connected spiral and arcs must have the same radius in this format]//message
[]
[Warning: vertical alignment cannot have both parabola and arc in this format]//message
[]
[Warning: vertical alignment cannot have parabolas in this format]//message
[]
[Weighted]//TTools; Adjustment; Column name
[]
[Weighted Point]//TTools; Adjustment; diagnistic message       
[]
[Weighted Point Residuals]//TTools; Adjustment; Table header
[]
[Westing]//TTools->Map View and Cad View->axis name in Ground and Grid system
[]
[Wet Zenit Path Delay]//for internal use only
[]
[WGS Point]//TTools; TLink; Localization; Properties; field name
[WGS Noktası]
[WGS84]//TTools;Tlink; Projection indicator in the status bar|TT and TL->in advanced import/export options and open file->Datum field->value
[WGS84]
[WGS84 Ell.Height]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[]
[WGS84 Lat, Lon, Ell.H]//TT and TL->in advanced import/export options  and open file->Coordinate type->content
[]
[WGS84 Latitude]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[]
[WGS84 Longitude]//TTools; CoGo; Intersection|TTools and TLink->Tab View->Point Properties->Coordinates tab->field name
[]
[White]//TTools->attribute properies->color list box->possible value
[Beyaz]
[Wide]//TTools and TLink->Images tab->Options->Show tab->check box name
[Geniş]
[Wide Lane]//TTools and TLink ->GPS Obs tab and Properties for Observation->Solution Type field->possible value
[Geniş Açı]
[WideLane]//TT->Residiul view window->legend window
[GenişAçı]
[Window]//TTools->Map View options and Cad View options->tab name
[Pencere]
[Window cannot be closed because at least one engine is running.]//text message when window can not be closed
[]
[Wireframe]//TT->3D View->click on the 3D View window->Pop-up menu item Fill mode->Wireframe
[]
[with Area >]//TTools->properties for Surface
[]
[with Interior Angle <]//TTools->properties for Surface
[]
[With Solution]//Selection Case
[]
[World File Background Image]//not used
[]
[World files]//TTools->Map View options->Browse->Open dialog->Format name
[]
[Writing file]//text in the Status Bar during export
[Dosya yazılıyor]
[Wrong coordinate system]
[Yanlış koordinat sistemi]
[X]//TTools and TLink->Export files and Convert File->Custom format properties->for XYZ systems field in the left panel|not used|TT ->in advanced import/export options->for internal use only
[X]
[X Measurement]//orientation points
[X Ölçümü]
[X Residual]//orientation points
[X Farkı]
[XD]
[XD]
[XD Data File]
[XD Data Dosyası]
[XD files]
[XD dosyası]
[XML Antenna]//TTools, TLink; - >  properties dialog; Caption
[XML Anten]
[XML Code Library]//TTools; Codes; Export to file; file format
[XML Kod Kütüphanesi]
[XML Export]
[XML Gönder]
[XML Filter]
[XML Filitre]
[XML filter not found]//log message
[XML filitre bulunamadı]
[XML not saved]//log message
[XML kayıtedilemedi]
[XML Topcon Feature File]//TTools; Export to File; Format name
[XML Topcon Özellik Dosyası]
[X-Section]//TT->Roads tab->Add X-Section
[En Kesit]
[X-Section Offset]//TT->X-Section Template tab->Add X-Section Segment
[En Kesit Ofseti]
[X-Section Set]
[En Kesit Ayarı]
[X-Section Template]//TT->X-Section Template tab->Add X-Section Template
[En Kesit Şablonu]
[X-Section Templates]//for internal use???
[En Kesit Şablonları]
[X-section view options]//TT->Roads tab->Options(for internal use)
[En Kesit opsiyonlarına bak]
[X-Sections]//TT->Roads tab->left panel->node name
[En Kesitler]
[XYZ]//TTools and TLink->Export files and Convert File->Custom format properties->Coordinate system list box->possible value|not used
[XYZ]
[Y]//TTools and TLink->Export files and Convert File->Custom format properties->for XYZ systems field in the left panel|not used|TT ->in advanced import/export options->for internal use only
[Y]
[Y Measurement]//orientation points
[Y Ölçümü]
[Y Residual]//orientation points
[Y Farkı]
[Yb]//units of files size - send file dialog
[Yb]
[Yellow]//TTools->attribute properies->color list box->possible value
[Sarı]
[Yes]//TLink->Compute Coordinates->Scale factor dialog(for TS measurments)->button name
[Evet]
[Yes to all]//TLink->Compute Coordinates->Scale factor dialog(for TS measurments)->button name
[Tümüne evet]
[You are at the top level, and cannot go up another level]//message box
[]
[You are trying to import %d files]//TTools;Tlink; Drop options dialog; text
[Tekrar %d dosyalarını yüklemeyi deneyin]
[You are trying to open %d file(s)]//TTools;Tlink; Drop options dialog; text
[]
[You can calculate Conditional Coordinates only]//TTools;   diagnostic message during Adjustment and Compute coordinate
[]
[You can calculate Conditional Coordinates Only for TS-Measurements]//TTools;   diagnostic message during Adjustment and Compute coordinate
[]
[You can calculate Conditional Coordinates Only for TS-Measurements in one component]//diagnostic message during Adjustment and Compute coordinate 
[]
[You did not save the parameters. Do you want to save them now?]//TTools; TLink; Datum Transformation...; message box while localization
[]
[You did not update localization parameters. Do you want to update them now?]//TTools; TLink; Localization; message box while localization
[]
[You did not update parameters. Do you want to update them now?]//TTools; TLink; Datum Transformation...; message box while localization
[Parametreleri güncellemediniz. Şu an da güncellemek istermisiniz?]
[You have %d %s components]//TTools;   diagnostic message during Adjustment and Compute coordinate
[]
[You have changed the list of modules to load. ]//Access codes dialog_>message
[]
[You must enter a job location]//TT->New job dialog->message
[İş yeri mutlaka girilmelidir]
[You must enter a job name]//TT->Creare a new job->message
[]
[You must restart Topcon Tools for the changes to take effect. ]//Access codes dialog->message
[]
[You shall assign code before assigning string]//message box
[]
[Z]//TTools and TLink->Export files and Convert File->Custom format properties->for XYZ systems field in the left panel|not used|TT ->in advanced import/export options->for internal use only
[Z]
[Z angle]//TT->Tool Bar->Select->Select TS Obs->list box name
[Z açısı]
[ZA]//TLink; Resect Export, Header Field name
[ZA]
[ZAngle Residual]//TT->TS Obs tab->Properties for TS Obs->Adjustment tab->field name
[ZAçı Farkı]
[Zb]//units of files size - send file dialog
[]
[Zenith]//TT and TL->in advanced import/export options and open file->Vertical angle mode list box->value|TL->Convert File->Advanced options->radio button name
[Zenit]
[Zenith Angle]//not used|TTools and TLink->Export files and Convert File->TSRaw custom format properties->field in the left panel|TT and TL->TS Obs tab->column name and Properties for TS Obs->Observation tab->field name
[Zenit Açısı]
[Zero objects]//error message
[Objeler Sıfır]
[Zoom]
[Zum]
[Zoom &Back]
[Zum &Geri]
[Zoom &In]
[Zum &Yaklş]
[Zoom &Out]
[Zum &Uzakl]
[Zoom Back]
[Zum Geri]
[Zoom In]
[Zum Yaklş]
[Zoom Out]
[Zoom Uzakl]
